
S T 3 5 0 4 0 A   M E D A L I S T   P R    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 6536|     |
Capacity form/unform  5040/      MB        Heads           8|     |     |
Seek time   / track   2.0/10.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA3 ENHANCED   Precompensation
Cache/Buffer           512 KB MULTI-SEGMEN Landing Zone
Data transfer rate   11.000 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext
Recording method     PRML                           operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 70
Power: sleep              W     Humidity     %                 |
       standby        1.0 W     Altitude    km                 |
       idle           7.3 W     Shock        g        10       |     75
       seek          10.0 W     Rotation   RPM      5400
       read/write     8.5 W     Acoustic   dBA        30
       spin-up            W     ECC        Bit   SMART
                                MTBF         h     500000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


