
S T 1 4 2 0 7 N V           C A Y M A N    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    4016|     |     |
Capacity form/unform  4294/      MB        Heads          20|     |     |
Seek time   / track   8.5/ 2.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST/AV      Precompensation
Cache/Buffer           512 KB              Landing Zone
Data transfer rate    6.700 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %         5 95    |      5 95
       standby            W     Altitude    km    -0.061  3.048|        12.192
       idle          12.8 W     Shock        g         5       |     50
       seek          14.3 W     Rotation   RPM      7200
       read/write    13.2 W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h    1000000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CFP-4207S  QUICK REFERENCE GUIDE REV. C, 12/1994

  +---------------------------------------------------------+
  |      +-J1                                            ++ |XX J2
  |      | |                                             || |XX
  |      | |                                             || |XX
  |      | |                                             || |XX I
  |      +-+                                             || |XX N
  |                                                      *+ |XX T
  |                                                    E8++ |XX E
  |                                                      ++ |XX R
  |                                             (Fuse)F1 xx |XX F
  |  J3                                                  ++ |XX A
  | +-+ SS                         ++++++++              || |XX C
  | | | LED                        ++++++++              || |XX E
  | | |                          E1 ****** E7            || |XX
  | +-+                          E4 RESERVED             || |
  |J6+0E1                                                *+ |xx
  || |                                                      |XX J4
  |+-+0E6                                                   |XX Power
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CFP-4207S  QUICK REFERENCE GUIDE 12/1994, REV. C

 Jumper Setting
 ==============


 Setting the SCSI Bus Address
 ----------------------------
 There are three jumpers available for configuration of the SCSI ID:
 E1, E2, and E3.

 OPTIONAL HEADER
      |     +-+
  0E1 | ----+ +-*  SCSI ID 1
  0E2 | ----+ +-*  SCSI ID 2
  0E3 | ----+ +-*  SCSI ID 4
  0E5 | ----+ +-*  Disable Spin
  0E6 | ----+ +-*  LED Driver
      |     +-J6
      |     PCB
      +---------------


 An optional 2mm pin pitch right angle header is located on the front
 of the PCBA (opposite the SCSI interface connector) which allows
 changing the SCSI IDs while the drive is mounted in the system. The
 header includes three pins, 0E1, 0E2 and 0E3 which can alternatively
 be used to select the SCSI Bus address. This connector may also be
 used to cable the SCSI ID select to a remote switch. A receptable
 connector AMP P/N 111622-1 or equivalent can be used to connect a
 ribbon cable to this header.

   +----------+-----------------------+
   | SCSI ID  | 0E3     0E2     0E1   |
   |          | E3    | E2    | E1    |
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    2     | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    3     | OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+
   |    4     | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    5     | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    6     | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+

 NOTE
 When controlling the SCSI ID remotely, IN (CLOSED) = Ground or TTL
 Low and OUT (OPEN) = Open or TTL High.


 Disabling Spin-Up at Power On
 -----------------------------
 A jumper in the E5 location, disables spin up after power-on for
 applications where spin up sequencing is necessary. An optional 2mm
 pin pitch right angle header is located on the front of the PCBA
 (opposite the SCSI interface connector) which can alternatively be
 used to disable spin up. Disabling spin up on application of power
 can also be enabled by setting the DSPN bit in MODE SELECT page 00H
 (Operating Parameters). The Host must issue a Start UNIT command to
 cause the drive to spin up.

   +---------+------+---------------------+
   |E5 or 0E5| DSPN | Result              |
   +---------+------+---------------------+
   |   IN    |  0   | Spin Disabled       |
   +---------+------+---------------------+
   |   IN    |  1   | Spin Disabled       |
   +---------+------+---------------------+
   |   OUT   |  0   | Spin up on Power On |
   +---------+------+---------------------+
   |   OUT   |  1   | Spin Disabled       |
   +---------+------+---------------------+
 NOTE
 IN = Ground or TTL Low and OUT = Open or TTL High.


 Delaying Spin Up at Power On
 ----------------------------
 A jumper in the E6 location, delays spin up on power-up by the value
 of the drive's SCSI ID multiplied by 4 seconds (i.e. SCSI ID 4 will
 delay 16 seconds). Delaying spin up on application of power can also
 be enabled by setting the SDLY bit in MODE SELECT page 00H (Operating
 Parameters.)

   +---------+------+---------------------+
   |   E6    | SDLY | Result              |
   +---------+------+---------------------+
   |   IN    |  0   | Spin Delayed        |
   +---------+------+---------------------+
   |   IN    |  1   | Spin Delayed        |
   +---------+------+---------------------+
   |   OUT   |  0   | Spin up on Power On |
   +---------+------+---------------------+
   |   OUT   |  1   | Spin Delayed        |
   +---------+------+---------------------+


 Disabling the SCSI Bus Parity
 -----------------------------
 SCSI parity is always enabled in both directions, unless the E7
 Parity disable jumper is installed. Installing the jumper will cause
 the drive to ignore SCSI bus Parity In but it will continue to
 generate SCSI bus Parity Out.


 Disabling SCSI Bus Terminator Power (TERMPWR)
 ---------------------------------------------
 Power to the on-board terminators is provided by the higher of the
 voltage supplied at Pin #26, J2 or the voltage level at the 5 Volt
 power input to the drive minus one diode drop. Termination Power to
 external terminators can be supplied by the drive through Pin #26,
 J2. The TERMPWR line can be disconnected from the drive by removing
 Jumper E8.


 Jumper E8   Result
   IN        TERMPWR (J2, Pin #26) connected to the drive's internal
             termination power.

   OUT       TERMPWR (J2, Pin #26) open circuit.


 Setting the Bus Termination
 ---------------------------
 This drive provides on-board Alternative 2 active termination for the
 SCSI bus. The termination resistors, which are contained in two
 Single Inline Packs (SIPs) should be removed from the drive unless it
 is a SCSI device at the physical end of the bus.

 NOTE
 The TERMPWR output of the drive is protected by a 1 Ampere fuse (F1).
 If external terminators are being powered from the drive and SCSI bus
 problems are suspected, verify that the fuse is still operational
 using a meter.



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
SEAGATE   SUPPORT SERVICES

 Seagate Technology
 ------------------
 Technical Support Services
 If you need assistance installing your drive, consult your dealer.
 Dealers are familiar with their unique system configurations and can
 help you with system conflicts and other technical issues. If you
 need additional assistance with your Seagate(r) drive or other
 Seagate products, use one of the Seagate technical support services
 listed below.

 SeaFONE at 1-800-SEAGATE (1-800-732-4283)
 Seagate's 800 number allows toll-free access to automated self-help
 services, providing answers to commonly asked questions,
 troubleshooting tips and specifications for disc drives and tape
 drives. This service is available 24 hours daily and requires a
 touch-tone phone. If you need to speak to a technical support
 engineer, dial this number and listen to the options for technical
 support. (International callers can also reach this automated
 self-help service by dialing 408-456-4496).


 Seagate Technology online services
 Using a modem, you can obtain troubleshooting tips, free utility
 programs, drive specifications and jumper settings for Seagate's
 entire product line. You can also download software for installing
 and analyzing your drive.

 SeaNET
 You can obtain technical information on Seagate drives, Seagate
 software and much more over the Internet from Seagate's World Wide
 Web home page (http://www.seagate.com) or Seagate's ftp server
 (ftp://ftp.seagate.com).

 You may also send E-mail with your questions to DiscSupport@
 Seagate.com or TapeSupport@Seagate.com.


 SeaBOARD
 SeaBOARD is a computer bulletin board system (BBS) that contains
 information about Seagate's disc and tape drive products and is
 available 24 hours daily. Set your communications software to eight
 data bits, no parity and one stop bit (8-N-1). SeaBOARD phone numbers
 are listed in the following table.

 BBS Location           Modem number
 United States      Disc: 408-434-1080; Tape: 408-456-4415
 England            44-1628-478011
 France                         33 1-48 25 35 95
 Germany            49-89-140-9331
 Singapore          65-292-6973
 Thailand           662-531-8111
 Australia          61-2-9756-2359
 Taiwan             886-2-719-6075

 Seagate CompuServe forum
 Online technical support for Seagate products is available on
 CompuServe. To access our technical support forum, type go seagate.
 This forum provides information similar to that found on SeaBOARD.
 In addition, you can type questions or browse through previous
 questions and answers on the forum messages.

 Seagate Technology FAX services
 SeaFAX
 You can use a touch-tone telephone to access Seagate's automated FAX
 system to receive technical support information by return FAX. This
 service is available 24 hours daily.
 Location               Telephone number
 United States          1-800-SEAGATE or 408-456-4496
 England                44-1628-894084
 Australia              61-2-9756-5170

 Seagate technical support FAX
 You can FAX questions or comments to technical support specialists 24
 hours daily. Responses are sent during business hours.
 Location               FAX number
 United States          408-944-9120
 England                        44-1628-890660
 France                 33 1-46 04 42 50
 Germany                        49-89-1430-5100
 Australia              61-2-9725-4052
 Singapore              65-293-4722
 Hong Kong              852-2368 7173
 Taiwan                 886-2-715-2923
 Korea                          82-2-556-7294/4251


 Seagate technical support
 You can talk to a technical support specialist during business hours
 Monday through Friday for one-on-one technical help.  Before calling,
 note your system configuration and drive model number (STxxxx). There
 are several technical support phone numbers available for various
 Seagate products.

 Location          Telephone  number
 United States Please dial 1-800-SEAGATE for the specific product
               telephone number.
               (6:00 A.M. to 11:15 A.M., 12:30 P.M. to 5:00 P.M.,
               Pacific time, M-F)
 England       44-1628-894083 (10:00 A.M. to 1:00 P.M., 2:00 P.M. to
               5:00 P.M., M-F)
 France        33 1-41 86 10 86 (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Germany       Disc: 49-89-140-9332; (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 4:00 P.M., M-F)
               Tape: 49-89-140-9333
 Australia     61-2-9725-3366 (9:00 A.M. to 5:00 P.M., M-F)
 Singapore     65-290-3998 (9:00 A.M. to 12:00 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Hong Kong     852-2368 9918
 Taiwan        886-2-514-2237
 Korea         82-2-556-8241


 SeaTDD 408-944-9121
 Using a telecommunications device for the deaf (TDD), you can send
 questions or comments 24 hours daily and exchange messages with a
 technical support specialist between 6:00 A.M. to 11:15 A.M. and
 12:30 P.M. to 5:00 P.M. (Pacific time) Monday through Friday.


 Customer Service Centers
 Seagate direct OEM, Distribution, System Integrator and Retail
 customers should contact your Seagate Service Representative for
 warranty information.  Other customers contact your place of
 purchase.  Seagate offers comprehensive customer support for all
 Seagate drives.  Seagate customer service centers are the only
 facilities authorized to service Seagate drives. These services are
 available worldwide.

 Location                       Telephone number                FAX number
 United States          1-800-468-3472;                 405-949-6740
 Other Americas
 (Canada & Brazil)      405-949-6706;               405-949-6738
 Mexico                         525-546-6965;                   525-546-4888
 Europe, Middle
 East & Africa          31-2065-43300;              31-2065-34320
 Asia Pacific &
 Australia              65-485-3595;                    65-485-4980
 Japan                          81-3-5462-2904;                 81-3-3462-2979


 Seagate, Seagate Technology and the Seagate logo are registered
 trademarks of Seagate Technology, Inc. SeaFAX, SeaFONE, SeaBOARD,
 SeaTDD, SeaNET, Medalist and DiscWizard are either trademarks or
 registered trademarks of Seagate Technology, Inc. or one of its
 subsidiaries. All other trademarks or registered trademarks are the
 property of their respective owners.


