
P L S - 3 0 8 5 4 A         A - P L U S    SAMSUNG
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    3842| 1647| 1024|
Capacity form/unform   850/      MB        Heads           4|   16|   16|
Seek time   / track  11.0/ 3.0 ms          Sector/track     |   63|   63|
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate    7.125 MB/S int       Bytes/Sector      512
                     13.300 MB/S ext DMA
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C         5 55    |    -40 65
Power: sleep          0.8 W     Humidity     %         8 80    |      8 95
       standby        1.1 W     Altitude    km    -0.061  3.048| -0.305 12.192
       idle           2.8 W     Shock        g        10       |     75
       seek           7.0 W     Rotation   RPM      4500
       read/write     4.8 W     Acoustic   dBA        38
       spin-up       15.0 W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SAMSUNG  PLS-30854A  JUMPER SETTING

 Jumper Setting
 ==============


 J2 Setting
 ----------

   1 2      1 2      1 2
  +---+    +---+    +---+
  |o o|    |o o|    |o o|
  |o o|    |o o|    |o o|
  |o o|    |o o|    |o o|
  |o o|    |o o|    |o o|
  |o o|    |o o|    |o o|DXX
  |o o|    |o o|    |o o|DCF
  |o o|    |o o|    |o o|DSP
  |xxx|    |xxx|    |o o|-C/D
  +---+    +---+    +---+
 1 Drive   Master    Slave

 DOS Set-Up Parameters CYL 1024, HD 16, SEC 63 => INSTALL the DCF
 Jumper


