
7 2 9 0 A    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |  941|     |
Capacity form/unform   290/      MB        Heads           4|   14|     |
Seek time   / track  14.0/ 3.0 ms          Sector/track     |   43|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    3.000 MB/S int       Bytes/Sector      512
                      9.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 71
Power: sleep          1.7 W     Humidity     %         5 95    |      5 95
       standby        1.7 W     Altitude    km    -0.061  3.048|
       idle               W     Shock        g        10       |     70
       seek           3.8 W     Rotation   RPM      3551
       read/write     4.0 W     Acoustic   dBA
       spin-up            W     ECC        Bit   88
                                MTBF         h     300000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   7290A  QUICK REFERENCE

  +---------------------------------------------------------+
  |                                           +-+-+-+-+     |
  |                                           +++++++++     |
  |                                        J25-+ |J23+--J22 XX
  |                                        J24---+    +-+   XX
  |                                                   +-+J20XX
  |                                                   +-+J19XX
  |                                                   +-+J18XX J1
  |                                                   +-+J17X*
  |                                                   +-+J16XX
  |                                                         XX
  |                                                         XX
  |                                                         XX
  |                                                         XX1-2
  |                                                         | 1
  |                                                         XX Power
  |                                                         XX J2
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   7290A  QUICK REFERENCE

 Jumper setting
 ==============

 Note: Jumper J25 is factory reserved.

 Jumper J19 is a spare shunt.


 J16  I/O Channel Ready
 ----------------------
      J16 CLOSED  Option Enabled
      J16 OPEN    Option Disabled (default)


 J17  ECC
 --------
      J17 CLOSED 4-Byte emulation
      J17 OPEN   11-Byte (default)


 J18  Low Power Spin Mode
 ------------------------
      J18 CLOSED  Enabled
      J18 OPEN    Disabled (default)


 J20  Master/Slave
 -----------------
      J20 CLOSED  Only drive in single drive system (Default)

      J20 CLOSED  Master in dual drive system

      J20 OPEN    Slave in dual drive system


 J22  Drive Compatibility
 ------------------------
      J22 CLOSED  Enabled
      J22 OPEN    Disabled (default)


 J23  Write Cache
 ----------------
      J23 OPEN    Enabled (default)
      J23 CLOSED  Disabled


 J24  Cable Select
 -----------------
      J24 OPEN    Disabled (default)
      J24 CLOSED  Enabled


