
S T 3 4 2 1 7 W   C O Z U M E L   4 L P    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    6028|     |     |
Capacity form/unform  4294/      MB        Heads          10|     |     |
Seek time   / track   8.5/ 1.8 ms          Sector/track     |     |     |
Controller           SCSI3 SI/WI/ULTRA     Precompensation
Cache/Buffer           512 KB MULTI-SEGMEN Landing Zone
Data transfer rate    9.000 MB/S int       Bytes/Sector      512
                     40.000 MB/S ext SYNC
Recording method     PRML                           operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle           8.1 W     Shock        g                 |
       seek               W     Rotation   RPM      7200
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h    1000000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


