
S T 1 1 0 2 N    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders        |     |     |
Capacity form/unform    84/      MB        Heads           5|     |     |
Seek time   / track  19.0/     ms          Sector/track     |     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation 65535
Cache/Buffer               KB              Landing Zone
Data transfer rate    1.500 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      50000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


