
C P - 3 0 1 0 0    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1524|     |     |
Capacity form/unform   122/      MB        Heads           4|     |     |
Seek time   / track  19.0/ 8.0 ms          Sector/track   39|     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation
Cache/Buffer            64 KB LOOK-AHEAD   Landing Zone
Data transfer rate    1.500 MB/S int       Bytes/Sector      512
                      4.500 MB/S ext SYNC
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %         8 80    |      8 80
       standby            W     Altitude    km    -0.061  3.050|        12.200
       idle           2.8 W     Shock        g         5       |     75
       seek           3.9 W     Rotation   RPM      3400
       read/write     3.8 W     Acoustic   dBA        40
       spin-up            W     ECC        Bit   48
                                MTBF         h     150000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates     CSA,IEC435,IEC380,TUV,UL47...

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CP30060/CP30080/CP30100  PRODUCT MANUAL 00501-044

  +-------------------------------------------------------+
  |   +-+                                            +-+  |XX 50 PIN
  |   | |HDA                                         | |  |XX SCSI
  |   | |J1                                          | |  |XX I
  |   +-+                                            +-+  |XX N
  |                                       SCSI       +-+  |XX T  J2
  |                                       Terminators| |  |XX E
  |                                                  | |  |XX R
  |                                                  +-+  |XX F
  |                                                  +-+  |XX A
  |                                                  | |  |XX C
  | LED DRIVE                                        | |  |XX E
  | CAPABILITY                                       +-+  |XX
  |1--2 J4                                                |XX1
  |+--+       +--+                                        |
  ||  |       |  |SCSI ID                                 |XX Power J3
  |+--+       +--+                                        |XX
  +-------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CP30060/CP30080/CP30100  PRODUCT MANUAL 00501-044

 Jumper setting
 --------------

 J2  SCSI Connector Pin Assignments
 ----------------------------------
          +------------+--------+-------------+-------+
          | Signal     |Pin No. |   Signal    |Pin No.|
          +------------+--------+-------------+-------+
          | -DB(0)     |   2    |   -DB(1)    |   4   |
          +------------+--------+-------------+-------+
          | -DB(2)     |   6    |   -DB(3)    |   8   |
          +------------+--------+-------------+-------+
          | -DB(4)     |  10    |   -DB(5)    |  12   |
          +------------+--------+-------------+-------+
          | -DB(6)     |  14    |   -DB(7)    |  16   |
          +------------+--------+-------------+-------+
          | -DB(P)     |  18    |   GROUND    |  20   |
          +------------+--------+-------------+-------+
          | GROUND     |  22    |   GROUND    |  24   |
          +------------+--------+-------------+-------+
          | TERMPWR    |  26    |   GROUND    |  28   |
          +------------+--------+-------------+-------+
          | GROUND     |  30    |   -ATN      |  32   |
          +------------+--------+-------------+-------+
          | GROUND     |  34    |   -BSY      |  36   |
          +------------+--------+-------------+-------+
          | -ACK       |  38    |   -RST      |  40   |
          +------------+--------+-------------+-------+
          | -MSG       |  42    |   -SEL      |  44   |
          +------------+--------+-------------+-------+
          | -C/D       |  46    |   -REQ      |  48   |
          +------------+--------+-------------+-------+
          | -I/O       |  50    |             |       |
          +------------+--------+-------------+-------+
          The minus sign (-) indicates active low.
          All odd pins except pin 25 must be connected to ground.
          Pin 25 is left open.

 SCSI ID Jumpers
 ---------------
  +--------------+----------+--------+--------+
  | Drive Select |   E1     |  E2    |  E3    |
  +--------------+----------+--------+--------+
  |     0        |  OPEN    | OPEN   | OPEN   |
  |     1        |  CLOSED  | OPEN   | OPEN   |
  |     2        |  OPEN    | CLOSED | OPEN   |
  |     3        |  CLOSED  | CLOSED | OPEN   |
  |     4        |  OPEN    | OPEN   | CLOSED |
  |     5        |  CLOSED  | OPEN   | CLOSED |
  |     6        |  OPEN    | CLOSED | CLOSED |
  |     7        |  CLOSED  | CLOSED | CLOSED |
  +--------------+----------+--------+--------+

 Parity option
 -------------
 NOTE: SCSI parity is always enabled.


 J4  LED DRIVE CAPABILITY
 ------------------------
 An optional external LED may be attached to pins 1 & 2 of LED DRIVE
 CAPABILITY.


 J3  Power
 ---------
      +---------+
      | 1 2 3 4 |
      +-+-+-+-+-+
        | | | +----------- + 5V
        | | +------------- GND
        | +--------------- GND
        +----------------- + 12V



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
CONNER   CP30060/CP30080/CP30100  PRODUCT MANUAL  00501-044

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+
 The drive may be mounted in any attitude!


 Recommended Mounting Configuration
 ----------------------------------
 The drive is designed to be used in applications where the unit may
 experience shock and vibrations at greater levels than larger and
 heavier disk drives.

 The design features which allow greater shock tolerance are the use
 of rugged heads and media, a dedicated landing zone, closed loop
 servo positioning and specially designed motor and actuator
 assemblies.

 Ten base mounting points are provided to the customer. The drive is
 mounted using 6-32 x 5/32" max. insertion for the sides, and 3/8"
 insertion for the bottom. The system integrator should allow ventila-
 tion to the drive to ensure reliable drive operation over the opera-
 ting temperature range.

 For additional vibration isolation, an external suspension system
 may be used.


 Cable Requirements
 ------------------
 A 50-conductor flat cable or 25-conductor twisted pair cable is re-
 quired. The maximum cable length is 6.0 meters (19.68 ft).

 The cable characteristic impedance should be 132 ohms   10% with a
 minimum conductor size of 28 AWG.

 Connector Requirements
 ----------------------
 The drive connector is a 50-conductor connector which consists of two
 rows of 25 male pins on 100 mil centers.

 The cable connector is a 50-conductor non-shielded connector which
 consists of two rows of 25 female contacts on 100 mil centers.

 Power Connector
 ---------------
 The drive has a 4-pin DC power connector mounted on the PCB. The
 recommended mating connector is AMP part number 1-480424-0 utilizing
 AMP pins, part number 350078-4 or equivalent.

 Electrical Description
 ----------------------
 The drive uses open collector drivers. All assigned aignals are
 terminated with 220 ohms to +5 volts and 330 ohms to ground. The
 termination resistors are removable for multi-device configurations.

 Terminator Power
 ----------------
 Terminator power (TERMPWR) is supplied through a diode to prevent the
 back-flow of power to the drive. TERMPWR has the following character-
 istics:
  +--------------------------------+--------------------------------+
  |Supply Voltage                  | 4.0 VDC to 5.25 VDC            |
  +--------------------------------+--------------------------------+
  |Minimum Source Drive Capability | 800ma                          |
  +--------------------------------+--------------------------------+
  |Maximum Sink Capability         | 1.0ma sink capability (except  |
  |                                | for the purpose of providing   |
  |                                | power to an internalterminator)|
  |                                | with a 1.0 amp fuse            |
  +--------------------------------+--------------------------------+

 Magnetic Field
 --------------
 The disk drive will meet its specified performance while operating in
 the presense of an externally produced magnetic field under the
 following conditions.
   +------------------+------------------+
   |Frequency         |   Field Intensity|
   +------------------+------------------+
   |   0 to 700 Khz   |   6 gauss maximum|
   | 700Khz to 1.5 Mhz|   1 gauss maximum|
   +------------------+------------------+

 Acoustic Noise
 --------------
 The sound pressure level will not exceed 40 dBA at a distance of 1
 meter from the drive.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
CONNER   CP30060/CP30080/CP30100  PRODUCT MANUAL 00501-044

 Key Features
 ------------
 The CP30060, CP30080 and CP30100 are high performance 3.5 inch low-
 profile (1") 60, 80 and 120 megabyte (formatted) disk drives with 19
 ms average seek time. They are designed to operate on the Small
 Computer System Interface (SCSI) and are compatible with the
 Common Command Set (CCS). The drives feature low power requirements
 and high shock resistance, enabling operation in portable environ-
 ments.

        1 : 1 Interleave

        Automatic Spindle Synchronization

        64KByte Look-Ahead Read Buffer

        Track Skewing

        48 Bit ECC


 Seek Times
 ----------

       +----------------------------------+--------+
       |Track-to-Track         msec.      |   8    |
       +----------------------------------+--------+
       |               Average msec. typ. |  < 19  |
       |               Average msec. max. |  35    |
       +----------------------------------+--------+
       |Latency                msec. avg. |   8.8  |
       +----------------------------------+--------+
       The timing is measured through the interface with the drive
       operating at nominal DC input voltages.
       The average seek time is determined by averaging the seek time
       for a minimum of 1000 seeks of random length over the surface
       of the disk.


 Output Characteristics
 ----------------------
 Each signal driven by the drive has the following output character-
 istics when measured at the drive connector:

  +--------------------------------+----------------------------+
  |Signal assertion                | 0.0 VDC to 0.4 VDC         |
  +--------------------------------+----------------------------+
  |Minimum driver output capability| 48ma (sinking) at 0.5 VDC  |
  +--------------------------------+----------------------------+
  |Signal negation                 | 2.5 VDC to 5.25 VDC        |
  +--------------------------------+----------------------------+

 Input Characteristics
 ---------------------
 Each signal received by the drive must have the following input
 characteristics when measured at the drive connector:

  +--------------------------------+----------------------------+
  |Signal assertion                | 0.0 VDC to 0.8 VDC         |
  +--------------------------------+----------------------------+
  |Minimum total input load        | -0.4ma at 0.4 VDC          |
  +--------------------------------+----------------------------+
  |Signal false                    | 2.0 VDC to 5.25 VDC        |
  +--------------------------------+----------------------------+

 Functional Description
 ----------------------
 The drive contains all necessary mechanical and electronic parts to
 interpret control signals, position the recording heads over the
 desired track, read and write data, and provide a contaminant free
 environment for the heads and disks.

 Read/Write and Control Electronics
 ----------------------------------
 One integrated circuit is mounted within the sealed enclosure in
 close proximity to the read/write heads. Its function is to provide
 head selection, read pre-amplification, and write drive circuitry.
 The single microporcessor-controlled circuit card provides the re-
 maining electronic functions which include:

        - Read/Write Circuitry
        - Rotary Actuator Control
        - Interface Control
        - Spin Speed Control
        - Dynamic Braking

 At power down the heads are automatically retracted to the inner dia-
 meter of the disk and are latched and parked on a landing zone that
 is inside the data tracks.

 Drive Mechanism
 ---------------
 A brushless DC direct drive motor rotates the spindle at 3400 RPM.
 The motor/spindle assembly is dynamically balanced to provide minimal
 mechanical runout to the disks. A dynamic brake is used to provide a
 fast stop to the spindle motor and return the heads to the landing
 zone when power is removed.

 Air Filtration System
 ---------------------
 The head-disk assembly is a sealed enclosure with an integral 0.3
 micron filter which maintains a clean environment for the heads and
 disks.

 Head Positioning Mechanism
 --------------------------
 The read/write heads are supported by a mechanism coupled to a rotary
 voice coil actuator.

 Read/Write Heads and Disks
 --------------------------
 Data is recorded on 95mm diameter disk through 3370 type heads.

 Error Correction
 ----------------
 The drive performs internal error correction. The dual six-byte error
 correction polynominal is capable of correcting two error bursts,
 each with a maximum of 8 bits per 512 byte block.


 Reliability and Maintenance
 ---------------------------
 MTBF                     150,000 hours
 MTTR                     10 minutes typical
 Preventive Maintenance   None
 Component Design Life    5 years


 Safety Standard
 ---------------
 Conner Peripherals disk drives are designed to comply with relevant
 product safety standards such as:

 - UL 478, 5th edition, Standard for Safety of Information Processing
   and Business Equipment, and UL 1950, Standard for Safety of
   Information Technology Equipment.

 - CSA 22.2#154, Data Processing Equipment and CSA 22.2#220, Inform-
   ation Processing and Business Equipment CSA 22.2#950, Safety of
   Information Technology Equipment

 - IEC 435 Safety Requirements for Data Processing Equipment, IEC 380,
   Safety of Electrically Energized Office Machines, and IEC 950,
   Safety of Information Technology Equipment Including Electrical
   Business Equipment

 - VDE 0805 Equivalent to IEC 435, VDE 0805 TIEL 100, Equivalent to
   IEC 950, and VDE 0806, Equivalent to IEC 380

 - TUV Essen and TUV Rheinland


 Notice
 ------
 Conner Peripherals makes no warranty of any kind with regard to this
 material, including, but not limited to, the implied warranties of
 merchantability and fitness for a particular purpose. Conner
 Peripherals shall not be liable for errors contained herein or for
 incidental consequential damages in connection with the furnishing,
 performance, or use of this material.


