
A - 8 0    AREAL
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        |  665|     |
Capacity form/unform    80/      MB        Heads            |   14|     |
Seek time   / track      /     ms          Sector/track     |   17|     |
Controller           IDE / AT              Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
AREAL    A-60/80  DRIVE OPTIONS AND BIOS INFORMATIONS

  +---------------------------------------------------------+
  |                                                         |
  |                                                         |XX44
  |                                                         |XX
  |                                                         |XX I
  |                                                         |XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                                         |.X R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |                                                         |XX
  |                                       ++J1              |XX
  |                                       ++                |  2
  +---------------------------------------------------------+




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
AREAL    A-60/80  DRIVE OPTIONS AND BIOS INFORMATION

 Jumper Setting
 ==============

 x = Factory Default Setting


 J1  Master/Slave Option
 -----------------------
  x  CLOSED  Master
     OPEN    Slave


