
S H D - 3 0 5 6 0 A   A P O L L O 5 6 0    SAMSUNG
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    2668| 1024| 1086|
Capacity form/unform   561/      MB        Heads           4|   16|   16|
Seek time   / track  12.0/     ms          Sector/track     |   63|   63|
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate    5.000 MB/S int       Bytes/Sector      512
                     11.000 MB/S ext PIO3
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |     75
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   88,REED SOLOMON
                                MTBF         h     250000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SAMSUNG  SHD-30280A/30420A/30560A  USER`S MANUAL 1994

  +---------------------------------------------------------+
  |                                            +-+DCF       |XX
  | +-+                                        | |DSP       |XX
  | | |                                        +-+-C/D      |XX
  | | |                                                     |XX
 ++ +-+                                                     |XX I
 ++ External                                                |XX N
  | LED                                                     |XX T
  |                                                         |*X E
  |                                                         |XX R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |                                                         |X1
  |                                                         |
  |                                                         |XX
  |                                                         |XX Power
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SAMSUNG  SHD-30280A/30420A/30560A  USER`S MANUAL 1994

 Jumper Setting
 ==============

 8-pin User Configurations Jumper Block
 --------------------------------------

    +---+          +---+         +---+
    |o o|          |o o|         |o o|
    |o o|DCF       |o o|DCF      |o o|DCF
    |o o|DSP       |o o|DSP      |xxx|DSP
    |o o|-C/D      |xxx|-C/D     |xxx|-C/D
    +---+          +---+         +---+
   2 Drive        1 Drive       2 Drive
   SLAVE                        MASTER


 DCF Jumper
 ----------
 The following table shows the recommended drive configuration for the
 SHD-30280A/30420A/30560A drives.
 +-------+-----+-----+----+-----------+----------+--------------+
 |Model  | Cyl.|Heads|Sec.|Formatted  |Formatted |DCF Jumper    |
 |       |     |     |    |CMOS MBytes|DOS MBytes|              |
 +-------+-----+-----+----+-----------+----------+--------------+
 |30280A | 869 | 10  | 63 |    267.3  |   280.3  |NONE          |
 +-------+-----+-----+----+-----------+----------+--------------+
 |30420A | 856 | 16  | 63 |    401.3  |   420.7  |NONE          |
 +-------+-----+-----+----+-----------+----------+--------------+
 |30560A |1024 | 16  | 63 |    503.5  |   528.4  |INSTALLED     |
 |       |1086 | 16  | 63 |    547.8  |   560.9  |NONE (default)|
 +-------+-----+-----+----+-----------+----------+--------------+



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SAMSUNG  SHD-30280A/30420A/30560A  USER`S MANUAL 1994

 Notes on Installation
 =====================

 Shipping
 --------
 When transporting or shipping a drive, a SAMSUNG-approved container
 must be used. Keep your original box. Shipping a drive in a non-
 approved container will void the drive warranty.

 Samsung recommends shipping by an air-ride carrier experienced in
 handling computer equipment.


 Environment
 -----------
 - Avoid excessive humidity and temperature.

 - Do not place near a magnet.

 - Samsung Hard Disk Drives do not require Low level Format because
   Samsung Drives have been formatted before shipping in the factory.

 - The head/disk assembly is sealed and does not contain any user-
   serviceable components. Tampering with the warranty label will
   void the warranty.


 Warranty
 --------
 The terms of your warranty are determined by your authorized Samsung
 Distributor or Dealer. Warranties do not extend to the data stored
 on Drives.


 Installing your Hard Disk Drive
 -------------------------------
 1. Turn off the system power.

 2. Remove the cover of your computer according to the instructions
    in your system manual.

 3. Master/Slave configuration.

 4. Most interface cables have a red stripe on one side to designate
    Pin 1. Make sure Pin 1 at the cable connector is aligned to Pin 1
    at the drive connector and Pin 1 at the motherboard or interface
    host adapter connector. The maximum cable length is 18 inches
    (0.46m, ATA Rev. 3.0).

 5. Connect the power cable to the drive 4-pin power connector.
    Make sure the connector is fully seated.

 6. When the interface cable, power cable are firmly seated, secure
    the drive in the mounting slot. Use the six #32 UNC screws that
    came yith your SAMSUNG drive. To prevent DAMAGE to the printed
    circuit board assembly, do not over tighten the UNC screws.


 DC Power and pin connector assignments
 --------------------------------------
   +------------+   pin 1    +12 VDC
   | 1  2  3  4 |   pin 2    +12 Volts Return
   \------------/   pin 3    + 5 Volts Return
                    pin 4    + 5 VDC



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SAMSUNG  SHD-30280A/30420A/30560A  USER'S MANUAL 1994

 System startup and operation
 ----------------------------
 1. Turn on the system power.

 2. Run the SETUP program.

 Use a system utility, such as SETUP, to enter the drive configuration
 into the system CMOS. If the CMOS setup utility does not offer our
 drive's configuration and does not support "user defined" drive type,
 select a drive type with a capacity less than or equal to the
 capacity given in the specification. BIOS in present systems may be
 limited to maximum of 1024 cylinders. So SHD-30560A has two
 configurations.

 The BIOS in most systems limits disk drives to 1024 cylinders. If you
 are going to install the SHD-30560A with the default configuration,
 your system should be able to support more than 528MB IDE drive. A
 BIOS or a device driver is required to overcome the limit of
 conventional BIOS. Refer to your system manual. If your system cannot
 recognize this disk size, install the DCF jumper and perform a high-
 level format again. Your system should than recognize the disk size
 as approximately 528MB.

 3. Formatting the drive.

 SAMSUNG low-level formats all AT interface drives at the factory. It
 is not necessary to do a low-level format again.

 CAUTION
 If you partition or format a drive at any level, you lose all of
 data. BACKUP the drive first. SAMSUNG assumes no liability for lost
 user data.


