
M A G - 3 1 8 2 F C    FUJITSU
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3"/SUPERSLIMLINE      Cylinders        |     |     |
Capacity form/unform 18200/      MB        Heads            |     |     |
Seek time   / track   5.5/     ms          Sector/track     |     |     |
Controller           ULTRA2 SCSI LVD       Precompensation
Cache/Buffer          2048 KB              Landing Zone
Data transfer rate   30.000 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM     10025
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h    1000000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
FUJITSU  MAG-3182 ALLEGRO 5E/5LE

 AL5E/5LE 10K RPM Ultra2 Wide LVD SCSI Enterprise Drive
 ------------------------------------------------------
 The latest in high performance enterprise storage, providing an
 incredible 36.4GB capacity in a 1.6" high device.


 Technology Features
 -------------------
 GMR(Giant Magnetoresistive) Heads combined with the latest EPRML
 (Enhanced Partial Response Maximum Likelihood) digital read
 channel enable an industry leading 36.4GB on 3-inch media with the
 same number of platters as previous generation 18.2GB product
 Ultra2 Wide LVD SCSI delivers an astounding 80MB/Sec interface
 data transfer rate to the host, with a maximum cable length of 12,5m.


 Performance Features
 --------------------
 With Internal Data Transfer Rates up to a blistering 45.0MB/Sec,
 Average Seek Times of 5.5ms & a 2048KB Multi-Segmented Buffer,
 these drives are performance enhanced for todays mission critical
 server applications.



 A/V (Audio/Visual) Compatibility
 --------------------------------
 The AL5E/5LE family employs an Embedded Servo System eliminating
 the need for Thermal Recalibration which were the cause of
 interrupted data transfers resulting in lost musical notes or jerky
 video frames.


