
D K 5 1 4 C - 3 8    HITACHI
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders     903|     |     |
Capacity form/unform   321/      MB        Heads          14|     |     |
Seek time   / track  16.0/ 4.0 ms          Sector/track   51|     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation
Cache/Buffer            24 KB FIFO BUFFER  Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                      4.000 MB/S ext SYNC
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 45    |    -20 50
Power: sleep              W     Humidity     %         8 80    |      8 90
       standby            W     Altitude    km                 |
       idle               W     Shock        g         2       |     20
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   48
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
HITACHI  DK514C-38  PRODUCT MANUAL K2500232

  +---------------------------------------------------------+
  |                                            JP198--+1    |
  |                                                +--+2    |
  | (PCB Rev. A/D2 or later)               TM195-+++-+TM199-+
  |                                            |  ||  | XX|
  |                                            |  ||  | XX|
  |                                            |  ||  | XX|
  |                                            +--++--+ XX|
  |                                                     XX|
  |                                                     XX|J1
  |                JP257--+1                            XX|
  |                    +--+2                            XX|
  |                                                     XX|
  |                                                       +-+
  |                                                       XXX J3
  |                    11+--------+1 JP292                XXX
  |                    12+--------+2                        |
  +---------------------------------------------------------+








  +---------------------------------------------------------+
  |                                             JP198-+     |
  |                                                 +-+     |
  | (PCB Rev. A/D1 or former)              TM195-+++-+TM199-+
  |                                            |  ||  | XX|
  |                                            |  ||  | XX|
  |                                            |  ||  | XX|
  |                                            +--++--+ XX|
  |                                                     XX|
  |                                                     XX|J1
  |               JP257+--++--+JP261                    XX|
  |                    2--12--1                         XX|
  |                                                     XX|
  |                                                       +-+
  |                                                       XXX J3
  |                    11+--------+1 JP292                XXX
  |                    12+--------+2                        |
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
HITACHI  DK514C-38  PRODUCT MANUAL K 2500232

 Jumper Setting
 ==============

 x = Shipped at the factory


 Jumper Plug Installation (PCB Rev. A/D2 or later)
 -------------------------------------------------
 The following jumpers are accessible to the user (use green jumper
 plugs):

 JP292 Pins 7 12  SCSI ID setting jumper
 JP292 Pins 5-6   SCSI bus parity jumper
 JP198 Pins 1 4   Terminator power on/off
 JP257 Pins 1-2   Write protection jumper
 JP257 Pins 3-4   Motor Start/Stop option

 NOTE
 The DK514C jumpers other than listed above are installed by the manu-
 facturer and must not be replaced by the user (black jumper plugs).

 NOTE
 The JP261 located near the JP257 is used as for Motor Start/Stop
 jumper in the P/B Rev. 0 and 1 PC board. The JP261 is replaced by
 JP257 (Pin 3-4) in the P/B Rev. 2 or more board.


 JP292  SCSI ID setting jumper
 -----------------------------
   11-+-+-+-+-+1+                  Pins
    |X|X|X|X| | |         11-12   9-10   7-8
   12-+-+-+-+-+2+         CLOSED  CLOSED CLOSED SCSI ID 0 x
     1 2 4 |              OPEN    CLOSED CLOSED SCSI ID 1
     +-+-+ +SCSI Parity   CLOSED  OPEN   CLOSED SCSI ID 2
    SCSI ID               OPEN    OPEN   CLOSED SCSI ID 3
                          CLOSED  CLOSED OPEN   SCSI ID 4
                          OPEN    CLOSED OPEN   SCSI ID 5
                          CLOSED  OPEN   OPEN   SCSI ID 6
                          OPEN    OPEN   OPEN   SCSI ID 7


 JP292 5-6 SCSI Bus Parity Jumper
 --------------------------------
 5-6 OPEN    Disables SCSI Bus parity
     CLOSED  Enables SCSI Bus parity x


 JP198 1-4 Terminator power on/off jumper
 ----------------------------------------
   +3-4+   Pins 1-2
   |xxx|   CLOSED +5V source for terminator is supplied from the SCSI
   |o o|          bus (host) (Pins 3-4 OPEN)
   +1-2+ x OPEN   +5V source for terminator is supplied from the
                  drive controller. (Pins 3-4 CLOSED)

 Note: Terminator power source is supplied to the terminator register
 module from the host that pulls up the SCSI interface signals in the
 controller so that the SCSI bus lines will not be pulled down when
 DK514C power is turned down.


 JP257 1-2 Write Protected
 -------------------------
 1-2 CLOSED  Write protected. The disk can be only read and cannot be
             written.
 1-2 OPEN    Read or write. The disk is enabled for both read and
             write. x


 JP257 3-4 Motor Start/Stop jumper
 ---------------------------------
 3-4 CLOSED  The motor start/stop option is not selected. The spindle
             motor is started when power is turned on. x
     OPEN    The motor start/stop option is selected. The spindle
             motor can be started or stopped by using SCSI command.

 When the motor start/stop option is selected, the drive enters the
 motor stop state when its power is turned on. Use the Start/Stop Unit
 (1BH) command to start or stop the drive.

 NOTE
 When motor start/stop option is not used, the controller does not
 respond to the host about 35 sec from Power turn-on to Drive Ready.

 The terminator of the DK514C other than the last drive of SCSI Daisy
 Chain MUST be removed.


 Jumper Plug Installation (PCB Rev. A/D1 or former)
 --------------------------------------------------
 The following jumpers are accessible to the user (use green jumper
 plugs):

 JP292 Pins 7 12  SCSI ID setting jumper
 JP292 Pins 5-6   SCSI bus parity jumper
 JP198            Terminator power on/off
 JP257            Write protection jumper
 JP261            Motor Start/Stop option

 NOTE
 The DK514C jumpers other than listed above are installed by the manu-
 facturer and must not be replaced by the user (black jumper plugs).

 NOTE
 The JP261 located near the JP257 is used as for Motor Start/Stop
 jumper in the P/B Rev. 0 and 1 PC board. The JP261 is replaced by
 JP257 (Pin 3-4) in the P/B Rev. 2 or more board.


 JP292  SCSI ID setting jumper
 -----------------------------
   11-+-+-+-+-+1+                  Pins
    |X|X|X|X| | |         11-12   9-10   7-8
   12-+-+-+-+-+2+         CLOSED  CLOSED CLOSED SCSI ID 0 x
     1 2 4 |              OPEN    CLOSED CLOSED SCSI ID 1
     +-+-+ +SCSI Parity   CLOSED  OPEN   CLOSED SCSI ID 2
    SCSI ID               OPEN    OPEN   CLOSED SCSI ID 3
                          CLOSED  CLOSED OPEN   SCSI ID 4
                          OPEN    CLOSED OPEN   SCSI ID 5
                          CLOSED  OPEN   OPEN   SCSI ID 6
                          OPEN    OPEN   OPEN   SCSI ID 7


 JP292 5-6 SCSI Bus Parity Jumper
 --------------------------------
 5-6 OPEN    Disables SCSI Bus parity
     CLOSED  Enables SCSI Bus parity x


 JP198 Terminator power on/off jumper
 ------------------------------------
   CLOSED +5V source for terminator is supplied from the SCSI
          bus or the controller.
 x OPEN   +5V source for terminator is supplied only from the
          controller.

 Note: Terminator power source is supplied to the terminator register
 module from the host that pulls up the SCSI interface signals in the
 controller so that the SCSI bus lines will not be pulled down when
 DK514C power is turned down.


 JP257 Write Protected
 ---------------------
 CLOSED  Write protected. The disk can be only read and cannot be
         written.
 OPEN    Read or write. The disk is enabled for both read and
         write. x


 JP261 Motor Start/Stop jumper
 -----------------------------
 CLOSED  The motor start/stop option is not selected. The spindle
         motor is started when power is turned on. x
 OPEN    The motor start/stop option is selected. The spindle
         motor can be started or stopped by using SCSI command.

 When the motor start/stop option is selected, the drive enters the
 motor stop state when its power is turned on. Use the Start/Stop Unit
 (1BH) command to start or stop the drive.

 NOTE
 When motor start/stop option is not used, the controller does not
 respond to the host about 35 sec from Power turn-on to Drive Ready.

 The terminator of the DK514C other than the last drive of SCSI Daisy
 chain MUST be removed.


