
S T 3 2 5 3 2 A   M E D A L I . 2 5 3 2    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 4956|  619| 1024
Capacity form/unform  2557/      MB        Heads           6|   16|     |   16
Seek time   / track  13.0/ 3.0 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA3 ULTRA      Precompensation
Cache/Buffer           128 KB              Landing Zone
Data transfer rate   10.000 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext UDMA
Recording method     RLL 1/7,ZBR 2/3                operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby        1.0 W     Altitude    km                 |
       idle           4.8 W     Shock        g         5       |     75
       seek           6.6 W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST32532A  JUMPER SETTING

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         1XXE
  |                                                         |+-+
  |                                                         || |Jumper
  |                                                         |+-+1
  |                                             +-+         |XX Power
  |                                             +-+         |XX
  +---------------------------------------------------------+  12V




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST32532A  JUMPER SETTING

   REAR VIEW

                              J2  40 pin I/O Cable Connection
                              |   pin-20 removed
                              |
                   +----------+---------+-----1-+---------+    TOP
 HDA              -+::::::::::*::::::::1| : : : | 0 0 0 0 +--
                   +--------------------+-+-+-+-+-5-G-G-12+    BOTTOM
                                          | | |
                   Master ON, Slave OFF --+ | |
         Slave Present (when Master ON) ----+ |
          Cable Select (when Slave OFF) ----+ |
                               Reserved ------+
                                                   o o1
                                                   o o2
                                                   | |
                   Limit capacity to 2.1 Gbytes ---+ |
                               (4092 cylinders)      |
                     Full capacity (as shipped) -----+

 Limit Capacity jumper sets the default cylinder translation to 4092
 to solve issues with certain BIOS that only auto-detect.

 Total available sectors are still at full capacity as reported via
 Identify Drive data words 52 - 61.  Third party partitioning software
 may be needed to achieve full capacity if this option jumper is used.


