
S T 1 4 8 0 N V    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    1476|     |     |
Capacity form/unform   426/  492 MB        Heads           9|     |     |
Seek time   / track  14.0/ 2.5 ms          Sector/track     |     |     |
Controller           SCSI1 NOVELL          Precompensation
Cache/Buffer            64 KB SEGMENTED    Landing Zone
Data transfer rate    2.588 MB/S int       Bytes/Sector      512
                      5.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 70
Power: sleep              W     Humidity     %         8 80    |      5 95
       standby            W     Altitude    km    -0.305  3.048| -0.305 12.210
       idle           9.0 W     Shock        g        10       |     50
       seek               W     Rotation   RPM      4412
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   48
                                MTBF         h     150000
                                Warranty Month        12
Lift/Lock/Park     YES          Certificates     CSA,SDA,FCC,IEC380,IEC435,...

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST1400N/1401N/1480N  PRODUCT MANUAL 77765458-A

  +------------------------------------------------1--------+  1
  1-+-+                                          J5++++++   |XX Power
  |-| |J7                                          +----+   |XX J3
  |-+-+                                                     |
  |                                                         |X1 SCSI
  |                                                    +1   |XX I/O
  |                                                    ||   |XX J4
  |                                       I/O          ||   |XX
  |                                       Terminators  ++   |XX
  |                                                    +1   |XX
  |                                                    ||   |XX
  |                                                    ||   |XX
  |                                                    ++   |XX
  |                                                    +1   |XX
  |                                                    ||   |XX
  |                                                    ||   |XX
  |             +-----+J6                              ++   |XX
  |             +++++++                                     |XX
  +-------------2-------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST1400N/1401N/1480N  PRODUCT MANUAL 77765458-A

 Jumper setting
 ==============

  J6  Motor Start/Write Protect/Terminator Power
  ----------------------------------------------

      +----------------------+-----------------------+
      |                      | 1  2  3  4  5  6  7  8|
      +----------------------+-----------------------+
      |Enable Motor Start    | o  X  o  o  o  o  o  o|
      |                      | 1  X  o  o  o  o  o  o|
      +----------------------+-----------------------+
      |Delay Motor Start     | o  o  x  o  o  o  o  o|
      |                      | o  o  X  o  o  o  o  o|
      +----------------------+-----------------------+
      |Write Protect         | o  o  o  x  o  o  o  o|
      |                      | o  o  o  X  o  o  o  o|
      +----------------------+-----------------------+
      |Parity Option         | o  o  o  o  x  o  o  o|
      |                      | o  o  o  o  X  o  o  o|
      +----------------------+-----------------------+
      |Terminator Power to   | o  o  o  o  o  o  x  o|
      |SCSI Bus              | o  o  o  o  o  o  X  o|
      +----------------------+-----------------------+
      |Terminator Power from | o  o  o  o  o  o  o  x|
      |Drive                 | o  o  o  o  o  o  o  X|
      +----------------------+-----------------------+
      |Terminator Power from | o  o  o  o  o  o  xxxx|
      |SCSI Bus              | o  o  o  o  o  o  o  o|
      +----------------------+-----------------------+

 J6   1           For Factory use only

      2   CLOSED  Enables Motor Start option. The drive waits for the
                  Start unit command from the host before starting
                  spindle motor.
          OPEN    Drive operation depends on whether or not there is a
                  jumper in position 3.

      3   CLOSED  Enables the Delayed Motor Start option (if jumper in
                  position 3 is off). Motor start delay is 16 times
                  the drive ID number in seconds; i.e., drive ID 0
                  immediately, drive one starts 16 seconds later etc.

      4  CLOSED   Entire drive is write protected.

      5  CLOSED   Parity checking by the drive is enabled.

      6           Reserved for later use.

      7,8         Select terminator power source. In position 7 drive
                  supplies power to the SCSI bus, pin 26. In position
                  8 the drive supplies power only to its own
                  terminators. Jumper horizontally, lower part,
                  between positions 7 and 8 means drive takes power
                  from the SCSI bus, pin 26. Jumpers on both 7 and 8
                  at the same time is allowed.


  J5  SCSI ID
  -----------
      +------------+----------+
      |            | 1  2  3  |
      +------------+----------+
      |SCSI ID = 0 | o  o  1  |
      |            | o  o  o  |
      +------------+----------+
      |SCSI ID = 1 | o  o  x  |
      |            | o  o  X  |
      +------------+----------+
      |SCSI ID = 2 | o  x  o  |
      |            | o  X  o  |
      +------------+----------+
      |SCSI ID = 3 | o  x  x  |
      |            | o  X  X  |
      +------------+----------+
      |SCSI ID = 4 | x  o  o  |
      |            | X  o  o  |
      +------------+----------+
      |SCSI ID = 5 | x  o  x  |
      |            | X  o  X  |
      +------------+----------+
      |SCSI ID = 6 | x  x  o  |
      |            | X  X  o  |
      +------------+----------+
      |SCSI ID = 7 | x  x  x  |
      |            | X  X  X  |
      +------------+----------+


  J7  SCSI ID
  -----------
      +------------+---------------+
      |            | 1  2  3  4  5 |
      +------------+---------------+
      |SCSI ID = 0 | o  o  o  o  o |
      |            | 1  o  o  o  o |
      +------------+---------------+
      |SCSI ID = 1 | o  o  x  o  o |
      |            | o  o  X  o  o |
      +------------+---------------+
      |SCSI ID = 2 | o  x  o  o  o |
      |            | o  X  o  o  o |
      +------------+---------------+
      |SCSI ID = 3 | o  x  x  o  o |
      |            | o  X  X  o  o |
      +------------+---------------+
      |SCSI ID = 4 | x  o  o  o  o |
      |            | X  o  o  o  o |
      +------------+---------------+
      |SCSI ID = 5 | x  o  x  o  o |
      |            | X  o  X  o  o |
      +------------+---------------+
      |SCSI ID = 6 | x  x  o  o  o |
      |            | X  X  o  o  o |
      +------------+---------------+
      |SCSI ID = 7 | x  x  x  o  o |
      |            | X  X  X  o  o |
      +------------+---------------+
      |Sync Spindle| o  o  o  x  o |
      |            | o  o  o  X  o |
      +------------+---------------+
      |Remote LED  | o  o  o  o  x |
      |            | o  o  o  o  X |
      +------------+---------------+

 Either J5 or J7 may be used to select drive ID. Both should not be
 used at the same time. The drive ID is binary coded positionwise
 (least significant position on the right), i.e. jumper in position
 1 is drive ID 1 etc.


 J7  Sync Spindle
 ----------------
 4   Used as a cable connection for the REF Index/+L signal
     for sync spindle feature. When no cable is connected, a jumper
     must be installed. OEM standard drives are shipped with jumper
     installed.


 J7  Remote LED
 --------------
 5   Used if needed for a connection to a remotely located LED
     indicator.Pin 10 (bottom), the anode connection, connects in the
     drive to the +5V supply through a pull-up resistor. Pin 9
     (top), the cathode connection connects in the drive to signal
     common through the emitter-collector jumction of a transistor
     switch that controls the LED on/off condition.


 50-Pin Single-ended cable Pin Assignments
 (Nonshielded Connector)
 -----------------------------------------
    Signal    Pin No.    Signal     Pin No.
    ----------------------------------------
    -DB(0)       2       Ground       28
    -DB(1)       4       Ground       30
    -DB(2)       6       -ATN         32
    -DB(3)       8       Ground       34
    -DB(4)      10       -BSY         36
    -DB(5)      12       -ACK         38
    -DB(6)      14       -RST         40
    -DB(7)      16       -MSG         42
    -DB(P)      18       -SEL         44
    Ground      20       -C/D         46
    Ground      22       -REQ         48
    Ground      24       -I/O         50
    TERMPWR     26

  Note: All odd pins, except pin-25 are connected to ground. Pin-25
        is left open.

 Pin 25 must not be connected to ground at the HOST end or the drive
 end of the cable. If the I/O connector should accidentally be plugged
 in upside down, terminator power on Pin 26 will be shorted to ground.

 The minus sign next to the signals indicates asserted state is the
 low voltage of the two levels used for logic signals.



 J3   DC Power and pin connector assignments
 -------------------------------------------
      +------------+     1 = + 12 V
    --+ 4  3  2  1 +--   2 = + 12 V Return
      +------------+     3 = +  5 V Return
                         4 = +  5 V



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SEAGATE  ST1400N/1401N/1480N  PRODUCT MANUAL 77765458-A

 Notes on installation
 =====================

 Drive Orientation
 -----------------
 The balanced rotary arm actuator design of the drive allows it to
 be mounted in any orientation. All drive performance characterization
 however, has been done with the drive in horizontal (disc level) and
 vertical (drive on its side) orientations, and these are the two
 preferred mounting orientations.

 The drive is designed, manufactured, and tested with a "Plug-in and
 Play" installation philosophy. This philosophy minimizes the
 requirements for highly trained personnel to integrate the drive
 into an OEM's system, wether in a factory or field environment.

 - Insure that the SCSI ID of the drive is not the same as the host
   adapter. Most host adapters use SCSI ID 7.

 - If multiple devices are on the bus insure that the SCSI ID of the
   drive is not already used by other devices on the bus.

 - If the drive is the only device on the bus it should be attached to
   end of the SCSI bus cable, and terminators should be installed
   (provided external terminators are not used).

 - If the drive is attached to a bus already containing other devices,
   and the drive is not attached to the end of the bus, the
   terminators should be removed.

 - Set all appropriate option jumpers for desired operation prior to
   power on. If jumpers are changed after power has been applied the
   drive must be power cycled for the new settings to be affect.

 - In all cases additional drives or software will be necessary to
   logically install the drive onto the system.


 Cooling
 -------
 Cabinet cooling must be designed by the customer so that the
 ambient temperature immediately surrounding the drive will not exceed
 temperature conditions. Specific consideration should be given to
 make sure adequate air circulation is present around the components
 on the PWA at the rear of the drive.


 Service Tools
 -------------
 No special tools are required for site installation or recommended
 for site maintenance. The depot repair philosophy of the drive
 precludes the necessity for special tools. If field repair of items
 external to the HDA is desired, a 6 point Torx T10 driver is
 required. This may be purchased through most commercial tool
 catalogs.


 Air Cleanliness
 ---------------
 The drive is designed to operate in a typical office environment with
 minimal environment control.


 Physical Description
 --------------------
 The drive may be chained together
 or with other compatible SCSI devices using a common cable. Both end
 of the cable must be terminated. The drive implements single ended
 drivers and receivers which allow a maximum cable length of six
 metres (19.6 feet) (primarily for connection within a cabinet). All
 signals are common between all SCSI devices. The drive may be daisy-
 chained only with SCSI devices having the same type drivers and re-
 ceivers. Devices having single-ended interface circuits cannot be on
 on the same daisy chain with devices having differential interface
 circuits. A maximum of 8 SCSI devices (including the Host) may be
 daisy chained together. The SCSI device at both ends of the daisy
 chain are to be terminated. Intermediate SCSI devices shall not be
 terminated. Remove the terminator resistor packs, not the terminator
 power source selector jumper.


 Cable Characteristics
 ---------------------
 Only nonshielded cable connectors are applicable. A 50 conductor flat
 cable or 25 twisted pair cable shall be used. The maximum total cable
 length shall be 6.0 metres more than 0.1 metre off the mainline
 interconnection within any connected equipment. An ideal impedance
 match with cable terminators implies a cable characteristic impedance
 of 132 ohm. In general, cables having characteristic impedance of
 those values are not available; however impedances that are somewhat
 lower are satisfactory. A characteristic impedance of 100 ohm   10%
 is recommended for unshielded flat or twisted pair ribbon cable.
 However, most available cables have a somewhat lower characteristic
 impedance. To minimize discontinuities and signal reflections, cables
 of different impedances should not be used in the same bus.
 Implementations may require trade-offs in shielding effectiveness,
 cable length, the number of loads, transfer rates, and cost to
 achieve satisfactory system operation. If shielded and unshielded
 cables are mixed within the same SCSI bus, the effect of impedance
 mismatch must be carefully considered.

 A minimum conductor
 size of 28 AWG should be used to minimize noise effects.

 Suggested nonshielded flat cable part numbers are:
   Flat cable -   35M-3365-50
   Twisted pair - Spectra Twist in flat 455-248-50
 Equivalent parts may be used.


    +--------------SCSI-DEVICE-----------------+
    |       +--+ HOST ADAPTER/INITIATOR ***    |
    |       |T |                               |
    +-------++-+-------------------------------+
            *|
             |
             |                1 thru 8 SCSI devices
             +---------------+--------------+
           **|             **|              |*
    +--------+---+ +---------+--+ +--------++-++
    |Disc Drive  | |Disc Drive  | |Disc    | T||
    |or other    | |or other    | |Drive or+--+|
    |SCSI device | |SCSI device | |other SCSI  |
    +------------+ +------------+ +------------+

 *    Closed end type connector used
 **   Open type (in-line application) Connector used.
 ***  Host need not beon the end of the daisy chain. Another device
      can be on the end with the terminator, the host having no
      terminator.

 T indicates termination required.


 DC Cable and Connector
 ----------------------
 The drive receives DC power through a 4 pin rigth angle connector
 mounted on the servo PWA. Recommended part numbers for the mating
 connector are listed below, but equivalent parts may be used.

 Type of cable:      18 AWG
 Connector:          AMP 1-480424-0
 Contacts:           AMP 60619-4 (Loose Piece); AMP 61117-4 (Strip)


 Connector Requirements
 ----------------------
 The nonshielded cable connector shall be a 50 conductor connector
 consisting of two rows of 25 female contacts with adjacent contents
 100 mils apart.

 Recommended Mating Flat Cable Connector Part Numbers are:

 Closed end   3M-3425-7000      W/O Strain Relief, No Center Key
 (for cable   3M-3425-7050      With Strain Relief, No Center Key
 ends)        Dupont-66900-290  With Strain Relief, With Center Key

 Open end     3M-3425-6000      W/O Strain Relief, No Center Key
 (In Daisy-   3M-3425-6050      With Strain Relief, No Center Key
 chain)       Dupont-66900-250  With Strain Relief, With Center Key

 The drive device connector is a nonshielded 50 conductor connector
 consisting of two rows of 25 male pins with adjacent pins 100 mils
 apart. The connector is keyed. The drive connector Part Number:
 Dupont 88049-002 or equivalent.


 Drive Termination
 -----------------
 This otpion may be incorporated during manufacture at the request of
 the customer. For single ended interface drives, termination consists
 of three 220/330 ohm resistor modules (SIP's) which are installed on
 the Main PWA via sockets.
 The Reference Index Signal is terminated with a 2K ohm resistor. The
 termination resistor is permanetly installed in each drive in the
 reference signal daisy chain.


 Terminator Power
 ----------------
 The drive may be configured to accept terminator power via pin 26 of
 the SCSI Bus, to supply power to the SCSI bus or to provide
 terminator power for optional internal termination resistors via the
 drive power connector. The drive can provide power both to its own
 terminators and to the SCSI Bus terminator power line (Pin 26).

 SCSI devices providing termination power (TERMPWR) shall have the
 following characteristics:

   V TERM = 4.0 V to 5.25 V
   800 mA min source drive capability
   1.0 A maximum


 Synchronized Spindle operation
 ------------------------------
 The interface consists of a twisted pair cable that connects the
 drives in the synchronized system in a daisy chain configuration.
 Master/slave operation will be automatically set by the drives in
 the system at power up time, or each drive in the system can be
 configured by the host (using Mode Select command) to operate in
 either the master or slave mode. While loading heads after power up,
 a drive checks for occurrences of the reference index signal. Drives
 can be re-configured by the host any time after power up to be
 master or slave by use of the Mode Select command Rigid Disc Drive
 Geometry page. The master provides the reference signal to which all
 other drives phase lock, including the master. There is only one
 master per system, and that can be a drive or the host computer. All
 drives may be configured as slaves allowing the host to provide the
 reference signal. All drives default to the synchronious mode when
 powered up.
 Each drive can later be configured for the non-synchronized mode in
 which it ignores the reference index signal that might be present.
 The connection to the host is required only if the host is to
 provide the reference signal. If the host does not provide the
 reference signal, the host should not be connected.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SEAGATE  ST1400N/1401N/1480N  PRODUCT MANUAL 77765458-A

 Standards
 ---------
 The drive has been developed as a system peripherals to the highest
 standards of design and construction. The drives depends upon its
 host equipment to provide adequate power and environment in order to
 achieve optimum performance and compliance with applicable industry
 and governmental regualations. Special attention must be given in the
 areas of safety, power distribution, shielding, audible noise
 control, and temperature regulation.


 The drive is a UL Recognized component per UL 478 and a CSA Certified
 Component per CSA C22.2, No. 220-M1986. It also meets the
 requirements of DIN IEC 380/VDE 0806/8.81, DIN IEC 435/VDE 0805/11.84
 and EN 60 950/9.87.

 The drive, as delivered, is designed for system integration before
 use. It is supplied as a component or subassembly as defined in the
 FCC Rules and Regulations, Part 15, Subpart J governing EMI of
 computing devices end the Radio Interference Regulations of the
 Canadian Department of Communications. The drive is, therefore not
 directly subject to the FCC rules and regulations or the Radio
 Interference Regulations of the Canadian Department of
 Communications.


 Media Description
 -----------------
 The media used on the drive has a diameter of approximately 3.5
 inches (89mm). The aluminium substrate is coated with a thin film
 magnetic material, overcoated with a proprietary protective layer
 for improved durability and environmental protection.


 Defect and Error Management
 ---------------------------
 The drive, as delivered, complies with this specification. The read
 error rate and specified storage capacity are not dependent upon use
 of defect management routines by the host (initiator).

 Defect and error management in the SCSI systm involves the drive
 internal defect/error management and SCSI systems error
 considerations (errors in communications between Initiator and the
 drive).


 Power Sequencing
 ----------------
 Power sequencing is not required for the drive. The drive protects
 against inadvertent writing during power up and down. Daisychain
 operation requires that power be maintained on the terminated unit
 to ensure proper termination of the peripherals I/O cables.


 Temperature
 -----------
 The drive will meet all specification over 41*F to 122*F (5*C to
 50*C) operating ambient temperature range with a maximum gradient of
 36* F (20* C) per hour.


 Heat/Power Dissipation
 ----------------------
 Typical dissipation is 12 watts (41 BTUs per hour) of DC power
 average at nominal voltages. Typical power dissipation under idle
 conditions is no greater than 9 watts (30.7 BTUs per hour).


 Seek Time
 ---------
                      Drive Level
                                          | ST1400N|        |
                                          | ST1480N| ST1401N|
        ----------------------------------+--------+--------+
        Track-to-Track         msec. typ. |   2.5  |   2.5  |
                               msec. max. |   4.5  |   4.5  |
                       Average msec. typ. |  14    |  12    |
                       Average msec. max. |  16    |  14    |
        Full Stroke            msec. typ. |  26    |  24    |
                               msec. max. |  32    |  28    |
        Latency                msec. avg. |   6.80 |   6.80 |
        ----------------------------------+--------+--------+


                      Including Controller Overhead
                      (without disconnect)
                                          | ST1400N|        |
                                          | ST1480N| ST1401N|
        ----------------------------------+--------+--------+
        Track-to-Track         msec. typ. |   3.1  |   3.1  |
                               msec. max. |   5.1  |   5.1  |
                       Average msec. typ. |  14.7  |  12.7  |
                       Average msec. max. |  16.7  |  14.7  |
        Full Stroke            msec. typ. |  26.7  |  24.7  |
                               msec. max. |  32.8  |  28.8  |
        Latency                msec. avg. |   6.80 |   6.80 |
        ----------------------------------+--------+--------+



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
SEAGATE   SUPPORT SERVICES

 Seagate Technology
 ------------------
 Technical Support Services
 If you need assistance installing your drive, consult your dealer.
 Dealers are familiar with their unique system configurations and can
 help you with system conflicts and other technical issues. If you
 need additional assistance with your Seagate(r) drive or other
 Seagate products, use one of the Seagate technical support services
 listed below.

 SeaFONE at 1-800-SEAGATE (1-800-732-4283)
 Seagate's 800 number allows toll-free access to automated self-help
 services, providing answers to commonly asked questions,
 troubleshooting tips and specifications for disc drives and tape
 drives. This service is available 24 hours daily and requires a
 touch-tone phone. If you need to speak to a technical support
 engineer, dial this number and listen to the options for technical
 support. (International callers can also reach this automated
 self-help service by dialing 408-456-4496).


 Seagate Technology online services
 Using a modem, you can obtain troubleshooting tips, free utility
 programs, drive specifications and jumper settings for Seagate's
 entire product line. You can also download software for installing
 and analyzing your drive.

 SeaNET
 You can obtain technical information on Seagate drives, Seagate
 software and much more over the Internet from Seagate's World Wide
 Web home page (http://www.seagate.com) or Seagate's ftp server
 (ftp://ftp.seagate.com).

 You may also send E-mail with your questions to DiscSupport@
 Seagate.com or TapeSupport@Seagate.com.


 SeaBOARD
 SeaBOARD is a computer bulletin board system (BBS) that contains
 information about Seagate's disc and tape drive products and is
 available 24 hours daily. Set your communications software to eight
 data bits, no parity and one stop bit (8-N-1). SeaBOARD phone numbers
 are listed in the following table.

 BBS Location           Modem number
 United States      Disc: 408-434-1080; Tape: 408-456-4415
 England            44-1628-478011
 France                         33 1-48 25 35 95
 Germany            49-89-140-9331
 Singapore          65-292-6973
 Thailand           662-531-8111
 Australia          61-2-9756-2359
 Taiwan             886-2-719-6075

 Seagate CompuServe forum
 Online technical support for Seagate products is available on
 CompuServe. To access our technical support forum, type go seagate.
 This forum provides information similar to that found on SeaBOARD.
 In addition, you can type questions or browse through previous
 questions and answers on the forum messages.

 Seagate Technology FAX services
 SeaFAX
 You can use a touch-tone telephone to access Seagate's automated FAX
 system to receive technical support information by return FAX. This
 service is available 24 hours daily.
 Location               Telephone number
 United States          1-800-SEAGATE or 408-456-4496
 England                44-1628-894084
 Australia              61-2-9756-5170

 Seagate technical support FAX
 You can FAX questions or comments to technical support specialists 24
 hours daily. Responses are sent during business hours.
 Location               FAX number
 United States          408-944-9120
 England                        44-1628-890660
 France                 33 1-46 04 42 50
 Germany                        49-89-1430-5100
 Australia              61-2-9725-4052
 Singapore              65-293-4722
 Hong Kong              852-2368 7173
 Taiwan                 886-2-715-2923
 Korea                          82-2-556-7294/4251


 Seagate technical support
 You can talk to a technical support specialist during business hours
 Monday through Friday for one-on-one technical help.  Before calling,
 note your system configuration and drive model number (STxxxx). There
 are several technical support phone numbers available for various
 Seagate products.

 Location          Telephone  number
 United States Please dial 1-800-SEAGATE for the specific product
               telephone number.
               (6:00 A.M. to 11:15 A.M., 12:30 P.M. to 5:00 P.M.,
               Pacific time, M-F)
 England       44-1628-894083 (10:00 A.M. to 1:00 P.M., 2:00 P.M. to
               5:00 P.M., M-F)
 France        33 1-41 86 10 86 (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Germany       Disc: 49-89-140-9332; (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 4:00 P.M., M-F)
               Tape: 49-89-140-9333
 Australia     61-2-9725-3366 (9:00 A.M. to 5:00 P.M., M-F)
 Singapore     65-290-3998 (9:00 A.M. to 12:00 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Hong Kong     852-2368 9918
 Taiwan        886-2-514-2237
 Korea         82-2-556-8241


 SeaTDD 408-944-9121
 Using a telecommunications device for the deaf (TDD), you can send
 questions or comments 24 hours daily and exchange messages with a
 technical support specialist between 6:00 A.M. to 11:15 A.M. and
 12:30 P.M. to 5:00 P.M. (Pacific time) Monday through Friday.


 Customer Service Centers
 Seagate direct OEM, Distribution, System Integrator and Retail
 customers should contact your Seagate Service Representative for
 warranty information.  Other customers contact your place of
 purchase.  Seagate offers comprehensive customer support for all
 Seagate drives.  Seagate customer service centers are the only
 facilities authorized to service Seagate drives. These services are
 available worldwide.

 Location                       Telephone number                FAX number
 United States          1-800-468-3472;                 405-949-6740
 Other Americas
 (Canada & Brazil)      405-949-6706;               405-949-6738
 Mexico                         525-546-6965;                   525-546-4888
 Europe, Middle
 East & Africa          31-2065-43300;              31-2065-34320
 Asia Pacific &
 Australia              65-485-3595;                    65-485-4980
 Japan                          81-3-5462-2904;                 81-3-3462-2979


 Seagate, Seagate Technology and the Seagate logo are registered
 trademarks of Seagate Technology, Inc. SeaFAX, SeaFONE, SeaBOARD,
 SeaTDD, SeaNET, Medalist and DiscWizard are either trademarks or
 registered trademarks of Seagate Technology, Inc. or one of its
 subsidiaries. All other trademarks or registered trademarks are the
 property of their respective owners.


