
S T 4 3 7 6 N    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/HH              Cylinders    1549|     |     |
Capacity form/unform   330/  376 MB        Heads           9|     |     |
Seek time   / track  17.5/ 4.0 ms          Sector/track     |     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation
Cache/Buffer            32 KB              Landing Zone
Data transfer rate    1.875 MB/S int       Bytes/Sector      512
                      4.700 MB/S ext SYNC
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek          27.0 W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     100000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST4350N/ST4376N  JUMPER SETTING

 Jumper Setting
 ==============


  Connects CHASIS ground to ground lug ------------+
  Connects SIGNAL ground to ground lug ----------+ |
                     Drive Select ID's -----+    | |
             Motor Start Option enable -+   |    G G
            Parity Check Option enable+ | +-+-+ +1+2+
                                     +P M 4 2 1+|o|o|    POWER
                                     |o o o o o||o|o|   +---------+
                                     |o o o o o|+-+-+   | O O O O |
 ------------------------------------+---------+--------+---------PWA-
 -+------+---+-------------------------+--------+--------+--Data-PWA--
  1------+   |XXXXXXXXXXXXXXXXXXXXXXXXX| +-+    1--------+
 Terminator  +------------------------1+ |o| o   Terminator
               INTERFACE                 |o+-o
                                         +++
 TERMPWR (+5v) from drive (vertical) -----+
 TERMPWR from the Bus (lower horizontal)


