
S T 1 1 7 0 0 N    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    2626|     |     |
Capacity form/unform  1430/ 1700 MB        Heads          13|     |     |
Seek time   / track  10.0/ 2.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate    4.000 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 70
Power: sleep              W     Humidity     %                 |
       standby        9.0 W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     500000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST11700N/12400N  PRODUCT DESCRIPTION

  +---------------------------------------------------------+
  |1-+                                         +---1 J5     |XX
  || |J6                                       +---+        |XX SCSI
  |+-+                                                  +1  |XX I/O
  |                                                     ||  |XX
  |                                                     ||  |XX
  |                                        Terminating  ++  |XX
  |                                        Resistors    +1  |XX
  |                                                     ||  |XX
  |                                                     ||  |XX
  |                                                     ++  |XX
  |                                                     +1  |XX
  |                                                     ||  |XX
  |                                                     ||  |XX
  |                                                     ++  |X1
  |                                                         |
  ++LED                           +---------1 J2            |XX Power
  ++                              +---------+               |XX
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST11700/12400-N  PRODUCT DESCRIPTION

 Jumper setting
 ==============

 Each disk drive has one or more option select header connectors on
 the back, side or front where jumper plugs are installed to select
 the way that the drive is to be configured or to select its ID on the
 I/O bus.


 J2  Motor Start/Write Protect/Terminator Power
 ----------------------------------------------

              Position Numbers
          +-1--2--3--4--5--6--7--8-+         X J3 Power
 ---------+ o  X  o  o  o  o  o  1 +---------X
          | o  X  o  o  o  o  xxxx |
          +----+-------------------+ \ Position A
              Position 2

     1   for Factory use only.

     2   Jumper installed in position 2 enables the Delayed Motor
         Start option (if jumper in position 3 is off). Motor start
         delays is 16 times the drive ID number in seconds; i.e. drive
         ID 0 starts immediately. Drive one starts 16 seconds later,
         etc.

     3   Jumper installed enables Motor Start option. The drive waits
         for the Start unit command from the host before starting the
         spindle motor. If no jumper is installed, drive operation de-
         pends on wether or not there is a jumper in position 2.

         If jumpers 2 and 3 are both off, drive spins up with no delay
         when power is applied.

     4   Jumper installed means entire drive is write protected.

     5   Jumper installed means parity checking by the drive is
         enabled.

     6   Enables Terminator Resistor

     7   Select terminator power source. In position 8 the drive
     8   supplies power to the SCSI bus, pin 26. In position 7 drive
         supplies power only to its own terminators. (Factory setting)
         Jumper horizontally between positions 7 and 8 (position A)
         means the drive takes power from the SCSI bus, pin 26.
         Jumpers installed on both 7 and 8 at same time is allowed.
         Default is jumper on position 7.


 J5 SCSI ID
 ----------
           SCSI ID 0        SCSI ID 1        SCSI ID 2
          +---------+      +---------+      +---------+
          | o  o  1 |      | X  o  o |      | o  X  o |
          | o  o  o |      | X  o  o |      | o  X  o |
        A +-0--1--2-+      +---------+      +---------+

           SCSI ID 3        SCSI ID 4        SCSI ID 5
          +---------+      +---------+      +---------+
          | X  X  o |      | o  o  X |      | X  o  X |
          | X  X  o |      | o  o  X |      | X  o  X |
          +---------+      +---------+      +---------+

           SCSI ID 6        SCSI ID 7
          +---------+      +---------+
          | o  X  X |      | X  X  X |
          | o  X  X |      | X  X  X |
          +---------+      +---------+

 Drive ID on SCSI Bus (J6 may be used instead). The drive ID is binary
 coded positionwise.


 J6 SCSI ID (optional)
 ---------------------

       A  A  A                         SCSI ID 0
     +-2--1--0----------+             +------------------+
     | o  o  o  o  o  1 |             | o  o  o  o  o  o |
     | o  o  o  o  o  o |             | o  o  o  o  o  o |
     +-1--2--3--4--5--6-+             +------------------+

      SCSI ID 1                        SCSI ID 2
     +------------------+             +------------------+
     | o  o  X  o  o  o |             | o  X  o  o  o  o |
     | o  o  X  o  o  o |             | o  X  o  o  o  o |
     +------------------+             +------------------+

      SCSI ID 3                        SCSI ID 4
     +------------------+             +------------------+
     | o  X  X  o  o  o |             | X  o  o  o  o  o |
     | o  X  X  o  o  o |             | X  o  o  o  o  o |
     +------------------+             +------------------+

      SCSI ID 5                        SCSI ID 6
     +------------------+             +------------------+
     | X  o  X  o  o  o |             | X  X  o  o  o  o |
     | X  o  X  o  o  o |             | X  X  o  o  o  o |
     +------------------+             +------------------+


      SCSI ID 7                        Sync Spindle
     +------------------+             +------------------+ Pin 6
     | X  X  X  o  o  o |             | o  o  o  X  o  o | REF SIG+
     | X  X  X  o  o  o |             | o  o  o  X  o  o |
     +------------------+             +------------------+


      Remote LED
     +------------------+  Pin 3
     | o  o  o  o  X  o |  +5V
     | o  o  o  o  X  o |
     +------------------+

 1,2,3  Either J5 or J6 (optional) may be used to select drive ID.
        Both should not be used at same time, because at some future
        time, settings may be changed, causing the drive to not
        respond correctly. The factory installs no ID jumpers on J5 or
        J6 (drive ID 0).

     4  Spindle Synchronization

     5  Used if needed for a connection to a remote LED indicator.

     6  Reserved.


 On SCSI I/O drives either J6 (on the front of the drive) or J5 (on
 the side behind the DC Power connector) may be used to set the drive
 ID. To avoid possible incorrect ID setting, do not use both J5 and
 J6 for ID selection.



 J3   DC Power and pin connector assignments
 -------------------------------------------
 -------------------+
 --+  +-----J3-----+|  pin 1    +12 VDC
  1|  | 4  3  2  1 ||  pin 2    +12 Volts Return
  -+  +------------+|  pin 3    + 5 Volts Return
  ------------------+  pin 4    + 5 VDC



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
SEAGATE   SUPPORT SERVICES

 Seagate Technology
 ------------------
 Technical Support Services
 If you need assistance installing your drive, consult your dealer.
 Dealers are familiar with their unique system configurations and can
 help you with system conflicts and other technical issues. If you
 need additional assistance with your Seagate(r) drive or other
 Seagate products, use one of the Seagate technical support services
 listed below.

 SeaFONE at 1-800-SEAGATE (1-800-732-4283)
 Seagate's 800 number allows toll-free access to automated self-help
 services, providing answers to commonly asked questions,
 troubleshooting tips and specifications for disc drives and tape
 drives. This service is available 24 hours daily and requires a
 touch-tone phone. If you need to speak to a technical support
 engineer, dial this number and listen to the options for technical
 support. (International callers can also reach this automated
 self-help service by dialing 408-456-4496).


 Seagate Technology online services
 Using a modem, you can obtain troubleshooting tips, free utility
 programs, drive specifications and jumper settings for Seagate's
 entire product line. You can also download software for installing
 and analyzing your drive.

 SeaNET
 You can obtain technical information on Seagate drives, Seagate
 software and much more over the Internet from Seagate's World Wide
 Web home page (http://www.seagate.com) or Seagate's ftp server
 (ftp://ftp.seagate.com).

 You may also send E-mail with your questions to DiscSupport@
 Seagate.com or TapeSupport@Seagate.com.


 SeaBOARD
 SeaBOARD is a computer bulletin board system (BBS) that contains
 information about Seagate's disc and tape drive products and is
 available 24 hours daily. Set your communications software to eight
 data bits, no parity and one stop bit (8-N-1). SeaBOARD phone numbers
 are listed in the following table.

 BBS Location           Modem number
 United States      Disc: 408-434-1080; Tape: 408-456-4415
 England            44-1628-478011
 France                         33 1-48 25 35 95
 Germany            49-89-140-9331
 Singapore          65-292-6973
 Thailand           662-531-8111
 Australia          61-2-9756-2359
 Taiwan             886-2-719-6075

 Seagate CompuServe forum
 Online technical support for Seagate products is available on
 CompuServe. To access our technical support forum, type go seagate.
 This forum provides information similar to that found on SeaBOARD.
 In addition, you can type questions or browse through previous
 questions and answers on the forum messages.

 Seagate Technology FAX services
 SeaFAX
 You can use a touch-tone telephone to access Seagate's automated FAX
 system to receive technical support information by return FAX. This
 service is available 24 hours daily.
 Location               Telephone number
 United States          1-800-SEAGATE or 408-456-4496
 England                44-1628-894084
 Australia              61-2-9756-5170

 Seagate technical support FAX
 You can FAX questions or comments to technical support specialists 24
 hours daily. Responses are sent during business hours.
 Location               FAX number
 United States          408-944-9120
 England                        44-1628-890660
 France                 33 1-46 04 42 50
 Germany                        49-89-1430-5100
 Australia              61-2-9725-4052
 Singapore              65-293-4722
 Hong Kong              852-2368 7173
 Taiwan                 886-2-715-2923
 Korea                          82-2-556-7294/4251


 Seagate technical support
 You can talk to a technical support specialist during business hours
 Monday through Friday for one-on-one technical help.  Before calling,
 note your system configuration and drive model number (STxxxx). There
 are several technical support phone numbers available for various
 Seagate products.

 Location          Telephone  number
 United States Please dial 1-800-SEAGATE for the specific product
               telephone number.
               (6:00 A.M. to 11:15 A.M., 12:30 P.M. to 5:00 P.M.,
               Pacific time, M-F)
 England       44-1628-894083 (10:00 A.M. to 1:00 P.M., 2:00 P.M. to
               5:00 P.M., M-F)
 France        33 1-41 86 10 86 (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Germany       Disc: 49-89-140-9332; (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 4:00 P.M., M-F)
               Tape: 49-89-140-9333
 Australia     61-2-9725-3366 (9:00 A.M. to 5:00 P.M., M-F)
 Singapore     65-290-3998 (9:00 A.M. to 12:00 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Hong Kong     852-2368 9918
 Taiwan        886-2-514-2237
 Korea         82-2-556-8241


 SeaTDD 408-944-9121
 Using a telecommunications device for the deaf (TDD), you can send
 questions or comments 24 hours daily and exchange messages with a
 technical support specialist between 6:00 A.M. to 11:15 A.M. and
 12:30 P.M. to 5:00 P.M. (Pacific time) Monday through Friday.


 Customer Service Centers
 Seagate direct OEM, Distribution, System Integrator and Retail
 customers should contact your Seagate Service Representative for
 warranty information.  Other customers contact your place of
 purchase.  Seagate offers comprehensive customer support for all
 Seagate drives.  Seagate customer service centers are the only
 facilities authorized to service Seagate drives. These services are
 available worldwide.

 Location                       Telephone number                FAX number
 United States          1-800-468-3472;                 405-949-6740
 Other Americas
 (Canada & Brazil)      405-949-6706;               405-949-6738
 Mexico                         525-546-6965;                   525-546-4888
 Europe, Middle
 East & Africa          31-2065-43300;              31-2065-34320
 Asia Pacific &
 Australia              65-485-3595;                    65-485-4980
 Japan                          81-3-5462-2904;                 81-3-3462-2979


 Seagate, Seagate Technology and the Seagate logo are registered
 trademarks of Seagate Technology, Inc. SeaFAX, SeaFONE, SeaBOARD,
 SeaTDD, SeaNET, Medalist and DiscWizard are either trademarks or
 registered trademarks of Seagate Technology, Inc. or one of its
 subsidiaries. All other trademarks or registered trademarks are the
 property of their respective owners.


