
P L S - 3 1 2 7 4 A    SAMSUNG
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 2466|     |
Capacity form/unform  1210/      MB        Heads           6|   16|     |
Seek time   / track  11.0/     ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     11.000 MB/S ext PIO3
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SAMSUNG  PLS-31084A/31274A/STG-31271A/WNR-31601/32501A  JUMPER SETTING

 Jumper Setting
 ==============

 Single Drive -C/D CLOSED
               DSP OPEN


 Master Drive -C/D CLOSED
               DSP OPEN


 Slave Drive  -C/D OPEN
               DSP OPEN


