
7 2 9 0 S    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1751|     |     |
Capacity form/unform   290/      MB        Heads           4|     |     |
Seek time   / track  16.0/ 5.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer            64 KB ON-BOARD     Landing Zone
Data transfer rate    2.800 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 71
Power: sleep              W     Humidity     %         5 95    |      5 95
       standby            W     Altitude    km    -0.061  3.048|
       idle               W     Shock        g        10       |     70
       seek           3.8 W     Rotation   RPM      3551
       read/write     4.0 W     Acoustic   dBA
       spin-up       11.8 W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   7290S  JUMPER SETTING

  +---------------------------------------------------------+
  |                                            +--J309      |XX
  |                                   +-+-+-+-+++           |XX
  |                                   +++++++++-+      ++   |XX J1
  |                                 +--+ | | +---+     ||   |XX
  |                              J305 J306 J307 J308   ||   |XX Inter-
  |                                            +-+     ||   |XX face
  |                                       J304/+-+RP301||   |XX
  |                                       J303/+-+     ++   |XX
  |                                       J302/+-+     ++   |XX
  |                                       J301/+-+     ||   |XX
  |                                                    ||   |XX
  |                                               RP302||   |XX
  |                                                    ||   |XX
  |                                                    ++   |X1
  |                                                         |
  |                                                         |XX Power
  |                                                         |XX J2
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   7290S  JUMPER SETTING

 Jumper setting
 ==============

 x = Jumper set at factory


 J301 Terminator Power Selection
 -------------------------------
 Terminator power generation may occur internally from the disk drive
 (when J301 is jumpered), or externally from the SCSI bus. Factory
 default is J301 jumpered.


 J302  Drive Power-Up Option
 ---------------------------
     Pin 1-2  OPEN   Wait for Start Command - The disk drive will not
                     spin-up until the initiator issues a START/STOP
                     UNIT command with the start bit equal to one.
              CLOSED Start When Power Applied - The spin motor starts
                     when power is supplied.


 J303  Parity Disable Option
 ----------------------------
 The parity disable jumper, J303, enables (open, factory default) or
 disables (jumperred) odd parity detection in the disk drive.


 J304  Reserved
 --------------
 RESERVED!


 J305  Reserved
 --------------
 RESERVED!


 J306  Reserved
 --------------
 RESERVED!


 J307/308/309  Addressing
 ------------------------
    +---------------+------------+
    |     Jumper    |  Address   |
    +---------------+------------+
    |     J309      | SEL 0 (LSB)|
    |     J308      | SEL 1      |
    |     J307      | SEL 2 (MSB)|
    +---------------+------------+
 When jumpered, the corresponding bit is a 1.

 The SCSI bus supports connection of up to seven devices, but
 communication can occur only between two SCSI devices at a time. Each
 device has an assigned ID bit that establishes device priority on the
 SCSI bus. When two SCSI devices communicate, one acts as an initiator
 and the other as a target. The initiator orginates an operation and
 the target performs the operation specified by the initiator. An
 initiator can address up to seven other logical units (LUNs) attached
 to one target. The drive has only one logical unit attached. (LUN=0).


 J307/308/309  SCSI ID
 ---------------------
 +--------+----------+-------+-------+-------+
 |SCSI ID | Priority |  J307 |  J308 |  J309 |
 +--------+----------+-------+-------+-------+
 |   0    | Lowest   |OPEN   |OPEN   |OPEN   |
 |   1    |   .      |OPEN   |OPEN   |CLOSED |
 |   2    |   .      |OPEN   |CLOSED |OPEN   |
 |   3    |   .      |OPEN   |CLOSED |CLOSED |
 |   4    |   .      |CLOSED |OPEN   |OPEN   |
 |   5    |   .      |CLOSED |OPEN   |CLOSED |
 |x  6    |   .      |CLOSED |CLOSED |OPEN   |
 |   7    | Highest  |CLOSED |CLOSED |CLOSED |
 +--------+----------+-------+-------+-------+

 Each 7000 Series SCSI drive is shipped from the factory with an
 ID of 6. This ID designation assures sufficient jumpers are available
 for any address except 7 (which is usually reserved for the host
 system).



 J2   DC Power and pin connector assignments
 -------------------------------------------
      +------------+   pin 1    +12 VDC
      | 1  2  3  4 |   pin 2    +12 V Ground Return
      +------------+   pin 3    + 5 V Ground Return
                       pin 4    + 5 VDC



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
MAXTOR    SCSI INSTALLATION

         GENERIC INSTALLATION PROCEDURE FOR A SCSI DRIVE
   -----------------------------------------------------------

 1. Install a 50 pin ribbon connector making sure pin 1, which
    can be identified by the striped edge of the cable, is closest
    to the power connector on the drive.

 2. Install a DC power cable to the back of the drive.

 3. Verify the SCSI ID selection.
    Note: SCSI ID usually needs to be set to 0 to be the boot drive.
    The last physical device on the SCSI bus must be terminated.
    Any other drive or SCSI device connected between the host and
    the device at the end of the bus must not be terminated.

 4. Apply power to the computer.

  4a. When memory test is complete go into your system's Standard
      C-MOS set-up.
      (Note:  There are various ways to get into C-MOS set-up,
      please refer to system's manual for instuctions.)

  4b. Set the drive type to "Not Installed". This intelligent drive
      will identify itself to the SCSI host adapter.

 5. Boot from a DOS diskette that has FDISK.EXE and FORMAT.COM on
    it. At the A> prompt type in FDISK. At the menu options select
    option 1 to create a DOS partition. Another menu will appear and
    from those options choose 1 to create a Primary DOS partition.
    Select yes to make 1 large partition and it will automatically
    become active. Then escape from FDISK.

 6. At the A> prompt type in FORMAT C:/S
    This does a high-level format on the drive and transfers the
    system files in order for the drive to be bootable.
    (Note: Maxtor SCSI drives are low-level formatted at the factory)

 7. The drive is now bootable. As a test remove the DOS diskette
    from A and press reset to re-boot the computer, a C> should be
    displayed, the drive is now ready for operation.


