
D Y K A - 2 2 1 6 0   T R A V E . 3 G N    IBM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        | 4200|     |
Capacity form/unform  2160/      MB        Heads            |   16|     |
Seek time   / track  13.0/ 4.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA3            Precompensation
Cache/Buffer            90 KB              Landing Zone
Data transfer rate    7.000 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext DMA
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 65
Power: sleep          0.1 W     Humidity     %         8 90    |      5 95
       standby        0.3 W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle           1.5 W     Shock        g       125       |
       seek           2.3 W     Rotation   RPM      4200
       read/write     2.0 W     Acoustic   dBA
       spin-up        4.7 W     ECC        Bit   ENHANCED, ON THE FLY,SMART
                                MTBF         h
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
IBM      DYKA-22160/23240  TRAVELSTAR  JUMPER SETTING


              +--------------------------------------+
              |                                      |
              |                                      |
              |                                      |
              +--------Interface-------------49------+
              |       **********************1 **47 Jumper
              |       *************x********* **48   |
              +------44----------------------50------+
              +                                      +

 Pin position 20 is left blank for secure connector insertion.

 Pin position 49: When grounded, no spin-up at POR when open/pull up,
                  normal spin-up at POR.






**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
IBM      DYKA-22160/23240  TRAVELSTAR 3GN  JUMPER SETTING

 Jumper Setting
 ==============

 Drive Address Setting
 ---------------------
 A jumper is available at the interface connector to determine the
 drive address. Using Cable Selection, the drive address depends on
 the condition of pin 28 of the AT interface cable. In the case when
 pin 28 is ground or low, the drive is a Master. If pin 28 is open or
 high level, the drive is a Slave.


   ---49--47+
    *   * * | Master
    *   * * | (Default setting)
   ---50--48+


   ---49--47+
    *   * X | Slave
    *   * X |
   ---50--48+


   ---49--47+
    *   * * | Cable Selection
    *   xxx |
   ---50--48+


   ---49--47+
    *   xxx | RESERVED       (MASTER)
    *   * * |
   ---50--48+


   ---49--47+
    *   X * | NEVER ATTACH A JUMPER HERE!
    *   X * |
   ---50--48+


 49-PIN: When grounded, no spin-up at POR
         When open/pull-up, normal spin-up at POR


