
S D - 3 8 0 - 2 0    TEAC
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1050|     |     |
Capacity form/unform    86/      MB        Heads           4|     |     |
Seek time   / track  19.0/     ms          Sector/track   40|     |     |
Controller           IDE / AT              Precompensation 65535
Cache/Buffer            64 KB              Landing Zone     1049
Data transfer rate    1.000 MB/S int       Bytes/Sector      512
                      4.000 MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g         5       |     60
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TEAC     SD-380  JUMPER SETTING

 Jumper Setting
 ==============

 Indicator LED
 -------------
 The indicator on the front bezel shall be kept lit after the HDD
 responds to a selection from an initiator, and before it completes
 the execution of the command.


 Parity Strap
 ------------
 The S3 on the PCBA is used as a parity strap. When the S3 is shorted
 with a plug, the input data (DB0 to DB7, DBP) shall be parity checked
 (odd) by the HDD. When the S3 is open, no parity check shall be
 executed.


 The SCSI ID shall be set with the individual straps of SP, S0, S1,
 and S2 on the PCBA.
 The SP strap is to reserve the setting logic for S0, S1 and S2.

   +----------+---------------+----------------+
   |          |     SP=ON     |     SP=OFF     |
   +----------+---------------+----------------+
   |SCSI ID   | S2   S1   S0  |  S2   S1   S0  |
   +----------+---------------+----------------+
   |   0      | ON   ON   ON  |  OFF  OFF  OFF |
   +----------+---------------+----------------+
   |   1      | ON   ON   OFF |  OFF  OFF  ON  |
   +----------+---------------+----------------+
   |   2      | ON   OFF  ON  |  OFF  ON   OFF |
   +----------+---------------+----------------+
   |   3      | ON   OFF  OFF |  OFF  ON   ON  |
   +----------+---------------+----------------+
   |   4      | OFF  ON   ON  |  ON   OFF  OFF |
   +----------+---------------+----------------+
   |   5      | OFF  ON   OFF |  ON   OFF  ON  |
   +----------+---------------+----------------+
   |   6      | OFF  OFF  ON  |  ON   ON   OFF |
   +----------+---------------+----------------+
   |   7      | OFF  OFF  OFF |  ON   ON   ON  |
   +----------+---------------+----------------+

 Note: The strap states are as follows:

       1: Strap open
       2: Strap short


