
9 0 7 5 0 D 6     D I A M O N D M A X P    MAXTOR
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |14542|     |
Capacity form/unform  7500/      MB        Heads           6|   16|     |
Seek time   / track   9.0/ 1.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA4 ULTRA      Precompensation
Cache/Buffer           512 KB SDRAM        Landing Zone
Data transfer rate   21.000 MB/S int       Bytes/Sector      512
                     33.000 MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 71
Power: sleep          0.8 W     Humidity     %         5 95    |      5 95
       standby        1.3 W     Altitude    km    -0.061  3.048| -0.061 12.192
       idle           5.8 W     Shock        g        20       |    200
       seek          10.2 W     Rotation   RPM      7200
       read/write     5.9 W     Acoustic   dBA        37
       spin-up            W     ECC        Bit   SMART
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   DIAMOND MAX PLUS 2500




                     Pin 1
     J1 IDE Connector  |                J2 Power
  +----------- --------+-++-----------++---------+
  | .................... || @ * *   * || X X X X |
  | .......... ......... || @ * * * * || X X X X |
  +----------------------++-+-+-+-+-+-++-+-+-+-+-+
                            | | | | |    | | | |
                            | | | | |    | | | |
      J50 Master/Slave -----+ | | | |    | | | +-+12V
      J48 Cable Select -------+ | | |    | | +---+12V Return
      J46 4092 Cyl Limitation---+ | |    | +----- +5V Return
      J44 Factory Reserved -------+ |    +------- +5V
      J42 Factory Reserved ---------+





**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   DIAMOND MAX  INSTALLATION SHEET

 Jumper Setting
 ==============

                                        +---+---+---+---+---+
                                        |J50|J48|J46|J44|J42|
  +-------------------------------------+---+---+---+---+---+
  | Master/Slave                        |   |   |   |   |   |
  |  Only Drive in single drive system* | J |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  |  Master in a dual drive system*     | J |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  |  Slave in a dual drive system       | O |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  | Cable Select                        |   |   |   |   |   |
  |  Disabled*                          |   | O |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  |  Enabled                            |   | J |   |   |   |
  +-------------------------------------+---+---+---+---+---+
    J=Jumpered O=Open *=Default



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
MAXTOR   91000D8/90910D8/90875D7/90840D7/90750D6/90625D5/90500D4

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).



 Idle
 The drive is spinning., the actuator is parked and powered
 off, and all other circuitry is powered on. The drive is
 capable of responding to read commands within 40 ms.

 Read/Write
 Data is being read from or written to the drive.

 Spin-up
 The drive is spinning up following initial application
 of power and has yet not reached full speed. Maximum
 current draw lasts one second.


 Standby
 The spin motor is not spinning. The drive will leave this
 mode upon receipt of a command that requires disk access.
 The time-out value for this mode is programmable. The
 buffer is active to accept write data.

 Sleep
 This is the lowest power state - with the interface set to
 inactive. A software or hardware reset is required to return
 the drive to the standby state.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
MAXTOR   DIAMOND MAX PLUS 2500

            INSTALLATION PROCEDURE FOR AN IDE DRIVE
            ---------------------------------------
 1. Install a 40 pin Data Cable ensuring that pin 1, which can be
    identified by the striped edge of the cable, is closest to the
    power connector on the drive.

 2. Install a DC power cable to the back of the drive.

 3. Verify the jumper configurations for Master/Slave operation
    (Note:  Master will be the bootable drive. The slave will not
    be bootable.) Also make sure the existing C: drive is jumped
    to be the Master in a two drive system, not the only drive in
    the system.

 4. Apply power to the computer.

 4a. When memory test is complete go into your system's Standard
     CMOS set-up.
     (Note: There are various ways to get into CMOS set-up, please
     refer to system's manual for instructions.)

 4b. If your system's BIOS supports a user programmable drive
     type, program the BIOS with the default parameters of your
     drive. If your system does not support a user programmable
     drive type choose parameters that closely match but do not
     exceed the drives MegaByte capacity. Escape from set-up
     then choose write to CMOS and exit.

 5. Boot from a DOS diskette that has FDISK.EXE and FORMAT.COM on
    it. At the A> prompt type in FDISK. At the menu options select
    option 1 to create a DOS partition. Another menu will appear
    and from those options choose 1 to create a Primary DOS
    partition. Select yes to make 1 large partition and it will
    automatically become active. Then escape from FDISK.

 6. At the A> prompt type in FORMAT C:/S This does a high-level
    format on the drive and transfers the system files in order for
    the drive to be bootable. (Note: IDE drives are low-level
    formatted from the manufacturer and only need a high-level
    format).

    To configure the drive as a slave drive repeat steps 1-4 and
    proceed with steps 5a. and 6a. as follows:

  5a. At the C> prompt type in FDISK. When the menu options appear
      select option 5 to switch to the second drive. Enter fixed
      disk drive number 2. Then choose option 1 to create a DOS
      partition, then select option 1 again to create a Primary DOS
      partition or option 2 to create an Extended DOS partition.
      (Note: C and D drives will always be the Primary partitions
      but only the Primary partition on C: will have a status of
      active).

  6a. Proceed with a high-level format on the drive by typing FORMAT
      D: (Note: Make sure the correct drive letter has been selected
      for format).

 7. The drive is now bootable. As a test remove the DOS diskette
    from A and press reset to reboot the computer,  a  C> should be
    displayed, the drive is now ready for operation.


