
A - 9 0 A T    AREAL
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders    1430|  715|     |
Capacity form/unform    90/      MB        Heads           2|   10|     |
Seek time   / track  15.0/     ms          Sector/track   62|   25|     |
Controller           IDE / AT              Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate    1.000 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     100000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
AREAL    A-90/130  DRIVE OPTIONS AND BIOS INFORMATION

  +---------------------------------------------------------+
  |                                       Not jumpers+++    |
  |                                                  +++    |XX44
  |                                                         |XX
  |                                                         |XX I
  |                                                         |XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                    +-+-+-+-+-+-+        |.X R
  |                                    +-1-2-3-4-5-6        |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |                                                         |XX
  | (4 Layer FAB only)                                      |XX
  |                                                         |  2
  +---------------------------------------------------------+




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
AREAL    A-90/130  DRIVE OPTIONS AND BIOS INFORMATION

 Jumper Setting
 ==============

 x = Factory default configuration


   Jumper 1
   --------
   x CLOSED  Master
     OPEN    Slave


   Jumper 2
   --------
     CLOSED  PDIAG disabled
   x OPEN    PDIAG enabled


   Jumper 3
   --------
     CLOSED  SPARE
   x OPEN    SPARE


   Jumper 4
   --------
   x CLOSED  IOCHRDY
     OPEN    N/A


   Jumper 5
   --------
     CLOSED  DACK
   x OPEN    N/A


   Jumper 6
   --------
     CLOSED  DREQ
     OPEN    N/A (default for the A-85 hard disk)


