
D H A S - 2 4 0 5   T R A V E L S T A R    IBM
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform   405/      MB        Heads           3|     |     |
Seek time   / track  14.0/     ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer            64 KB LOOK-AHEAD   Landing Zone
Data transfer rate    3.000 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 65
Power: sleep              W     Humidity     %         8 90    |      5 95
       standby            W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle           1.2 W     Shock        g        20       |    120
       seek               W     Rotation   RPM      3800
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   ON THE FLY
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates     EEC,FCC,VDE                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
IBM      DHAS-2270/2405/2540  JUMPER SETTING


                 +---------------------------+
                 |                           |
                 |     J1                J2  |
                 +---------------------------+
                 |ooooooooooooooooooo1  ooo1 |
                 40ooooooooooooooooooo  8ooo |
                 +---------------------------+

 J2
 Pin 1 UNUSED          Note
     2 -NO SPIN UP     If Pin 2 is grounded the drive will not spin up
     3 -INDEX          at power up - drive must be started with a
     4 UNUSED          start stop unit command.
     5 -ID1
     6 -ID2
     7 -ID4
     8 -LED



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
IBM      DHAS-2270/2405/2540  JUMPER SETTING

 Jumper Setting
 ==============


 J2  SCSI ID
 -----------
   +----------+-----------------------+
   | SCSI ID  | Pin 7   Pin 6   Pin 5 |
   |          | ID4   | ID2   | ID1   |
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | GND   |
   +----------+-------+-------+-------+
   |    2     | OPEN  | GND   | OPEN  |
   +----------+-------+-------+-------+
   |    3     | OPEN  | GND   | GND   |
   +----------+-------+-------+-------+
   |    4     | GND   | OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    5     | GND   | OPEN  | GND   |
   +----------+-------+-------+-------+
   |    6     | GND   | GND   | OPEN  |
   +----------+-------+-------+-------+
   |    7     | GND   | GND   | GND   |
   +----------+-------+-------+-------+


 Cabling
 -------
 The maximum cable length from the host system to the drive is
 limited to 6 inches with external 1 K-ohm pull up resistors.

 In case that appropriate termination resistors are externally
 equipped to the interface lines, the cable length can be extended.
 The maximum cable length depends on the condition of various
 electrical parameters of the interface. IBM will offer technical
 guidance on request.


 Device Address
 --------------
 The drive recognizes its device address, namely SCSI ID, with the
 condition of -ID1, -ID2 and -ID4. The signal condition and the device
 address are shown above.


 Signal termination
 ------------------
 The drive does not have termination nor pull up resistors for SCSI
 interface.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
IBM      DHAS-2270/2405/2540  JUMPER SETTING

 Notes On Installation
 =====================


 Mounting Orientation
 --------------------

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+


 The drive will operate in all axes (6 directions). The drive will
 operate within the specified error rates when tilted + or - degrees
 from these positions.

 Performance and error rate will stay within specification limits if
 the drive is operated in the other permissible orientations from
 which it was formatted. Thus a drive formatted in a horizontal
 orientation will be able to run vertically and vice versa.

 The recommended mounting screw torque is 3 + or - 0.5 kgf. cm. The
 recommended mounting screw depth is 3.5 + or - 0.5 mm for bottom and
 5.0 + or - mm for horizontal mounting.

 The system is responsible for mounting the drive securely enough to
 prevent excessive motion or vibration of the drive at seek operation
 or spindle rotation, using appropriate screws or equivalent mounting
 hardware. Consult the issuer of this specification for actual
 application.

 Vibration test and shock test are to be conducted with mounting the
 drive to the table using bottom four screws.


 ELECTRICAL CONNECTOR LOCATIONS Driver/Receiver
 ----------------------------------------------
 The drives support single ended drivers and receivers


 Connector
 ---------
 The SCSI signal connectors is designed to mate with AMP part number
 6-176135 or equivalent. Size and location of the mounting holes
 comply with MCC.


 Mechanical Data
 ---------------
 Dimensions     All models
 Height (mm)    17.0 + 0.35/-0.3
 Width (mm)     70.0 + or - 0.25
 Length (mm)   100.0 + or - 0.25
 Weight (gram) 180 Max



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
IBM      DHAS-2270/2405/2540  JUMPER SETTING

 General
 -------
 The latest 2.5" disk drives from IBM provide up to 540 MB in a slim
 17 mm high package. Using the latest MR head technology IBM provides
 high performance drives particularly suited to the mobile computing
 market.


 Applications
 ------------
 - High performance portable computers

 - Non-IT - process control/fax

 - Removable/secure storage units


 Features
 --------
 270/405/540 MB at (512 bytes/sector)

 SCSI2 interface

 Media data rate 24.9/36.0 Mbits/s (8 zones)

 Rotational speed 3800 rpm

 Average seek time 14 ms (Read)

 Magneto resistive heads

 64K Look Ahead Buffer

 ECC on the fly

 1.2 watt idle

 Shock 250G (2ms) non operating

 All 6 axis mounting

 Spin up 2.2 sec (typical)

 Power saving modes


 Benefits
 --------
 High capacity 2.5" drives

 Popular interface with excellent performance

 Excellent data rate across disk surface

 Fast access to data

 High areal density, low component count

 Fast access to data and improved throughput

 Low power for battery powered applications

 Robust design for portable computing applications

 Fast recovery from standby

 Features for Green PC and battery systems

 Assured reliability


 Electormagnetic Compatibility
 -----------------------------
 The Drive meets the following EMC requirements when installed in the
 user system and exercised with a random accessing routine at maximum
 data rate:

 United States Federal Communication Commission (FCC) Rules and
 Regulations Part 15, Subject J -Computer Devices "Class B Limits".

 European Economic Community (EEC) directive #76/889 related to the
 control of radio frequency interference and the Verband Deutscher
 Elektrotechniker (VDE) requirements of Germany (GOP).


 Operating Modes
 ---------------
 Spin-Up
 -------
 This power on mode is defined as the period of time from receipt of
 power at the drive assembly or receipt of Start SCSI command, to Idle
 mode (or 'Ready' state).

 Idle
 ----
 In this mode the disks are spinning at rated speed, the drive is
 able to accept and immediately execute commands requiring disk
 access. Actuator assembly is located on track in the 'Ready' state.

 Standby
 -------
 Spindle motor is stopped. All modules except the host interface are
 sleeping. Commands can be received immediately. Drive is in an
 interrupt waiting mode with the lowest power dissipation.

 Seek/Read/Write
 ---------------
 This is a command execution mode where the driver actuator is moving
 or data is being written to or read from the media.

 Note 1:
 After power down or spindle stopped, a head locking mechanism
 secures the heads in the ID parking position.


 Air Cooling Requirement
 -----------------------
 The host system must provide sufficient air flow across the drive to
 maintain the temperature at less than 60 C (measured at the center of
 the drives' top cover).


 Operating Shock
 ---------------
 The Drive will withstand (with no hard error) a 20G half-sine wave
 shock pulse of 12ms duration and no data loss or permanent damage at
 idle, seek and read modes within shock pulses of 60 G3.5 ms half-sine
 wave.


 Non-Operating Shock
 -------------------
 The Drive will withstand (with no permanent damage or degradation in
 performance) a 120G half-sine wave shock pulse of 11 ms duration or
 250G for 2 ms.


 Operating and Non-Operating Vibration
 -------------------------------------
 Due to the complexity of this subject we recommend that users contact
 the Distributor to discuss how to perform the necessary measurements
 if they believe this to be an area which requires evaluation.


 PACKAGING:
 The drive must be protected against Electro-Static Discharge
 especially when being handled. The safest way to avoid damage is to
 put the drive in an antistatic bag before ESD wrist straps etc are
 removed. Drives should only be shipped in approved containers, severe
 damage can be caused to the drive if the packaging does not
 adequately protect against the shock levels induced when a box is
 dropped. Consult your IBM marketing representative if you do not have
 an approved shipping container.



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
IBM       SCSI INSTALLATION

 SCSI Installation Guide Generic

 Installation requirements
 -------------------------
 To install a drive inside your computer or in an external storage
 enclosure for SCSI devices, you must have:

 1 The documentation that came with your computer or storage
   enclosure.

 2 The documentation that came with your hard drive.

 3 A small, flat blade screwdriver.

 4 A SCSI controller, which is either built into the system board or
   on an adapter inside your computer.

 5 An installation kit, if it is required for your computer. Contact
   your place of purchase if you are not sure.

 6 If you are installing this into a PS/2 computer, you will also need
   the up-to-date backup copy of your reference diskette and
   diagnostic diskette.

 WARNING: Do not open the static-protective bag containing the drive
 until instructed to do so. Static electricity can damage the drive.


 Hardware and software considerations
 Operating system
 ----------------
 The operating system and hardware are two of the factors that
 determine the number of drives a computer can support. The manuals
 for your computer and operating system can help you to determine the
 number and type of hard disk drives you can use.


 Power supply
 ------------
 Two factors that determine the number of internal drives that a
 computer or SCSI storage enclosure can support are:

 1 The available current of the power supply

 2 The nominal operating current of each drive installed

 Most computer power supplies have output over-current protection. If
 the total allowed current is exceeded, the power supply shuts down.
 The computer must be turned off and turned on again.

 SCSI ID Each SCSI device connected to a SCSI adapter must be assigned
 a unique SCSI identification number (ID). The ID you assign to this
 device depends on the number of SCSI devices connected to the SCSI
 adapter and the SCSI IDs already assigned to those devices.

 Note: All IBM SCSI controllers support SCSI IDs 6 through 0. (ID 7 is
 used for the SCSI controller.) Some SCSI controllers support SCSI IDs
 15 through 8. If your SCSI controller supports more than seven
 devices, then you can use SCSI IDs 15 through 8. If you are not sure
 if your SCSI controller supports more than seven devices, refer to
 the documentation that came with your SCSI controller for
 information.

 If you have an IBM PS/2 computer, you can view your SCSI ID settings
 by accessing the system programs. From the main menu, select Set
 configuration. The select Set and view SCSI configuration.
 Other computers might have utility programs that enable you to view
 the SCSI configuration, or you might have to physically inspect the
 installed SCSI devices to see how the IDs are set. For more
 information, refer to the documentation that came with your computer
 or SCSI controller.


 Handling precautions
 --------------------
 1 Turn off all attached devices first; then turn off the computer.

 2 Unplug all the power cords from electrical outlets before starting
   installation.

 3 Disconnect all power cables from your computer and attached devices
   before starting installation.

 4 Limit your movement. Movement can cause static electricity to build
   up around you.

 5 Handle the drive carefully and by the edges.

 6 Do not touch any exposed printed circuitry.

 7 Prevent other people from touching the components or the drive.

 8 When you are installing the drive, touch the static-protective
   package containing the drive to a metal expansion-slot screw or
   other unpainted metal surface on the computer, for at least 2
   seconds. (This drains static electricity from the package and your
   body.)

 9 When possible, remove the drive and install it directly into the
   computer without setting it down. If this is not possible, place
   the drive, component side up, on the static-protective bag on a
   flat surface until the drive is installed.

 10 Do not place the drive on the computer cover or on a metal table.


 Installing the drive
 --------------------
 These instructions guide you as you install the drive inside your
 computer or storage enclosure.

 Step 1. Setting the jumpers and terminators

 Note: Be sure you have chosen the SCSI ID before continuing. If you
       did not yet choose the SCSI ID, go to "SCSI IDs" above, then
       return here. Follow these steps to set the SCSI ID to match
       your chosen SCSI ID.

 1 Touch the static-protective bag containing the drive to a metal
   expansionslot cover on the computer. This drains any static
   electricity from the package and your body.

 2 Remove the drive from the static-protective bag, holding the drive
   by the edges. Do not touch any exposed components on the drive.

 3 Place the drive on the bag, on a flat surface.

 4 When the Auto Start feature is enabled, the hard disk drive motor
   starts as soon as the computer is turned on. Locate the Auto Start
   jumper by referring to the documentation that came with your drive.
   If the Auto Start jumper is not in place, the hard disk is started
   by a command from the SCSI controller. For drives installed in
   IBM computers or storage enclosures ensure that this jumper is off.
   The hard disk drive is started in a staggered sequence. This
   reduces the start-up load on the power supply. For non-IBM
   computer, refer to the documentation that came with your
   computer for further information.

 5 Set the SCSI ID that you selected. To remove a jumper, pull it
   straight off. To install a jumper, line up the two holes in the
   jumper with the appropriate two pins on the drive. Then push the
   jumper onto the pins until it is completely seated and covers
   both pins.

 6 Store any jumpers you do not use in a safe place, in case you need
   to change the SCSI ID for this drive later. WARNING: If you have
   extra jumpers, do not store them on any of the extra pins on the
   connector. Storing them on a set of pins could damage the drive.

 Step 2. Connecting the terminator
 The location of the drive you are installing inside the computer or
 storage enclosure determines whether you need to connect a terminator
 or put a jumper on the Enable Active Termination pins. Read the
 information in the following table to determine if you must install
 the terminator. For more information about termination, refer to the
 documentation that came with your computer.

 Note: A SCSI chain of devices consists of multiple SCSI devices
 connected by a SCSI cable to a SCSI controller.

 If the hard disk drive is:                   Then:
 The last physical device on a SCSI chain of  Install the terminator
 devices inside the computer.

 The last physical device on a SCSI chain of  Install the terminator
 devices inside an external storage enclosure.

 Step 3. Enabling term power
 If your drive has a jumper for term power and your SCSI controller is
 suppling term power, (check with the manufacturer of your controller)
 then you do not need to enable the term power. The jumper should be
 off. For help in locating the term power jumper, refer to the
 documentation that came with your drive.

 Step 4. Installing the drive
 For the specific information on installing a hard disk drive, refer
 to the documentation that came with your computer. You will be
 required to mount the drive inside your computer, and connect signal
 and power cables to the hard drive. When installed in an enclosure,
 the drive is attached by cable to the external connector of a SCSI
 controller. The controller can be either on a SCSI adapter or built
 into the system board inside of your computer.

 Note: Be sure to use the correct screws provided with your drive.
 Using the wrong ones might cause damage to the drive.

 Step 5. Completing the installation procedure
 The installation of the drive is complete. Reinstall the cover on the
 computer or storage enclosure. Store these instructions and any extra
 parts in a safe place in case you change your configuration.

 After installing your hard disk drive, use the information that came
 with your computer to reconfigure your system. When you power on your
 system, turn on all attached devices first; then turn on the
 computer.

 If you have any problems at this point, turn off all attached
 devices; then, turn off the computer and check that:

 1 The cables are installed correctly

 2 No options or cables are loose

 3 The SCSI ID is properly set

 4 No two SCSI drives have the same SCSI ID

 5 The terminators are properly installed

 Turn on all attached devices; then, turn on the computer. If you
 still have a problem, refer to the troubleshooting information in the
 documentation that came with your computer.

 Step 6. Update configuration
 Whenever you add or remove an option from your computer, you must
 update the configuration information. Your computer might have an
 automatic configuration program, or you might have to follow a
 specific procedure. For more information, refer to the documentation
 that came with your computer.

 Step 7. Preparing the drive for use
 Having successfully installed the hard disk drive, you need to
 prepare it for use. Depending on the operating system you are using,
 you might need to partition then format the hard disk. Refer to the
 documentation that came with your operating system for information on
 how to format your new drive. To make the drive just installed your
 primary drive, you might need to create a new system partition on the
 drive. For information on creating a new system partition, refer to
 the documentation that came with your operating system.


 Troubleshooting
 ---------------
 You might be able to solve a problem yourself. Before calling IBM,
 you might want to try some or all of the following troubleshooting
 procedures.

 1 Remove and reattach all drive cables

 2 Remove and reseat the drive

 3 Place the drive in a different slot, if one is available


 4 If your drive contains jumpers or switches, check that they are set
   as specified

 5 Reread any software instructions; be sure software settings are
   correct

 6 Inspect the drive for damage, such as bent pins

 7 Check the computer manual for instructions about the installation
   of upgrades. Look for a section about system setup or system
   configuration. Follow all procedures.

 8 After completing these steps, reassemble the computer and connect
   the power cord.

 If you are still having problems and want to call IBM technical
 support, have available as much of the following information as
 possible:

 1 Drive model or P/N and description

 2 Computer manufacturer and model

 3 Exact wording of error message (if any)

 4 Description of the problem

 5 Hardware and software configuration information for your system
   If possible, be at your computer. Your technical support rep might
   want to walk you through the problem during the call.


