
Q M   3 1 0 8 0 S G A     P I O N E E R    QUANTUM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 2097|     |
Capacity form/unform  1082/      MB        Heads            |   16|     |
Seek time   / track  12.0/ 4.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate   12.625 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C           55    |    -40 65
Power: sleep              W     Humidity     %         5 85    |      5 95
       standby            W     Altitude    km            3.048|        12.192
       idle               W     Shock        g        10       |     70
       seek               W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA        30
       spin-up            W     ECC        Bit   48BIT ON THE FLY,SMART
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
QUANTUM  PIONEER SG  JUMPER SETTING

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX1
  |                                                         |xx
  |                                                         |xx
  |                                                         |
  |                                                         |XX Power
  |                                                         |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
QUANTUM  PIONEER SG  JUMPER SETTING

 Jumper Setting
 ==============


                              ATA CABLE PIN+        Not Used
    +--------------------------------------1----------++--------+
    |* * * * * * * * * * * * * * * * * * * *  * * * * *| XXXXXX |
    |* * * * * * * * * *   * * * * * * * * *    * * * *| xxxxxx |
    +--------------------+----------------------+-+-+--+-Power--+
                      Blank key               DS+ | PK
                                                  CS
 Single Drive = DS only
 Master Drive = DS only
 Slave Drive = No Jumpers

 Quantum IDE disk drives have multiple jumper setting options and are
 used to set specific drive features. The most common settings are
 used to define the drive as the primary or secondary drive on the
 IDE cable.

 Master / Slave
 --------------
 Quantum IDE drives have additional jumper settings used for optional
 features found on the drive. Listed below are the various jumper
 options that may be found on Quantum IDE drives and the corresponding
 feature that they enable.


 DS Jumper - Drive Select
 ------------------------
 Used to identify the drive as the primary (MASTER) drive in a single
 or dual drive configuration. This is the factory default setting.


 SP Jumper - Slave Present
 -------------------------
 Used only when the second (SLAVE) drive in a two drive configuration
 does not support DASP.


 DASP
 ----
 (Drive active / drive 1 present) is a CAM (Common Access Method)
 defined signal that indicates the presence of a second drive, DASP is
 used during power on initialization and after a reset. Prior to this
 definition, products were introduced which did not utilize this
 method to detect the presence of a second drive. The SP jumper is
 used on the MASTER drive, with the DS jumper, when the second drive
 does not support DASP.


 CS Jumper - Cable Select
 ------------------------
 Only used in systems that support the cable select feature. Cable
 Select allows for each IDE disk drive to be jumped the same and the
 position on the cable determines the ID. This requires a special
 cable and both drives on the interface would have to support this
 feature.


 PK Jumper - Park (Spare)
 ------------------------
 This jumper does not enable any feature. It is used, instead, to
 provide a spare location to any jumper removed from the drive
 during a configuration change.


