
S T 3 2 1 0 9 N             C A Y M A N    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform  2147/      MB        Heads            |     |     |
Seek time   / track   9.0/ 2.0 ms          Sector/track     |     |     |
Controller           -                     Precompensation
Cache/Buffer           512 KB READ-AHEAD   Landing Zone
Data transfer rate    6.700 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


