
M 1 6 0 6 S A U   <   1 1 / 1 9 9 5    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    3456|     |     |
Capacity form/unform  1091/      MB        Heads           6|     |     |
Seek time   / track  10.0/ 3.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer           512 KB SEGMENTED    Landing Zone
Data transfer rate    5.500 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %         8 80    |      5 95
       standby            W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle               W     Shock        g         5       |     50
       seek               W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA        38
       spin-up            W     ECC        Bit
                                MTBF         h     800000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M1603S/M1606S  JUMPER SETTING A1CA 01310-0011

  +---------------------------------------------------------+
  |                                            CNH1 +----+  |XX
  |                                            1+-+ |    |  |XXI
  |                                      CN6    | | |    |  |XXN
  |                                     ++++++  +-+8|RP1 |  |XXT
  |                                     +----+      |TERM|  |XXE
  |                                     10   2      |    |  |XXR
  |                                      9   1      +----+  |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  | 2 1                                                     |XX
  | +-+ CN5                                                 |XX
  | +-+                                                     |   +5V
  |                                                         |XX
  |                                                         |XX
  +---------------------------------------------------------+   +12V
          Drives manufactured before November 1995!



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M1603S/M1606S  JUMPER SETTING C1CA 01310-0011


 Jumper Setting
 ==============

 x = Factory default setting


 CNH1  SCSI ID
 -------------
   +----------+-----------------------+
   | SCSI ID  |        Jumpers        |
   |          | 5-6   | 3-4   | 1-2   |
   +----------+-------+-------+-------+
   |x   0     | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    2     | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    3     | OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+
   |    4     | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    5     | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    6     | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+

 NOTE
 Always ensure that the device ID selected is unique to the SCSI bus.
 The controller is often configured at ID 7 so it is the best to
 avoid this ID number for the drive.


 CNH1 Spindle Motor Control
 --------------------------
 Pins 7-8  OPEN   By Command
          xCLOSED Auto


 CN6 Remote SCSI ID Connector
 ----------------------------
    +1-3-5-7-9+
    |o o o o o|  Side View
    |o o o o o|
    +2-4-6-8-10

       +------------+--------+
       |  PINS      | SIGNAL |
       +------------+--------+
       |Pin 2       |-ID0    |
       +------------+--------+
       |Pin 4       |-ID1    |
       +------------+--------+
       |Pin 6       |-ID2    |
       +------------+--------+
       |Pins 1, 3, 5|GND     |
       +------------+--------+
       |Pins 7   10 |RESERVED|
       +------------+--------+


 CN5 External operator panel connector
 -------------------------------------
 Pin 01    LED(V)
 Pin 02    -LED



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
FUJITSU  M1603S/M1606S  JUMPER SETTING A1CA 01310-0011

 Notes On Installation
 =====================

 Drive mounting
 --------------

     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  | x
   |                 |   |  |     | |     |  | x+----------------+x
 +-+-----------------+-+ |  |     | |     |  | ||x              x||
 +---------------------+ |  |     | |     |  | ||  x          x  ||
                         |  |     | |     |  | ||    x      x    ||
      x           x      |  |     | |     |  | ||      x  x      ||
 +------x------x-------+ |  +-----+ +-----+  | ||       xx       ||
 +-+------x--x-------+-+ +--+             +--+ ||     x    x     ||
   |       xx        |                         ||   x        x   ||
   |     x    x      |                         || x            x ||
   +---x--------x----+                         |x                x|
     x            x                           x++----------------++x
      UNACCEPTABLE!                                UNACCEPTABLE!


 Orientation
 -----------
 The drive may be installed in one of three orientations; PCA down
 or on either edge. Inclination from vertical or horizontal should
 not exceed 5*.


 Mounting screw fixing
 ---------------------
 When the mounting screw holes on the side of the drive are used, then
 use only the two pairs of outer holes. Do not use the centre hole
 in conjunction with only one of the outer holes. The screw must not
 penetrate the drive by more than 4.5 millimetres.


 Grounding
 ---------
 Sufficient grounding will be provided for correct operation when
 the drive is screwed into an electrically grounded frame.


 Cooling
 -------
 Allow space above and below the drive to provide for adequate air
 flow. Fan cooling is recommended. The disk enclosure temperature,
 measured at top centre, should never exceed 60*C.



 Termination
 -----------
 A terminating resistor should be installed at both ends of the
 SCSI bus. When shipped from the factory, this drive is terminated.
 If the drive is to be used in the middle of the SCSI cable with
 other terminated devices at the ends, or if external termination
 is to be used, then the terminating resistor pack on the drive MUST
 be removed.


 Termination Power
 -----------------
 Terminator power is supplied internally and to the SCSI BUS via a
 fuse.


