
S T 3 6 3 6 A           M E D A L I S T    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    4893| 1241|  620| 1024
Capacity form/unform   640/      MB        Heads           2|   16|   32|   16
Seek time   / track  12.5/ 3.0 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB READ/WRITE   Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     RLL1/7 ZBR                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby        1.0 W     Altitude    km                 |
       idle           3.5 W     Shock        g         5       |     75
       seek           4.6 W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST3636A/ST34340A  JUMPER SETTING

 Jumper Setting
 ==============

               J2                   +------ 5 Volt
  +----------------------------+---+----+
  |XXXXXXXXXXXXXXXXXXXXXXXXXXXX|:::|OOOO|Power
  +----------------------------+++++----+
   Pin 20 removed               ||+--- RESERVED
                                |+-+-- Slave Present (when Master ON)
                                |  +-- Cable Select (when Slave OFF)
                                +----- Master ON, Slave OFF


