
M A F - 3 3 6 4 L P     A L 5 E / 5 L E    FUJITSU
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3"/SUPERSLIMLINE      Cylinders        |     |     |
Capacity form/unform 36400/      MB        Heads            |     |     |
Seek time   / track   5.5/     ms          Sector/track     |     |     |
Controller           ULTRA2 SCSI LVD       Precompensation
Cache/Buffer          2048 KB MULTI-SEGMEN Landing Zone
Data transfer rate   45.000 MB/S int       Bytes/Sector      512
                     80.000 MB/S ext
Recording method     EPRML                          operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM     10025
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h    1000000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
FUJITSU  MAF-3364LP

 AL5E/5LE 10K RPM Ultra2 Wide LVD SCSI Enterprise Drive.
 -------------------------------------------------------
 The latest in high performance enterprise storage, providing an
 incredible 36.4GB capacity in a 1.6" high device.


 Technology Features
 -------------------
 - GMR(Giant Magnetoresistive) Heads combined with the latest
   EPRML(Enhanced Partial Response

 - Maximum Likelihood) digital read channel enable an industry leading
   36.4GB on 3-inch media with the same number of platters as
   previous generation 18.2GB product

 - Ultra2 Wide LVD SCSI delivers an astounding 80MB/Sec interface
   data transfer rate to the host, with a maximum cable length of
   12.5m


 Performance Features
 --------------------
 With Internal Data Transfer Rates up to a blistering 45.0MB/Sec,
 Average Seek Times of 5.5ms & a 2048KB Multi-Segmented Buffer,
 these drives are performance enhanced for todays mission critical
 server applications.


 A/V (Audio/Visual) Compatibility
 --------------------------------
 The AL5E/5LE family employs an Embedded Servo System eliminating the
 need for Thermal Recalibration which were the cause of interrupted
 data transfers resulting in lost musical notes or jerky video frames.


 Quality Features
 ----------------
 Capitalising on Fujitsu's global reputation for 'Quality &
 Reliability' these drives offer an exceptional MTBF (Mean Time
 Between Failure) specification in excess of 1,000,000POH (Power On
 Hours).


