
W N R - 3 2 5 0 1 A   W I N N E R   P R    SAMSUNG
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 4681|     |
Capacity form/unform  2416/      MB        Heads           6|   16|     |
Seek time   / track  11.0/     ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           128 KB READ-AHEAD   Landing Zone
Data transfer rate    5.200 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     PRML 8/9                       operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 70
Power: sleep          1.2 W     Humidity     %         5 80    |      5 90
       standby        1.5 W     Altitude    km    -0.305  3.048| -0.305 12.192
       idle           3.5 W     Shock        g        10       |     75
       seek           8.0 W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA        38
       spin-up       15.8 W     ECC        Bit   ON THE FLY
                                MTBF         h     500000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SAMSUNG  WNR-32501A  JUMPER SETTING


 Jumper Setting
 ==============

 J5 Setting
 ----------

    o o  DXX
    o o  DCF
    o o  CSL    MASTER (1 DRIVE)
    xxx  -C/D
    1 2



    o o  DXX
    o o  DCF
    o o  CSL    SLAVE
    o o  -C/D
    1 2



    o o  DXX
    o o  DCF
    xxx  CSL     CABLE SELECT
    o o  -C/D
    1 2


