
S T 3 4 5 7 3 D C   B A R R A C . 9 L P    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform  4550/      MB        Heads           5|     |     |
Seek time   / track   7.1/ 1.2 ms          Sector/track     |     |     |
Controller           SCSI3 DI/WI/ULT/SCA2  Precompensation
Cache/Buffer           512 KB MULTI-SEGMEN Landing Zone
Data transfer rate   15.300 MB/S int       Bytes/Sector      512
                     40.000 MB/S ext SYNC
Recording method     EPR4 16/17                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 50    |    -40 70
Power: sleep              W     Humidity     %         5 90    |      5 95
       standby            W     Altitude    km                 |
       idle               W     Shock        g        10       |     75
       seek          10.0 W     Rotation   RPM      7200
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   ON THE FLY,SMART
                                MTBF         h    1000000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


