
V P - 3 4 3 6 0 S     E M P I R E   I I    QUANTUM
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform  4360/      MB        Heads          10|     |     |
Seek time   / track   9.5/ 2.0 ms          Sector/track     |     |     |
Controller           SCSI3 SI/ULTRA        Precompensation
Cache/Buffer           512 KB              Landing Zone
Data transfer rate   10.000 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     PRML 16/17                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C           55    |    -40 75
Power: sleep              W     Humidity     %         5 90    |      5 95
       standby            W     Altitude    km    -0.061  3.048| -0.305 12.192
       idle           6.5 W     Shock        g        10       |     60
       seek           9.5 W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA        33
       spin-up            W     ECC        Bit   ON THE FLY,REED SOLOMON
                                MTBF         h    1000000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
QUANTUM  JUMPER DEFINITION

 Jumper Settings
 ----------------

 SCSI Disk Jumper Definitions
 ----------------------------
 Quantum SCSI disk drives have multiple jumper setting options
 and are used to set specific drive features. The most common settings
 are used to define the drive SCSI ID and bus termination. Quantum
 SCSI drives have additional jumper settings used for optional
 features found on the drive. Listed below are the various jumper
 options that may be found on Quantum SCSI drives and the
 corresponding feature that they enable.


 DS - Delay Spin
 ---------------
 At power on or reset the drive motor starts to spin automatically
 and the drive prepares itself to perform read or write operations.
 With the Spin Delay feature enabled, at power on or reset the host
 [SCSI adapter] must send a START/STOP UNIT command to activate the
 drive motor for read or write operations. Spin Delay allows the drive
 to perform power sequencing to prevent an overload of the system
 power supply due to simultaneous, peak start-up current demands from
 multiple devices.


 EP - Enable Parity
 ------------------
 When enabled the drive generates parity information and performs
 parity checking of data across the SCSI bus. When disabled, parity
 information is still generated but not checked.


 J13 - Termination Power
 -----------------------
 When enabled this jumper supplies +5vdc termination power from
 the drive to the SCSI bus. With this jumper removed the SCSI bus
 must supply termination power. This jumper was used in place of
 the Term Power jumper on earlier model drives that supported Term
 Power as an option. At the factory, Quantum configures the disk drive
 with the J13 jumper enabled; that is, with a jumper installed across
 the pins labeled J13. To disable Termination Power supply from the
 disk drive, remove the jumper across the pins labeled J13.


 PF - Program Flash
 ------------------
 This jumper is used on drives which support flash programming of
 drive firmware. This feature is found on early models only. This is
 not used in the field and should be open, ignore this jumper.


 SCSI-Bus Device Identification
 ------------------------------
 Used in combination, the jumper settings across the SCSI ID
 reference pins determine the disk drive's SCSI-bus device I.D.


 SD - Spin Delay
 ---------------
 At power on or reset the drive motor starts to spin automatically
 and the drive prepares itself to perform read or write operations.
 With the Spin Delay feature enabled, at power on or reset the host
 [SCSI adapter] must send a START/STOP UNIT command to activate the
 drive motor for read or write operations. Spin Delay allows the drive
 to perform power sequencing to prevent an overload of the system
 power supply due to simultaneous, peak start-up current demands from
 multiple devices.


 SS - Self Seek
 --------------
 With the Self Seek jumper enabled the drive performs, at power on, a
 continuous seek diagnostic. This diagnostic will not terminate
 until: 1) Power is removed, 2) SS jumper removed. This feature
 performs no other function on the drive and should not be used.


 SY - Spindle Sync
 -----------------
 Used with disk drives that support synchronized spindle operation.
 Master or slave synchronized operation is set through a SCSI Mode
 Select Page. When the drive operates as a Master drive, it generates
 a spindle synchronization reference signal. When operating as a
 slave, the drive synchronizes its spindle according to the input
 reference. The drive always maintains local speed regulation when no
 reference signal is applied.


 TE - Termination Enable
 -----------------------
 One of the requirements of the SCSI bus is that it be properly
 terminated. If more than one SCSI device is connected to the host,
 only the last device must be terminated. The Terminator Enable
 (TE) jumper, when installed, enables an active termination circuit,
 thereby terminating the SCSI bus. With the TE jumper removed, bus
 termination is disabled.

 At the factory, Quantum configures the disk drive with termination
 enabled; that is, with a jumper installed across the termination pins
 on the corresponding jumper. To disable termination, the jumper must
 be removed.


 TP - Termination Power
 ----------------------
 The Termination Power (TP) jumper, when installed, enables
 termination power to be provided by the disk drive. At the factory,
 Quantum configures the disk drive with termination power enabled;
 that is, with a jumper installed across the termination power pins on
 the corresponding jumper. To disable termination power, remove the
 jumper.


 WP - Write Protect
 ------------------
 This feature, when present, is used to enable write protection on
 the drive. Installing the WP jumper disables the write feature to the
 drive and makes the device read only. At the factory, Quantum
 configures the disk drive with the WP jumper disabled.


 WS - Wait Spin
 --------------
 At power on or reset the drive motor starts to spin automatically
 and the drive prepares itself to perform read or write operations.
 With the Wait Spin feature enabled, at power on or reset the host
 [SCSI adapter] must send a START/STOP UNIT command to activate the
 drive motor for read or write operations. Wait Spin allows the drive
 to perform power sequencing to prevent an overload of the system
 power supply due to simultaneous, peak start-up current demands from
 multiple devices.



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


