
M 2 6 8 2 T A M    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    2379|  992|     |
Capacity form/unform   352/      MB        Heads           4|   11|     |
Seek time   / track  14.0/ 4.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate    4.200 MB/S int       Bytes/Sector      512
                     11.100 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -45 60
Power: sleep              W     Humidity     %        20 80    |      5 95
       standby            W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle               W     Shock        g         5       |     50
       seek               W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA        43
       spin-up            W     ECC        Bit
                                MTBF         h     250000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M2681T/2682T/2684T  JUMPER SETTING C141-E008-IM 1994

  +---------------------------------------------------------+
  |                                                         |XX I
  |                                                         |XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                                         |XX R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |    +-+CN5                                               |XX
  |    +-+                                                  |XX
  |                                                         |XX
  |                                                         |XX
  |                              +-CNH1                     |XX
  |                              | |                        |
  |                              | |                        |XX POWER
  |                              +-+                        |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M2681T/2682T/2684T  JUMPER SETTING C141-E008-IM 1994

 Jumper Setting
 ==============

 x = Factory default


 CNH1 1-2  Master/Slave
 ----------------------
    x 1-2  CLOSED  Master drive
           OPEN    Slave drive


 CNH1 3-4  IORDY I/O Channel Ready signal to interface
 -----------------------------------------------------
      3-4  CLOSED  IORDY connected to Host interface
    x      OPEN    IORDY is not connected to Host interface


 CNH1 5-6  ACMODE signal to interface
 ------------------------------------
      5-6  CLOSED  ACMODE signal connected to Host interface all power
                   safe commands executed normally
    x      OPEN    ACMODE signal is not connected to Host interface
                   all power safe commands are ignored


 CNH1 7-8  Automatic idle control
 --------------------------------
      7-8  CLOSED  Automatic idle control is disabled
    x      OPEN    Automatic idle control is enabled


 CNH1 9-10  Cable Select CSEL mode
 ---------------------------------
    x 9-10  OPEN   CSEL is not connected to Host interface normal mode
            CLOSED CSEL is connected to Host interface (Special cable
                   needed)


 CNH1 11-12  OPEN
 ----------------
 OPEN  DO NOT SHORT


 CNH1 13-14  RESERVED
 --------------------
 CLOSED RESERVED!



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
FUJITSU => GDT

 Tips & Hints about ICP controllers and other peripherals
 ========================================================

 Tagged queues and Fujitsu M 26xx harddisks
 ------------------------------------------
 Fujitsu Harddisks of the M26XX series do not support the SCSI-II
 feature tagged queues. You should disable this feature in the
 initialize disks menue of the GDTSetup program. An inquiry command
 shows, that the harddisk supports tagged queues (this is why you can
 enable it in the GDTSetup) but this is not true as stated by Fujitsu
 Germany.


