
R Z 7 4    AVASTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders        |     |     |
Capacity form/unform  3570/ 4520 MB        Heads            |     |     |
Seek time   / track  12.0/ 1.3 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer           512 KB SEGMENTED    Landing Zone
Data transfer rate    4.600 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C        10 50    |    -40 66
Power: sleep              W     Humidity     %        10 90    |      8 95
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek          33.0 W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA        54
       spin-up            W     ECC        Bit   264
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,FCC,TUV,UL1950,VDE



**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
DEC      DSP5300/5350/5400  INSTALLATION GUIDE EK-RH1CA-IG.A01

  +---------------------------------------------------------+
  |                                        Busy and Fault*  |XX J1
  |                                        LED (on bottom   |XX
  |                                        side)            |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |+-+
  |                                                         || |Option
  |                                                         || |J3
  |                                                         |+-+
  |+-+J6                                                    |XX J5
  |+-+LED                                                   |XX Power
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
DEC      DSP5000 SERIES  INSTALLATION GUIDE EK-RH1CA-IG.A01

 Jumper Setting
 ==============

 TERMPWR (Terminator Power)
 --------------------------
 Generally, the host is the only device on the SCSI bus required to
 provide TERMPWR for the bus. To ensure that there is a sufficient
 level of power along the entire SCSI bus, Digital Equipment
 Corporation recommends that all devices on the SCSI bus supply
 TERMPWR (if they are capable). SCSI devices are protected by a diode
 or similar semiconductor to prevent back flow of the terminator
 power when more than one device supplies this power.

               Option Connector
           +-----------------------+
 DSP5300   | o o o X o o o o o o 1 |  Pin 15-16
 DSP5350   |22 o o X o o o o o o o |
 DSP5400 --+-----------------------+---


               Option Connector
           +-----------------------+
 DSP5300W  | o o X o o o o o o o 1 |  Pin 17-18
 DSP5350W  |22 o X o o o o o o o o |
 DSP5400W--+-----------------------+---


 SCSI Bus Termination
 --------------------
 Both ends of the SCSI bus cable must be terminated. One end is
 terminated at the host. The other end must be terminated by the last
 SCSI device on the SCSI bus.

 When this drive is the last device on the SCSI bus, configure the
 drive to enable active termination.


 SCSI Bus Termination - DSP5300/5300W/5350/5350W/5400/5400W
 ----------------------------------------------------------
 DSP5300/5300W/5350/5350W/5400/5400W drives contain internal
 components to provide active termination of the SCSI bus.

 If active termination not required for this drive, make sure that the
 jumper is not installed.


               Option Connector
           +-----------------------+
 DSP5300   | o o X o o o o o o o 1 |  Pin 17-18
 DSP5350   |22 o X o o o o o o o o |
 DSP5400 --+-----------------------+---


               Option Connector
           +-----------------------+
 DSP5300W  | o X o o o o o o o o 1 |  Pin 19-20
 DSP5350W  |22 X o o o o o o o o o |
 DSP5400W--+-----------------------+---


 SCSI ID (Address) Selection
 ---------------------------
 Each device on the SCSI bus must have a unique SCSI ID number
 assigned to it. ID number for DSP5300/5350/5400 drives
 are from 0 through 7. For DSP5300W/5350W/5400W drives, the ID numbers
 range from 0 through 15 (wide SCSI). The SCSI ID is configured by
 placing jumpers across the referenced pins on the Option connector.


 SCSI ID - DSP5300/5350/5400
 ---------------------------

               Option Connector
           +---------------------1-+
 DSP5300   | o o o o o o o o * * * |
 DSP5350   |22 o o o o o o o * * * |
 DSP5400 --+-----------------------+---

   +----------+-----------------------+
   | SCSI ID  |   Jumper Loacation    |
   |          |         PINS          |
   |          |  5-6  |  3-4  |  1-2  |
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   |    1     | OPEN  | OPEN  | CLOSED|
   |    2     | OPEN  | CLOSED| OPEN  |
   |    3     | OPEN  | CLOSED| CLOSED|
   |    4     | CLOSED| OPEN  | OPEN  |
   |    5     | CLOSED| OPEN  | CLOSED|
   |    6     | CLOSED| CLOSED| OPEN  |
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+


 SCSI ID - DSP5300W/5350W/5400W
 ------------------------------

               Option Connector
           +---------------------1-+
 DSP5300W  | o o o o o o o * * * * |
 DSP5350W  |22 o o o o o o * * * * |
 DSP5400W--+-----------------------+---

   +----------+-------------------------------+
   | SCSI ID  |       Jumper Location         |
   |          |             PINS              |
   |          |  7-8  |  5-6  |  3-4  |  1-2  |
   +----------+-------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  | OPEN  |
   |    1     | OPEN  | OPEN  | OPEN  | CLOSED|
   |    2     | OPEN  | OPEN  | CLOSED| OPEN  |
   |    3     | OPEN  | OPEN  | CLOSED| CLOSED|
   |    4     | OPEN  | CLOSED| OPEN  | OPEN  |
   |    5     | OPEN  | CLOSED| OPEN  | CLOSED|
   |    6     | OPEN  | CLOSED| CLOSED| OPEN  |
   |    7     | OPEN  | CLOSED| CLOSED| CLOSED|
   |    8     | CLOSED| OPEN  | OPEN  | OPEN  |
   |    9     | CLOSED| OPEN  | OPEN  | CLOSED|
   |   10     | CLOSED| OPEN  | CLOSED| OPEN  |
   |   11     | CLOSED| OPEN  | CLOSED| CLOSED|
   |   12     | CLOSED| CLOSED| OPEN  | OPEN  |
   |   13     | CLOSED| CLOSED| OPEN  | CLOSED|
   |   14     | CLOSED| CLOSED| CLOSED| OPEN  |
   |   15     | CLOSED| CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+

 Configure Optional Features
 ---------------------------
 CAUTION
 The 5-volt signals of two or more drives should not be connected
 together or to any other current source by using the Option
 connector. Doing so may cause drive malfunction or component damage.

 Except when connecting several drives together for a spindle
 synchronization application, do not connect the ground signals of two
 or more drives together or to any other current source using the
 Option connector. Doing so may introduce ground loop problems.


 The following optional features can be configured according to your
 system requirements. They include:

 - On-Board Busy and Fault LEDs

 - Notification of AC power failure

 - Spindle synchronization

 - Write protection

 - Spin delay


 On-Board Busy and Fault LED Indicators
 --------------------------------------
 The drive's on-board Busy and Fault LED indicators are operational
 only when they are enabled by jumpers installed at the drive's
 option connector.

 Remote LED Connector J6
 -----------------------
           +3-1+
 Fault-----+o o+---- Busy Cathode
 Cathode +-+o o+---- +5VDC
         |-+4-2+--
         +5VDC


 Option Connector LED Hook-Up
 ----------------------------
 Some DSP5350W drive versions do not contain a Remote LED connector.
 If your drive does not contain the Remote LED connector, the remote
 or bezel-mounted LED may be attached at the drive's Option connector
 J3.

 NOTE
 External current limiting resistors must be provided to limit the
 current to 6 mA or less in the external LED circuit when using the
 Option connector. No current limiting resistor is required when the
 LED is rated to handle up to 7 mA maximum. The remote LED supplied as
 part of a Digital Equipment Corporation bezel not require the current
 limiting resistor.


 Remote Busy - To remotely monitor Busy status of the drive, remove
 the On-Board Busy LED Enable jumper from the Option connector, if
 present. Connect the cathode side of the remote Busy LED to the
 BSY_SINK L pin. The anode side of the LED connects to the +5 VDC pin.


 Remote Fault - To remotely monitor Fault status of the drive, remove
 the On-Board Fault LED Enable jumper from the Option connector, if
 present. Connect the cathode side of the remote Fault LED to the
 FLT_SINK L pin. The anode side of the LED connects to the +5 VDC
 pin.

                      BSY_SINK L
                  +5VDC+ | +------- FLT_SINK L
           +-----------+-+-+-------+
 DSP5350   | o o o o o * * * o o 1 | Option Connector
           |22 o o o o o o o o o o |
         --+-----------------------+---

                    BSY_SINK L
                +5VDC+ | +------- FLT_SINK L
           +---------+-+-+---------+
 DSP5350W  | o o o o * * * o o o 1 |  Pin 17-18
           |22 o o o o o o o o o o |
         --+-----------------------+---

            +--------+--------+--------+---------+
            |Drive   | Remote | Remote | Remote  |
            |        | Busy   | Fault  | LED     |
            |        | Cathode| Cathode| Anode   |
            +--------+--------+--------+---------+
            |DSP5350 | Pin 9  | Pin 7  | Pin 11  |
            +--------+--------+--------+---------+
            |DSP5350W| Pin 11 | Pin 9  | Pin 13  |
            +--------+--------+--------+---------+


 AC Failure Warning
 ------------------
 The drive can be warned that an AC failure is imminent in one of two
 ways:

 - Assert the AC_LOW L signal to a logic low
 - Assert the RESET signal on the SCSI bus

 The system must provide the warning at least 1 ms before it can no
 longer deliver safe voltages to the drive. When a warning is re-
 ceived, the drive prevents write-splices for outstanding writes and
 prohibits further write operations.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
DEC      DSP5000 SERIES  INSTALLATION GUIDE EK-RH1CA-IG.A01

 Notes on Installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 Mounting the Drive
 ------------------
 Mount the disk drive in any position.

 CAUTION
 Observe the screw length instruction printed on the chassis. There
 should be no more than 0.020 inch thread protrusion inside chassis.
 Excessive screw length will result in inadequate HDA clearance and
 possible drive malfunction.

 Allow at least 0.10 inch of clearance from adjacent surfaces and
 sufficient slack in all cables to provide adequate room for any drive
 movement on its shock mounts. Route cables carefully to prevent
 chaffing the cable insulation.

 Follow these directions to mount the drive in the bay.

 1. Position the drive in the bay, and select the drive chassis
    mounting locations (bottom or side mounting) that match your
    enclosure.

 2. Secure the unit using four #6-32 screws at the selected mounting
    locations. Screw length must not result in more than 0.020 inch
    thread protrusion inside chassis. Excessive screw length will
    result in inadequate HDA clearance, and may lead to drive mal-
    functions.


 Bezel Installation
 ------------------
 We recommended using only bezels supplied by Digital Equipment
 Corporation. Otherwise, the drive's isolation characteristics could
 be compromised. Contact your authorized representative for ordering
 information.


 SCSI Connector - DSP5200/5200D/5300/5350/5400
 ---------------------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-18762-10     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 104341-9        | AMP                     |
  +-----------------+-------------------------+
  | 90693-0050      | Molex                   |
  +-----------------+-------------------------+
    50-pin SCSI connector


 SCSI Connector - DSP5300W/5350W/5400W
 -------------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-38751-02     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 750737-7        | AMP                     |
  +-----------------+-------------------------+
    68-pin SCSI connector


 Option Connector - DSP5200/5200D
 --------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-12965-08     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 89511-620       | DuPont                  |
  +-----------------+-------------------------+
  | 90720-0020      | Molex                   |
  +-----------------+-------------------------+
    20-pin (2x10) connector


 Option Connector - DSP5300/5300W/5350/5350W/5400/5400W
 ------------------------------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-12965-09     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 79257-622       | DuPont                  |
  +-----------------+-------------------------+
    22-pin (2x11) connector

 Option Connector DSP5300/5350/5400
 ----------------------------------
 NOTE Pin 19 is removed from Revision 07 and later boards!


 Power Connector - DSP5000 Series
 --------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-18855-03     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | CA-1853-01      | Methode                 |
  +-----------------+-------------------------+
  | 15-24-4041      | Molex                   |
  +-----------------+-------------------------+
    4-pin connector

 J5   DC Power and pin connector assignments
 -------------------------------------------
      +-----J5-----+   pin 1    +12 VDC
      | 4  3  2  1 |   pin 2    +12 Volts Return
      +------------+   pin 3    + 5 Volts Return
                       pin 4    + 5 VDC


 Remote LED Connector - DSP5000 Series
 -------------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-12965-00     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 65624-104       | DuPont                  |
  +-----------------+-------------------------+
    4-pin connector


 Termination Resistor Pack - DSP5200
 -----------------------------------
  +------------------+-------------------------+
  | Part Number      | Vendor                  |
  +------------------+-------------------------+
  |13-26547-01       | Digital Equipment Corp. |
  +------------------+-------------------------+
  |4608X-104-221/331 | Bourns                  |
  +------------------+-------------------------+
  |CSC08A-05-221/331G| Dale Electronics        |
  +------------------+-------------------------+
   Resistors are 8-pin, plug-in resistors. Three required per drive.


 Termination Resistor Pack - DSP5200D
 ------------------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 13-36034-01     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 4614M-820-002   | Bourns                  |
  +-----------------+-------------------------+
   Resistors are 14-pin, plug-in resistors. Three required per drive.


 Shunt Jumper - DSP5000 Series
 -----------------------------
  +-----------------+-------------------------+
  | Part Number     | Vendor                  |
  +-----------------+-------------------------+
  | 12-14314-00     | Digital Equipment Corp. |
  +-----------------+-------------------------+
  | 530153-2        | Amp Canada              |
  +-----------------+-------------------------+
  | 65474-001       | DuPont                  |
  +-----------------+-------------------------+



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
DEC      DSP5000 SERIES  INSTALLATION GUIDE EK-RH1CA-IG.A01

 Product Summary
 ---------------
 DSP5000 Series 5.25-inch Disk Drives are high-performance, high
 capacity drives, designed and manufactures by Digital Equipment
 Corporation.


 Features
 --------
 Features of the DSP5000 Series drives include the following:

 - Formatted capacity ranging from 2000 MB to 4000 MB, depending
   upon model

 - 1.3 ms to 3.0 ms track-to-track seek time, depending upon model

 - 512 KB segmented cache buffer; 1,024 KB for DSP5400/5400W

 - End-to-end Error Detection Code/Parity on cache RAM

 - Four headers per sector

 - Embedded quadrature servo

 - Self-diagnostics

 - Downloadable SCSI firmware

 - Tagged command queuing

 - Seek ordering

 - Automatic block realloction

 - Glitch-free power on/off operation

 - Synchronized spindle operation (all DSP5300/5350/5400 models)

 - Low power consumption


 Seek Time
 ---------
       +----------------------------------+---------+--------+
       |                                  |DSP5300  |DSP5200 |
       |                                  |5350/5400|        |
       +----------------------------------+---------+--------+
       |Track-to-Track         msec. typ. |   1.3   |   3    |
       +----------------------------------+---------+--------+
       |Average                msec. typ. | <12     |  12.5  |
       |                       msec. max. |  25     |  22    |
       +----------------------------------+---------+--------+
       |Latency                msec. avg. |   5.6   |   8.33 |
       +----------------------------------+---------+--------+


 LED Indicators
 --------------
 The green Busy LED illuminates to signify the drive is working on a
 SCSI command. The amber Fault LED indicates a fault status.

 Both the Busy and Fault indicators light briefly during power up.
 This serves as a hardware and lamp test.

 During a calibration operation, the Busy LED is illuminated and the
 Fault LED flashes. Calibrations occur following some firmware up-
 grades. Generally, calibration periods last only about five minutes,
 after which the drive comes on-line and both indicators go out.

 If the Fault indicator lights at any other time, the drive has failed
 and likely requires service (unless the Fault LED was turned on by
 means of a MODE SELECT command).

 Remote Busy and Fault indicators can be connected to the drive to
 provide status display at a remote location or panel.


 Power-On Tests
 --------------
 After power is applied, and before spin-up is completed, the drive
 performs self-test diagnostics prior to making itself visible on the
 SCSI bus. These intitial self-test check most of the electronics that
 control HDA, but not the SCSI transceiver or SCSI connector.

 After spin-up, additional tests complete self-test coverage of the
 electronics module and the HDA. The unit appears not ready to the
 host between completion of the initial self-tests and completion of
 the drive's post spin-up tests.


