
A U 6 3 - I I I    AURA
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 PCMCIA TYPE III       Cylinders        |     |     |
Capacity form/unform    63/      MB        Heads           2|     |     |
Seek time   / track  16.0/ 5.0 ms          Sector/track     |     |     |
Controller           PCMCIA                Precompensation
Cache/Buffer            32 KB              Landing Zone
Data transfer rate    3.800 MB/S int       Bytes/Sector      512
                      5.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 60
Power: sleep          0.2 W     Humidity     %         8 80    |      8 80
       standby            W     Altitude    km    -0.305  3.048| -0.305 12.192
       idle           0.6 W     Shock        g        20       |    200
       seek               W     Rotation   RPM      5400
       read/write     1.9 W     Acoustic   dBA        32
       spin-up        2.8 W     ECC        Bit   -
                                MTBF         h     250000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
-ANY DIREC.

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
AURA     AU63-III

 The AU63-III is a fully compliant PCMCIA Type III disk drive that's
 designed for removability and portability. Its rugged, shock-
 resilient design is ideal for pen-based systems, palmtops, notebooks
 and full-featured portable computers equipped with the PCMCIA Type
 card slots.


