
7 8 1 3 A P    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 1579|     |
Capacity form/unform   813/      MB        Heads            |   16|     |
Seek time   / track      /     ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   71050/71626/71260/71084/7813/7541AP  QUICK REFERENCE

  +---------------------------------------------------------+
  |                                          J20******      |
  |         COMPONENT SIDE                      ******      |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |  1
  |                                                         |XX Power
  |                                                         |XX
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   71626/71260/71084/7813/7541AP  QUICK REFERENCE

 Jumper Setting
 ==============

 Jumper Designation
 ------------------
     +---------------- J20
     |  +------------- J21 RESERVED!
     |  |  +---------- J22 RESERVED!
     *  *  *  *  *  *
     *  *  *  *  *  *
              |  |  +- J25
              |  +---- J24
              +------- J23
  +-----------------------+------+------+------+
  |                       | J24  | J23  | J20  |
  +-----------------------+------+------+------+
  | Cable Select          |      |      |      |
  |  Disabled (default)   |OPEN  |      |      |
  |  Enabled              |CLOSED|      |      |
  +-----------------------+------+------+------+
  | Write Cache           |      |      |      |
  |  Enabled (default)    |      |OPEN  |      |
  |  Disabled             |      |CLOSED|      |
  +-----------------------+------+------+------+
  | Master/Slave          |      |      |      |
  |  Only Drive in system |      |      |CLOSED|(default)
  |  Master               |      |      |CLOSED|
  |  Slave                |      |      |OPEN  |
  +-----------------------+------+------+------+
 A spare shunt is shipped between J23 and J24.

 NOTE
 Jumpers J21 and J22 are factory reserved.


 DC Power connector
 ------------------
  pin 1    +12 VDC
  pin 2    +12 Volts Return
  pin 3    + 5 Volts Return
  pin 4    + 5 VDC



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
MAXTOR   71626/71260/71084/7813/7541  QUICK REFERENCE


 Installation Steps
 ------------------
 Warning
 Pre-loaded Software on Drive
 This Maxtor hard drive is factory configured with a 112MB partition
 containing Max Blast Disk Manager installation software by Ontrack
 Systems. Please leave this partition intact until you choose the
 appropriate installation option.

 As a precautionary measure, Maxtor recommendeds that you download a
 copy of the MaxBlast software to a blank diskette even if you choose
 an alternate high-level formatting method.

 Install a 40-pin ribbon connector. The striped edge of this cable
 represents pin 1 and must be oriented towards pin 1 at the drive
 connector and at the host connector.

 Install a DC power connector...

 If AT BIOS supports user programmable parameters, program System BIOS
 with one of these default Parameters.

 Model      Cylinders   Heads    Sectors   Capacity
 71262AP    3158        16       63        1,626 MB
 71260AP    2632        16       63        1,260 MB
 71084AP    2105        16       63        1,084 MB
  7813AP    1579        16       63          813 MB
  7541AP    1052        16       63          541 MB

 If AT
 BIOS does not support programmable drive type, choose parameters that
 closely match, but do not exceed, the drive's formatted capacity.

 The drive is now ready for partitioning and high-level formatting
 with any operating system. For example:

          Partition the drive using the FDISK command from MS-DOS
          version 3.3 of higher.
          High level format the drive using the FORMAT command from
          MS-DOS version 3.3 or higher.

 Secure the drive in a suitable drive bay with 6-32 x 1/4" screws.

 NOTE
 WPC and Landing Zone BIOS entries do not need a specific number for
 proper operation. Maxtor AT interface hard drives will ignore and
 override any numbers programmed.


 Important - Please Read
 -----------------------
 This Quick Reference is intendened only for experienced engineers and
 technicans. If you are not familar with the procedures described
 here, please have a qualified computer technican perform drive
 handling and installation.


