
D 3 7 3 5    NEC
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1084|  537|     |
Capacity form/unform    44/      MB        Heads           2|    4|     |
Seek time   / track  23.0/     ms          Sector/track   41|   41|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    1.500 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek          10.0 W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      50000
                                Warranty Month
Lift/Lock/Park     NO           Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
NEC      D3735  INSTALLATION GUIDE DEC. 92

  +---------------------------------------------------------+
  |                                                  JP13+-+|
  |                                                  JP12+-+|
  |                                                  JP11+-+|
  |                                                      +-+|   I
  |                                                        40XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                                         |XX R
  |                                                         |XX F
  |                                                         |XX A
  |                            +--JP17                      |XX C
  |                            +--+                         |XX E
  |                           3 2 1                         |X1
  | +-+LED                                                  |
  | +-+CONNECTOR                    +-------+               |XX
  |                                 +-------+               |XX Power
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
NEC      D3735  INSTALLATION GUIDE DEC. 92

 Jumper Setting
 ==============

 JP12/JP13  Master/Slave
 -----------------------
 +-------------+--------------+--------------------------------+
 |    D37x5    |   D3765      | Function                       |
 +------+------+------+-------+--------------------------------+
 | JP12 | JP13 | JP12 | JP13  |                                |
 +------+------+------+-------+--------------------------------+
 |OPEN  |OPEN  |CLOSED|CLOSED | Single drive (default setting) |
 +------+------+------+-------+--------------------------------+
 |CLOSED|OPEN  |OPEN  |CLOSED | Master (dual drive system)     |
 +------+------+------+-------+--------------------------------+
 |CLOSED|CLOSED|OPEN  |OPEN   | Slave (dual drive system)      |
 +------+------+------+-------+--------------------------------+



 JP17  Power Mode Jumper
 -----------------------
          +---------+
          | O--O  O |
          +-1--2--3-+

    1-2  CLOSED  Auto power save mode disabled
    2-3  CLOSED  Auto power save mode enabled


 The other jumpers are reserved for factory use!



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
NEC      D3735/3781/3772  INSTALLATION GUIDE DEC. 92 REV. A

 NOTES ON INSTALLATION
 =====================

 First install the drive with the components side to the bottom.
 Connect the system power and interface cables to the drive
 connectors. Both connectors are keyed and can only be connected one
 way. The interface connector may not be keyed. In this case check
 if the red edge of the interface cable is connected to the pin 1 of
 the drive connector.

 After installing the hardware please turn on your computer system
 and run the setup program. Please identify which model has to be
 installing and use the NEC recommended drive parameter for the set up
 setting. For this purpose edit the logical parameters into the
 "User type 47/48". The IDE interface accept two drives
 (Master/Slave). For a dual drives installation jumper both drives.
 The Master/Slave operation is guranteed only with NEC disk products.
 In order to install DOS please run the DOS program FDISK and Format
 C:/s accordingly.
 In case of installation trouble please contact NEC hotline:
              Tel. 49/89/93006 708

 Caution: IDE drives don't need a low level format. If a new low
 level format become neccessary, please run only qualified programs
 for IDE devices like WDFMT.EXE by use of physical parameters.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
NEC      NEC DRIVES  INSTALLATION GUIDE DEC. 92 REV. A

 NEC drives
 -----------
 The NEC IDE/SCSI drives are designed to work in the IBM AT and
 compatible systems and gurantee the operation with any standard IDE
 and SCSI Controller. Further, the NEC drives provide compatibility to
 the ATA/SCSI CAM and ANSI (X3-131-199x) standard as well as to all
 known operating systems.


