
7 2 7 3 S    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform   273/      MB        Heads           2|     |     |
Seek time   / track  12.0/     ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                      5.600 MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
MAXTOR    SCSI INSTALLATION

         GENERIC INSTALLATION PROCEDURE FOR A SCSI DRIVE
   -----------------------------------------------------------

 1. Install a 50 pin ribbon connector making sure pin 1, which
    can be identified by the striped edge of the cable, is closest
    to the power connector on the drive.

 2. Install a DC power cable to the back of the drive.

 3. Verify the SCSI ID selection.
    Note: SCSI ID usually needs to be set to 0 to be the boot drive.
    The last physical device on the SCSI bus must be terminated.
    Any other drive or SCSI device connected between the host and
    the device at the end of the bus must not be terminated.

 4. Apply power to the computer.

  4a. When memory test is complete go into your system's Standard
      C-MOS set-up.
      (Note:  There are various ways to get into C-MOS set-up,
      please refer to system's manual for instuctions.)

  4b. Set the drive type to "Not Installed". This intelligent drive
      will identify itself to the SCSI host adapter.

 5. Boot from a DOS diskette that has FDISK.EXE and FORMAT.COM on
    it. At the A> prompt type in FDISK. At the menu options select
    option 1 to create a DOS partition. Another menu will appear and
    from those options choose 1 to create a Primary DOS partition.
    Select yes to make 1 large partition and it will automatically
    become active. Then escape from FDISK.

 6. At the A> prompt type in FORMAT C:/S
    This does a high-level format on the drive and transfers the
    system files in order for the drive to be bootable.
    (Note: Maxtor SCSI drives are low-level formatted at the factory)

 7. The drive is now bootable. As a test remove the DOS diskette
    from A and press reset to re-boot the computer, a C> should be
    displayed, the drive is now ready for operation.


