
S H D - 3 1 7 2 A   A P O L L O   3 5 0    SAMSUNG
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    2210|  968|     |
Capacity form/unform   356/      MB        Heads           4|   16|     |
Seek time   / track  13.0/ 4.0 ms          Sector/track     |   45|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    3.000 MB/S int       Bytes/Sector      512
                      8.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 65
Power: sleep              W     Humidity     %         8 85    |      8 95
       standby            W     Altitude    km    -0.061  3.048|        12.192
       idle           3.6 W     Shock        g         5       |     75
       seek           6.4 W     Rotation   RPM      3600
       read/write     6.6 W     Acoustic   dBA        40
       spin-up        1.5 W     ECC        Bit   88,REED SOLOMON
                                MTBF         h     250000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SAMSUNG  SHD-3211A/3212A/3171A1/3172A1  USER'S MANUAL 264 034001 BAAK

  +---------------------------------------------------------+
  |                                            +-+C/D       |XX A1
  | +-+                                        | |DSP       |XX
  | | |                                        +-+          |XX
  | | |                                                     |XX
  |++++                                                     |XX I
  |+-+External                                              |XX N
  |   LED                                                   |XX T
  |                                                         |*X E
  |                                                         |XX R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |                                                         |X1
  |                                                         |
  |                                                         |XX
  |                                                         |XX Power
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SAMSUNG  SHD-3211A/3212A/3171A1/3172A1  USER'S MANUAL 264 034001 BAAK

 Jumper Setting
 ==============


 8-pin User Configurations Jumper Block
 --------------------------------------

    +---+          +---+         +---+
    |o o|C/D       |xxx|C/D      |xxx|C/D
    |o o|DSP       |o o|DSP      |xxx|DSP
    |o o|          |o o|         |o o|
    |o o|          |o o|         |o o|
    +---+          +---+         +---+
   2 Drive        1 Drive       2 Drive
   SLAVE                        MASTER



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SAMSUNG  SHD-3211A/3212A/3171A1/3172A1  USER'S MANUAL 264 034001 BAAK

 Notes on Installation
 =====================

 Shipping
 --------
 When transporting or shipping a drive, a SAMSUNG-approved container
 must be used. Keep your original box. Shipping a drive in a non-
 approved container will void the drive warranty.

 Samsung recommends shipping by an air-ride carrier experienced in
 handling computer equipment.


 Environment
 -----------
 - Avoid harsh humidity and temperature. Do not place near the magnet.
   Samsung Hard Disk Drives do not require Low level Format because
   Samsung Drives have been formatted before shipping in the factory.

 - The head/disk assembly is sealed and does not contain any user-
   serviceable components. Tampering with the warranty label will
   void the warranty.


 Warranty
 --------
 The terms of your warranty are determined by your authorized Samsung
 Distributor or Dealer. Warranties do not extend to the data stored
 on Drives.


 Installing your Disk Drive
 --------------------------
 1. Turn off the system power.

 2. Remove the top cover of your computer according to the
    instructions in your system manual.

 3. Master/Slave configuration.

 4. Most interface cables have a red stripe on one side to designate
    Pin 1. Make sure Pin 1 at the cable connector is aligned to Pin 1
    at the drive connector and Pin 1 at the motherboard or interface
    host adapter connector. The maximum cable length is 18 inches
    (0.46m, ATA Rev. 3.0).

 5. Connect the power cable to the drive 4-pin power connector.

 6. Position drive in the mounting slot of your system. #6-32 UNC
    screws should be used. Be careful not to over-tighten screws. You
    could damage the PCBA.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SAMSUNG  SHD-3211A/3212A/3171A1/3172A1  USER'S MANUAL 264 034001 BAAK

 System startup and operation
 ----------------------------
 1. Power up the system.
 2. Run the SETUP program.
 3. Formatting the drive.
    Samsung AT interface drives are low-level formatted at the factory
    an do not need low-level formatting. Partition the drive using the
    DOS FDISK utility. Then, high level format the drive using the
    DOS FORMAT utility. Use DOS 3.3 or higher.

    CAUTION
    If you partition or format a drive at any level you erase all your
    data. Backup the drive first. Samsung assumes no liability for
    lost user data.


