
C P - 2 0 4 4    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders     548|  980|     |
Capacity form/unform    42/      MB        Heads           4|    5|     |
Seek time   / track  15.0/ 2.0 ms          Sector/track   38|   17|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            32 KB              Landing Zone      980
Data transfer rate    1.500 MB/S int       Bytes/Sector      512
                      4.500 MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 60
Power: sleep          0.2 W     Humidity     %         8 80    |      8 80
       standby        0.3 W     Altitude    km    -0.061  3.048|        12.192
       idle           1.5 W     Shock        g        10       |    100
       seek           2.5 W     Rotation   RPM      3486
       read/write     2.5 W     Acoustic   dBA        34
       spin-up            W     ECC        Bit
                                MTBF         h     150000
                                Warranty Month        12
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CP2044  CUSTOMER OPTIONS

  +------------------------------------------------------+
  | +-+                                        MS+++CD   |X44
  | | |                                          +++   I |XX Power
  | | |                                                N |XX +5V 41/42
  | +-+                                                T |XX GND 43
  |                                                    E |XX
  |                                                    R |XX
  |                                                    F |X* Position
  |                                                    A |XX 20-Key
  |                                                    C |XX
  |                                                    E |XX
  |                                                      |XX
  |                                                      |XX
  |                                                      |1X
  |                                                      |XX Factory
  |                                                      |XX test
  +------------------------------------------------------+   points




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CP2044  CUSTOMER OPTIONS

 Jumper setting
 --------------

 M/S C/D   Master/Slave
 -----------------------
      M/S  C/D    For Master (C Drive) when M/S is CLOSED, place
      +-+         Jumper as shown.
      |*|  *
      |*|  *
      +-+

      M/S  C/S     If Master/slave feature is selected at Pin 28 of
               the interface/power connector, jumper M/S should be
       *   *       left open as ashown.
      +-----+
      |*   *|
      +-----+

 The CP2044 drives are designed to operate either as a Master drive
 (C Drive) or a Slave Drive (D Drive). This feature is dependent on
 two drive settings; the status of hardware Jumper M/S and the firm-
 ware setting of a feature bit. When (M/S) is closed, and the feature
 bit is set, the drive will assume the role of a Master Drive.
 When M/S is open, and the feature reset, the drive will act as the
 Slave. In single drive configurations M/S must remain in the closed
 position.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
CONNER   CP2044  CUSTOMER OPTIONS

 Mounting Holes
 --------------
 Side:   3 mm x 0.5 mm THD (4x) 4 mm Max. Insertion
 Bottom: 3 mm x 0.5 mm THD (4x) 4 mm Max. Insertion


