
S T 1 2 5 5 1 N D    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    2756|     |     |
Capacity form/unform  2100/ 2547 MB        Heads          19|     |     |
Seek time   / track   9.0/ 0.9 ms          Sector/track     |     |     |
Controller           SCSI2 DIFFERENTIAL    Precompensation
Cache/Buffer          1024 KB              Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 70
Power: sleep              W     Humidity     %                 |
       standby       12.0 W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      7200
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     500000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


