
S T 3 3 4 4 0 A   M E D A L I . 3 4 4 0    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 6610|  826| 1024
Capacity form/unform  3411/      MB        Heads           8|   16|     |   16
Seek time   / track  10.5/ 2.0 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           128 KB SEACACHE     Landing Zone
Data transfer rate    5.500 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     ZBR PRML89                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby        1.0 W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek           7.2 W     Rotation   RPM      5376
       read/write     9.2 W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST33440A/34250A  MEDALIST 3440/4250AT  QUICK REFERENCE GUIDE

 Jumper Setting
 ==============


 Front View

                            Slave drive ON (OFF for Master) ------+
                             Slave Present (used on Master) ----+ |
                 Master/Slave timing protocol causes Master --+-+ |
                  drive to wait up to 31 seconds for slave    | | |
    (TOP)         to respond. Must be used with pins 3-4      | | |
                                                           +--+-+-++
                                                           |o o o o1
 Option Block  -----PWA------------------------------------+o o o o2--
                                                           ++----+-+
  (BOTTOM)                                Cable Select -----+    |
                       Spare jumper stored on pins 2-4 ----------+


