
M P C - 3 1 0 2 A T    FUJITSU
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders   11467|16383|     |
Capacity form/unform 10200/      MB        Heads           6|   16|     |
Seek time   / track  10.5/ 2.0 ms          Sector/track     |   63|     |
Controller           ULTRA ATA             Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate   15.000 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext UDMA
Recording method     EPRML16/17                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %         8 80    |      5 85
       standby            W     Altitude    km    -0.060  3.000| -0.060 12.000
       idle           4.2 W     Shock        g        10       |     75
       seek               W     Rotation   RPM      5400
       read/write     5.5 W     Acoustic   dBA
       spin-up            W     ECC        Bit   SMART
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  MPC3102AT  JUMPER SETTING

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |+-+Master
  |                                                         || |/Slave
  |                                                         |+-+
  |                                                         |XX Power
  |                                                         |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  MPC3102AT  JUMPER SETTING

 Jumper Settings
 ===============

 Master Drive
 ------------
 +--2-4-6+
 |  X * *|
 |  X xxx|
 +--1-3-5+


 Slave Drive
 -----------
 +--2-4-6+
 |xxx * *|
 |  * xxx|
 +--1-3-5+


 Cable Select Mode Setting (CSEL)
 --------------------------------
 Cable select mode gives an alternative method by which the drive may
 be set to Master or Slave. A special cable is needed to implement
 this features and should only be used if supported by BOTH drives.

 +--2-4-6+
 |  xxx *|
 |  * xxx|
 +--1-3-5+


 ********************************************************************

 Spare Jumper Settings
 ---------------------
 If the drive cannot be recognized by the system, due to non-
 translating BIOS (legacy), which does not allow drives with
 capacities greater than 2.1GB, the following jumper setting should be
 applied.


 Master Drive Setting
 --------------------
 +--2-4-6+
 |  X * X|
 |  X * X|
 +--1-3-5+


 Slave Drive Setting
 -------------------
 +--2-4-6+
 |xxx * X|
 |  * * X|
 +--1-3-5+


 Cable Select Mode Setting (CSEL)
 --------------------------------
 +--2-4-6+
 |  xxx X|
 |  * * X|
 +--1-3-5+



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
FUJITSU  MPC3102AT  JUMPER SETTING

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
      x           x                |  |     |           |     |  |
 +------x------x-------+           |  +-----+           +-----+  |
 +-+------x--x-------+-+           +--+                       +--+
   |       xx        |
   |     x    x      |
   +---x--------x----+
     x            x

 Orientation
 -----------
 The drive may be installed in one of three orientations; PCA down or
 on either edge. Inclination from vertical or horizontal should not
 exceed 5*.


 Grounding
 ---------
 Sufficient grounding will be providing for correct operation when
 the drive is screwed into an electrically grounding frame.


 Cooling
 -------
 Allow space above and below the drive to provide for adequate air
 flow. Fan cooling is recommended. The disk enclosure temperature,
 measured at top center, should never exceed 60*C.


