
M 2 3 9 1 K    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 8"/FH                 Cylinders    1916|     |     |
Capacity form/unform      / 1062 MB        Heads          11|     |     |
Seek time   / track  12.0/ 2.0 ms          Sector/track     |     |     |
Controller           ESMD                  Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                      3.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     36/12V       Temperature *C         5 40    |    -40 60
Power: sleep              W     Humidity     %        20 80    |      5 95
       standby       99.9 W     Altitude    km            3.000|        12.000
       idle               W     Shock        g         3       |     25
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     200000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M2392K  JUMPER SETTING

  +-----------++--------------------------------------------------+
  | INTERFACE ||               +---SW4---+                  RDY * |
  | PCA       || +--SW3----+   8---------1 ON               ST0 * |
  |           || 8---------1 ON                              |  * |
  |           ||                                             |  * |
  |           ||                                             |  * |
  |           ||     MAIN PCA                                |  * |
  |           ||                                             V  * |
  |           ||                                            ST6 * |
  |           ||                                                  |
  |           ||                                                  |
  |         +-+|                                                  |
  |       ON|+-+                                                  |
  |    1+--+||                                                    |
  |   SW1  |||                                                    |
  |     |  |||                                                    |
  |     |  |||         +--SW1-------1+---SW2------1               |
  |    8+--+||      ON +------------++------------+ON             |
  +---------++----------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M2392K  JUMPER SETTING

 Jumper Setting
 ==============


 Terminal SW3 Main PCA
 =====================

 KEY 1(2^3)  2(2^2)  3(2^1)  4(2^0)  Disk address
 ------------------------------------------------
     OFF     OFF     OFF     OFF          0
     OFF     OFF     OFF     ON           1
     OFF     OFF     ON      OFF          2
     OFF     ON      ON      ON           3
     OFF     ON      OFF     OFF          4
     OFF     ON      OFF     ON           5
     OFF     ON      ON      OFF          6
     OFF     ON      ON      ON           7
     ON      OFF     OFF     OFF          8
     ON      OFF     OFF     ON           9
     ON      OFF     ON      OFF         10
     ON      OFF     ON      ON          11
     ON      ON      OFF     OFF         12
     ON      ON      OFF     ON          13
     ON      ON      ON      OFF         14
     ON      ON      ON      ON          15

 Keys 1 to 4 are used for setting the disk logical address (0 - 15).
 Switch positions are binary coded.

    Key 5
        -----
    ON  Enable
    OFF Disable

 This drive supports the tag 4/5 functions.  The user can select these
 functions by setting Key 5.  In the OFF position tag 4/5 are
 disabled. Control units that do not support teg 4/5 require this set
 to OFF.


    Key 6
    -----
    ON  Soft sector mode
    OFF Hard sector mode

 The user can select either hard sector or soft sector mode

    Key 7
    -----
    ON  Tag 2 system (ANSI type 1 mode)
    OFF Tag 4 system (ANSI type 2 mode)

 Tag 2 and Tag 4 systems have different methods of sending the most
 significant bits (2 bits).  Select the system used with Key 7.


    Key 8
    -----
    ON  Remote mode
    OFF Local mode

 SW3 Key 8 determines the disk drive initiation condition. When the
 drive is in remote mode, the control unit initiates the drive and
 rotates the disk by issuing the PICK/HOLD signal. In local mode the
 disks rotate as soon as the power is turned on.


 Terminal SW4 Main PCA
 ---------------------
 Keys   1, 2, 3, 4, 5.
 These keys must not be moved. They are factory settings only.

    Key 6
    -----
    ON  Runt sector enabled
    OFF Runt sector disabled

 When this key is ON and the track capacity cannot be divided by the
 number of sectors, the last dummy sector is shorter than usual. When
 this switch is OFF, the last sector is longer than usual.


    Key 7
    -----
        ON      Vertical mounting (on side)
        OFF     Horizontal mounting

 This key adjusts the servo characteristics that depend on the
 orientation of the drive.

 NOTE : A wrong setting may cause seek or write offtrack errors.


    Key 8
    -----
    ON  Release timer period = 1500 milliseconds
    OFF Release timer period = 500 milliseconds
                (See SW2 Key 3 for further details)


 Terminal SW2 Main PCA
 ---------------------
 Key  1    2    Function
 -----------------------
     OFF OFF    Both channels enabled
     ON  OFF    Channel A disabled
     OFF ON     Channel B disabled
     ON  ON     Both channels enabled

 These keys determine the connection state between the drive and the
 control unit of the host computer. Key 1 corresponds to Channel A
 while Key 2 to Channel B. The drive port is disconnected from the
 control unit and all interface signals are disabled when each setting
 is ON.

    Key 3
    -----
    ON  Release timer activated
    OFF Release timer not activated

 When the release timer is activated, the drive reserved condition
 shall be released automatically after the specified period in the
 RESERVE command. (See SW4 Key 8). When not activated, the reserved
 condition may be released only by a RELEASE command issued by the
 controller.


    Key 4
    -----
    ON  Enable write protection
    OFF Disable write protection

    Key 5
    -----
    ON  Calibration seek performed
    OFF Normal

 Calibration seek must be executed at any time the main PCA is
 replaced to optimise the servo control coefficient. To execute the
 calibration seek set key 5 to the ON position and turn on the power.
 Calibration seek is performed automatically. After completion in
 approx. 4 minutes the STOP LED will blink. Set key 5 to the OFF
 position to put the drive in the READY state.


    Key 6
    -----
    ON  Set device type to M2391K/D
        OFF     Set device type to M2392K/D


    Keys    Number of bytes per sector
 --------------------------------------
      7     16384   (2^14)
      8      8192   (2^13)
      9      4096   (2^12)
     10      2048   (2^11)

 The number of sectors per track is determined by the settings of SW1
 Main PCA keys 1 to 10 and SW2 keys 7 to 10 which controls the number
 of bytes per sector regardless of the sector mode setting (SW3 Key
 6). The actual bytes/sector value is obtained by adding 2 to the
 position setting value. The bytes/sector must be an even number.


 Terminal SW1 Main PCA
 ---------------------
 Setting the sector count : Use in conjunction with SW2 keys 7 to 10

 Keys Number of bytes per sector
 -------------------------------
   1   1024    (2^10)
   2    512    (2^9)
   3    256    (2^8)
   4    128    (2^7)
   5     64    (2^6)
   6     32    (2^5)
   7     16    (2^4)
   8      8    (2^3)
   9      4    (2^2)
  10      2    (2^1)

 (See notes for SW2 keys 7 to 10)


 Terminal SW1 Interface PCA
 --------------------------
 Spindle synchronisation mode :

 Key    1       2       3       Function
 -------------------------------------------
     Ignored Ignored   OFF      Program mode
     OFF     OFF       ON       Slave mode
     ON      OFF       ON       Master mode
     OFF     ON        ON       Self (local) mode
     ON      ON        ON       Master control mode

 The mode is set by switch for the drive or command (program mode)
 from the control unit through the interface.


    Key 4
    -----
    ON  Disable spindle sync from channel B
    OFF Enable spindle sync from channel B

 In the ON position spindle sync mode is enabled only from channel A.


 Key  5   6
      ON  ON    Slave synch termination enabled
      OFF OFF   Slave synch termination disabled

 Key  7   8
      ON  ON    Master synch termination enabled
      OFF OFF   Master synch termination disabled

 A pair of signal lines in a balanced differential type must be
 terminated properly. The line termination is alread mounted in the
 interface PCA and can be activated through keys 5 to 8.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
FUJITSU  M2392/91K  JUMPER SETTING

 Notes On Installation
 =====================

 Drive mounting
 --------------

     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  | x
   |                 |   |  |     | |     |  | x+----------------+x
 +-+-----------------+-+ |  |     | |     |  | ||x              x||
 +---------------------+ |  |     | |     |  | ||  x          x  ||
                         |  |     | |     |  | ||    x      x    ||
      x           x      |  |     | |     |  | ||      x  x      ||
 +------x------x-------+ |  +-----+ +-----+  | ||       xx       ||
 +-+------x--x-------+-+ +--+             +--+ ||     x    x     ||
   |       xx        |                         ||   x        x   ||
   |     x    x      |                         || x            x ||
   +---x--------x----+                         |x                x|
     x            x                           x++----------------++x
      UNACCEPTABLE!                                UNACCEPTABLE!
      Never install PC board on the Top!


 Installation direction
 ----------------------
 The drive may be installed either PCA up or on left edge (viewed from
 the rear).


 Mounting Kit
 ------------
 It is recommended that the drive should be mounted in the special
 mounting frame designed for this purpose.


 Cooling
 -------
 Cooling should be provided to keep the temperature of the disk
 enclosure within specified limits. An air flow of at least 1m(3)/min
 is recommended.


