
S D - 3 2 1 0 - 0 0    TEAC
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1695|     |     |
Capacity form/unform   215/      MB        Heads           4|     |     |
Seek time   / track  17.0/ 7.0 ms          Sector/track   62|     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation
Cache/Buffer            64 KB LOOK-AHEAD   Landing Zone
Data transfer rate    2.500 MB/S int       Bytes/Sector      512
                      4.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 60
Power: sleep          0.1 W     Humidity     %         8 80    |      8 80
       standby        0.5 W     Altitude    km                 |
       idle           3.2 W     Shock        g         5       |     70
       seek           5.1 W     Rotation   RPM      3600
       read/write     3.4 W     Acoustic   dBA        45
       spin-up            W     ECC        Bit
                                MTBF         h     100000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,TUV,UL478


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TEAC     SD-3210-00  3.5-IN. HARD DISK DRIVE SPECIFICATION 10530646-00

 Jumper Setting
 ==============

 The SCSI ID shall be set with the individual straps of SP, S0, S1,
 and S2 on the PCBA.
 The SP strap is to reserve the setting logic for S0, S1 and S2.

   +----------+---------------+----------------+
   |          |     SP=ON     |     SP=OFF     |
   +----------+---------------+----------------+
   |SCSI ID   | S2   S1   S0  |  S2   S1   S0  |
   +----------+---------------+----------------+
   |   0      | ON   ON   ON  |  OFF  OFF  OFF |
   +----------+---------------+----------------+
   |   1      | ON   ON   OFF |  OFF  OFF  ON  |
   +----------+---------------+----------------+
   |   2      | ON   OFF  ON  |  OFF  ON   OFF |
   +----------+---------------+----------------+
   |   3      | ON   OFF  OFF |  OFF  ON   ON  |
   +----------+---------------+----------------+
   |   4      | OFF  ON   ON  |  ON   OFF  OFF |
   +----------+---------------+----------------+
   |   5      | OFF  ON   OFF |  ON   OFF  ON  |
   +----------+---------------+----------------+
   |   6      | OFF  OFF  ON  |  ON   ON   OFF |
   +----------+---------------+----------------+
   |   7      | OFF  OFF  OFF |  ON   ON   ON  |
   +----------+---------------+----------------+

 Note: The strap states are as follows:

       1: Strap open
       2: Strap short



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
TEAC     SD-3210-00/3240-00/30

 Notes on Installation
 =====================

 Drive Orientation
 -----------------
 The head assembly uses a rotary actuator that provides circular arc
 head motion about the support point. This keeps the drive well-
 balanced and allows it to be installed in virtually any physical
 orientation.


     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+


 Screws
 ------
 3-#6-32UNC 4 deep each side.
 4-#6-32UNC 4 deep bottom.


 Auto shipping lock function
 ---------------------------
 The auto shipping lock is designed to protect the media against the
 risk of damage due to vibration and shock during transport. When the
 power is turned off, the head carriage is locked automatically at the
 shipping zone, within the inside limit of the work zone, to protect
 your important stored data.


 Automatic self-diagnosis
 ------------------------
 When the power is switched on, the SD-3210 and SD-3240 automatically
 performs a selfcheck sequence, checking program ROM, buffer RAM, and
 interface register.


