
P A L L A D I U M   P 1 2 0 0 - 2 A F    JTS CORP.
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SUPERSLIMLINE    Cylinders        | 2332|     |
Capacity form/unform  1200/      MB        Heads            |   16|     |
Seek time   / track  14.0/     ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     16.600 MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
JTS      PALLADIUM P1000/1200-2AF  INSTALLATION GUIDE P/N 88098-001

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |
  |                                                         |XX Power
  |                                                         |XX
  |                                                         |
  |                                                         |+-+
  |                                                         || |JP1
  +---------------------------------------------------------++-+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
JTS      PALLADIUM P1000/1200-2AF  INSTALLATION GUIDE P/N 88098-001

 Jumper Setting
 ==============

     JP1
  +8-----2+ +-POWER-++---IDE-----
  |o o o o| |O O O O||oooooooooooo
  |o o o o| |+12  +5||1oooooooooooo
  +7-----1+ \-------/+--------------


 Master (Default)
 -----------------
  o o x o           When installing only one drive, leave the jumper
  o o X o           in this factory set position. You can also use
                    this setting for the first (Master) drive, when
                    attaching a second (Slave) drive that conforms
                    ATA-2 specifications.

 Master with Slave
 -----------------
  o x o o           Use this jumper setting for the first (Master)
  o X o o           drive, in two drive installations where the
                    second (Slave) drive does NOT conform to ATA-2
                    (EIDE) specifications.

 Slave
 -----
  o o o x           Use this jumper setting for the setting for the
  o o o X           second drive of a two drive installation. Only one
                    of the two drives attached can have this setting.


 Cable Select
 ------------
  o o o o           When using this jumper setting, the cable select
  o o xxx           line (pin 28) determines the assignment of Master
                    and Slave in two drive installations. Verify that
                    you have the necessary signal cable modifications
                    before using this jumper setting. If the select
                    line in your cable is not modified, use the
                    appropriate jumper settings for Master and Slave
                    above.

 The first drive attached to a host adapter must be a Master.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
JTS      PALLADIUM  JUMPER SETTING

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).


