
7 1 6 8 7 A    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 3280|     |
Capacity form/unform  1687/      MB        Heads           5|   16|     |
Seek time   / track  12.0/ 2.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB MAXCACHE     Landing Zone
Data transfer rate    5.000 MB/S int       Bytes/Sector      512
                     16.700 MB/S ext PIO4
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 71
Power: sleep          0.4 W     Humidity     %         5 95    |      5 95
       standby        0.6 W     Altitude    km    -0.061  3.048| -0.061 12.192
       idle           4.5 W     Shock        g        35       |    150
       seek           5.4 W     Rotation   RPM      4480
       read/write     5.5 W     Acoustic   dBA        39
       spin-up       13.3 W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   72700AP/72577AP/72025AP/71687A/AP/71350A/AP  QUICK REFERENCE


  J1 IDE Interface                                       J2 Power
 +----------------------------------------++J50------J42------+
 |o o o o o o o o o o o o o o o o o o o 1 || o o o   o | OOOO |
 |o o o o o o o o o o   o o o o o o o o o || o o o o o |      |
 +----------------------------------------++-----------+------+

 ====================================================================



  J1 IDE Interface                                       J2 Power
 +----------------------------------------++J46--J42---+------+
 |o o o o o o o o o o o o o o o o o o o 1 || o o o     | OOOO |
 |o o o o o o o o o o   o o o o o o o o o || o o o     |      |
 +----------------------------------------++-----------+------+





**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   72700AP/72577AP/72025AP/71687A/AP/71350A/AP  QUICK REFERENCE

 Jumper Setting
 ==============


  J1 IDE Interface                                       J2 Power
 +----------------------------------------++J50------J42------+
 |o o o o o o o o o o o o o o o o o o o 1 || o o o   o | OOOO |
 |o o o o o o o o o o   o o o o o o o o o || o o o o o |      |
 +----------------------------------------++-----------+------+

 J50  Master Slave
 -----------------
 CLOSED  Only drive in single drive system (default)
 CLOSED  Master in dual drive system
 OPEN    Slave in dual drive system


 J48  Cable Select
 -----------------
 OPEN   Disabled (default)
 CLOSED Enabled


 J46  Write Cache
 ----------------
 OPEN   Enabled (default)
 CLOSED Disabled


 J44 FACTORY RESERVED
 --------------------
 OPEN


 J42  4092 Cylinder Option
 -------------------------
 OPEN   Disabled (default)
 CLOSED Enabled


 Setting System BIOS
 -------------------
 Power up the computer and set the system BIOS/CMOS to Type 9.

 NOTE
 Refer to your system's user guide for help on enabling and
 programming system BIOS CMOS.

 Type 9 should equal 900 cylinders 15 heads and 17 sectors per track
 (SPT). If BIOS Type 9 does not match these parameters, select a user
 definable drive type and program the BIOS with 900 cylinders, 15
 heads and 17 SPT. If the BIOS does not have a user-definable drive
 type, choose a drive type with 15 heads and 17 SPT. This will allow
 the system to see the hard drive.


 Important Note for Installing Drives larger than 2.1GB
 ------------------------------------------------------
 If your system locks up before you can access the system BIOS/CMOS,
 the system may have a BIOS with a 4095 cylinder limitation. Please
 perform the following steps:

 1. Turn off the system.

 2. Install jumper J42 on the drive using the spare jumper supplied.

 3. Restart the system and set the system BIOS/CMOS to Type 9.



  ===================================================================


  J1 IDE Interface                                       J2 Power
 +----------------------------------------++J46--J42---+------+
 |o o o o o o o o o o o o o o o o o o o 1 || o o o     | OOOO |
 |o o o o o o o o o o   o o o o o o o o o || o o o     |      |
 +----------------------------------------++-----------+------+


 J46  Master Slave
 -----------------
 CLOSED  Only drive in single drive system (default)
 CLOSED  Master in dual drive system
 OPEN    Slave in dual drive system


 J44  Cable Select
 -----------------
 OPEN   Disabled (default)
 CLOSED Enabled


 J42  Write Cache
 ----------------
 OPEN   Enabled (default)
 CLOSED Disabled


