
S T 1 8 3 0 N    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    1325|     |     |
Capacity form/unform   702/  834 MB        Heads          13|     |     |
Seek time   / track  12.0/     ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer           256 KB READ-AHEAD   Landing Zone
Data transfer rate    4.000 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL1/7 ZBR                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle           9.0 W     Shock        g        10       |     60
       seek          11.0 W     Rotation   RPM      4535
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     200000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,FCC,IEC380,UL1950,VDE    

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST1830N  JUMPER SETTING

  +---------------------------------------------------------+
  |1-+                                         +---1 J5     |XX
  || |J6                                       +---+        |XX SCSI
  |+-+                                                  +1  |XX I/O
  |                                                     ||  |XX
  |                                                     ||  |XX
  |                                        Terminating  ++  |XX
  |                                        Resistors    +1  |XX
  |                                                     ||  |XX
  |                                                     ||  |XX
  |                                                     ++  |XX
  |                                                     +1  |XX
  |                                                     ||  |XX
  |                                                     ||  |XX
  |                                                     ++  |X1
  |                                                         |
  ++LED                           +---------1 J2            |XX Power
  ++                              +---------+               |XX
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST1830N  JUMPER SETTING

 Jumper setting
 ==============

 Each disk drive has one or more option select header connectors on
 the back, side or front where jumper plugs are installed to select
 the way that the drive is to be configured or to select its ID on the
 I/O bus.


 J2  Motor Start/Write Protect/Terminator Power
 ----------------------------------------------

              Position Numbers
          +-8--7--6--5--4--3--2--1-+         +-J1
 ---------+ o  X  o  o  o  o  o  1 +---------+
          | o  X  o  o  o  o  xxxx |         +----
          +------------------------+

     8   RESERVED

     7   Jumper installed in position 2 enables the Delayed Motor
         Start option (if jumper in position 3 is off). Motor start
         delays is 12 times the drive ID number in seconds; i.e. drive
         ID 0 starts immediately. Drive one starts 12 seconds later,
         etc.

     6   Jumper installed enables Motor Start option. The drive waits
         for the Start unit command from the host before starting the
         spindle motor.


     5   Jumper installed means entire drive is write protected.

     4   Jumper installed means parity checking by the drive is
         enabled.

     3   FACTORY USE

     2   Select terminator power source. In position 1 the drive
     1   supplies power to the SCSI bus, pin 26. In position 2 drive
         supplies power only to its own terminators. (Factory setting)
         Jumper horizontally between positions 1 and 2
         means the drive takes power from the SCSI bus.

  Terminator Power-source Table
  -----------------------------
  1 2             1 2             1 2
 +----           +----           +----
 |X o            |o X            |o o
 |X o            |o X            |xxx
 +------         +------         +-------
 Drive Supplies  Drive Supplies  Bus Supplies
 Bus             Own             Drive


 J5 SCSI ID
 ----------

 LEFT SIDE VIEW                                  J5
                     TOP (HDA)                  +--1+   +-+   Back of
 Front-------PWA--------------------------------+:::+---+X|J1 drive
 of drive                                       +---+   +-+
                                            ID1--+||
                                            ID2---+| If these jumpers
                                            ID4----+ are used, the ID
                                                     jumpers in front
                                                     view ARE NOT USED

           SCSI ID 0        SCSI ID 1        SCSI ID 2
          +---------+      +---------+      +---------+
          | o  o  1 |      | X  o  o |      | o  X  o |
          | o  o  o |      | X  o  o |      | o  X  o |
          +-0--1--2-+      +---------+      +---------+

           SCSI ID 3        SCSI ID 4        SCSI ID 5
          +---------+      +---------+      +---------+
          | X  X  o |      | o  o  X |      | X  o  X |
          | X  X  o |      | o  o  X |      | X  o  X |
          +---------+      +---------+      +---------+

           SCSI ID 6        SCSI ID 7
          +---------+      +---------+
          | o  X  X |      | X  X  X |
          | o  X  X |      | X  X  X |
          +---------+      +---------+

 Drive ID on SCSI Bus (J6 may be used instead). The drive ID is binary
 coded positionwise.

 NOTE
 On erarly drives with PCB 75782395 or 75782485 ID jumpers are
 reserved!


 J6 SCSI ID (optional)
 ---------------------

 FRONT VIEW                           J6
              TOP (HDA)             +-----1+
 ---PWA-----------------------------+::::::+-----
                                    +------+
                                ID4 -+||||+- RESERVED
                                ID2 --+||+-- Remote LED (pin-3 +5V)
                                ID1 ---++--- Spindle Sync (pin-6 REF
                                             SIG+) default CLOSED


                                       SCSI ID 0
     +-2--1--0----------+             +------------------+
     | o  o  o  o  o  1 |             | o  o  o  o  o  o |
     | o  o  o  o  o  o |             | o  o  o  o  o  o |
     +-1--2--3--4--5--6-+             +------------------+

      SCSI ID 1                        SCSI ID 2
     +------------------+             +------------------+
     | o  o  X  o  o  o |             | o  X  o  o  o  o |
     | o  o  X  o  o  o |             | o  X  o  o  o  o |
     +------------------+             +------------------+

      SCSI ID 3                        SCSI ID 4
     +------------------+             +------------------+
     | o  X  X  o  o  o |             | X  o  o  o  o  o |
     | o  X  X  o  o  o |             | X  o  o  o  o  o |
     +------------------+             +------------------+

      SCSI ID 5                        SCSI ID 6
     +------------------+             +------------------+
     | X  o  X  o  o  o |             | X  X  o  o  o  o |
     | X  o  X  o  o  o |             | X  X  o  o  o  o |
     +------------------+             +------------------+


      SCSI ID 7                        Sync Spindle
     +------------------+             +------------------+ Pin 6
     | X  X  X  o  o  o |             | o  o  o  X  o  o | REF SIG+
     | X  X  X  o  o  o |             | o  o  o  X  o  o |
     +------------------+             +------------------+


      Remote LED
     +------------------+  Pin 3
     | o  o  o  o  X  o |  +5V
     | o  o  o  o  X  o |
     +------------------+

 1,2,3  Either J5 or J6 (optional) may be used to select drive ID.
        Both should not be used at same time, because at some future
        time, settings may be changed, causing the drive to not
        respond correctly. The factory installs no ID jumpers on J5 or
        J6 (drive ID 0).

     4  Spindle Synchronization

     5  Used if needed for a connection to a remote LED indicator.

     6  Reserved.


 On SCSI I/O drives either J6 (on the front of the drive) or J5 (on
 the side behind the DC Power connector) may be used to set the drive
 ID. To avoid possible incorrect ID setting, do not use both J5 and
 J6 for ID selection.



 J3   DC Power and pin connector assignments
 -------------------------------------------
 -------------------+
 --+  +-----J3-----+|  pin 1    +12 VDC
  1|  | 4  3  2  1 ||  pin 2    +12 Volts Return
  -+  +------------+|  pin 3    + 5 Volts Return
  ------------------+  pin 4    + 5 VDC



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SEAGATE  ST11200NC/1950N/1830N/1980N INSTALLATION GUIDE 77738480 REV.D

 Notes On Installation
 =====================

 Installation Overview
 ---------------------
 Installation of the drive can be divided into distinct phases as
 outlined below. Some of these may not be applicable to your
 particular installation requirements. Refer to the individual
 drive installation sections for specific information on your
 drive model.

 - Drive configuration: The user must select which of the drive
   features are appropriate to enable for installation in their
   system. This is done by installing or removing of the user
   configuration jumpers found on the drive PCB. "NC" models are
   probably configured by the host over the 80 pin interface.

 - Mechanical installation: After setting up the drive configuration
   the drive must be mechanically in-stalled into the host system and
   the power and I/ O cables attached. Previously mentioned
   precautions should be observed

 - SCSI drives should not be defined in the CMOS: The SCSI Host
   adapter has its own BIOS to handle the Input/output procedures. The
   CMOS setting for SCSI drive is either drive type zero, or the "no
   drive installed" option.


 Drive installation
 ------------------
 This section describes the physical mounting of the drive in the host
 cabinet and the logical installation as a system member, which is
 called drive setup.


 Disc drive mounting
 -------------------
 Do not touch the connector pins or any PCB components without
 observing static-discharge precautions. Always handle the drive by
 the frame only.


 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).
 The drive may be mounted in any orientation.

 - Mount to host system chassis using four 6-32 UNC screws. Three
   mounting holes are in each side and four in the bottom of the
   drive. The maximum length that the screws should extend into the
   side chassis mounting holes is 0.150 inch (3.81 mm), and 0.20 inch
   (5.08 mm) into bottom holes, measured from the outer surface of the
   chassis. The minimum thread engagement for all mounting screws is
   .12 inch (3.0 mm). Tighten the screws evenly to a maximum torque of
   8 in-lb. Do not over tighten or force when screw does not seem to
   screw in easily (threads not correctly engaged).

 - Verify that all connections between the drive and the host system
   are correctly installed. Most cables have a contrasting color
   stripe indicating pin 1.

 - Verify option select and drive ID select jumpers and installation
   of terminator resistor packs where applicable. Do not power up the
   host system until the drive is mounted and the system cover is
   replaced.

 - Connect DC power connector to the drive (not required on "NC"
   model drives).

 - Replace the Host System cover.

 - Turn on DC power.
 - Boot the system from the floppy drive or from a previously
   installed hard-drive if there is one.

 - Proceed with drive setup of the new hard drive.


 Grounding
 ---------
 Signal ground (PCB) and HDA ground are connected together in the
 ST11200 drives family and cannot be separated by the user. The
 equipment in which the drive is mounted is connected directly to the
 HDA and PCB with no electrically isolating shock mounts. If it is
 desired for the system chassis to not be connected to the HDA/PCB
 ground, the systems integrator or user must provide a nonconductive
 (electrically isolating) method of mounting the drive in the host
 equipment.


 NOTES
 Mounting holes three on each side, 6-32 UNC. Max screw length into
 side of drive 0.15 in. (3.81 mm). Screw tightening torque 8.0 in-lb
 max with minimum thread engagement of .12 in (3.00 mm).

 Mounting holes four on bottom, 6-32 UNC. Max screw length into bottom
 of drive 0.20 in. (5.08 mm). Screw tightening torque 8.0 in-lb max
 with minimum thread engagement of .12 in (3.00 mm).

 Power and interface connections can extend past the "A" dimension by
 0.040 in (1.02 mm).

 Decorative front panel.

 Connector is centered (side to side) on drive within  0.020 in. (.508
 mm).


 SCSI interface cable connection
 -------------------------------
 Model ST11200 family are SCSI interface drives. On "N/ND" models,
 system connection is via a 50 pin, SCSI connector. On "NC" models
 system connection and DC power is via a single 80 pin SCSI connector.
 Because of its shape, there is only one way the drive can mate with
 the input connector. Pin 1 is noted in Figure 2. Some cables have a
 contrasting color stripe on one edge to indicate pin 1. Strain relief
 is recommended at the cable. Do not block system cooling air flow by
 the routing of cables.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SEAGATE  ST11200NC/1950/1980/1830N INSTALLATION GUIDE 77738480, REV. D

 Introduction
 ------------
 Before attempting any installation, please read through all
 applicable sections of this document, including all warnings and
 cautions.

 Warning. This equipment generates, uses, and can radiate radio
 frequency energy and if not installed in accordance with these
 instructions, may cause interference to radio communications.


 Electromagnetic interference (EMI) considerations
 -------------------------------------------------
 The drive(s) described herein, as delivered, are designed for
 system integration and installation into a suitable enclosure
 prior to use. As such, the drive(s) described herein are supplied
 as a subassembly and are not subject to Subpart J of Part 15 of
 the FCC Rules and Regulations nor the Radio Interference Regula-
 tions of the Canadian Department of Communications. However, the
 unit has been tested using proper shield-ing and grounding and
 found to be compliant with the Class A limits of the FCC Rules
 and the Regulations of the Canadian Department of Communications.

 The physical design characteristics of the drive(s) described
 herein, serve to minimize EMI radiation when installed in an
 enclosure that provides reason-able shielding. As such, the
 drive(s) are capable of meeting the Class B limits of the FCC
 Rules and the Regulations of the Canadian Department of Communi-
 cations.

 Note. It is the end users responsibility to assure that the
 drive(s) described herein meet the appropriate EMI requirements
 of their system. Shielded I/ O cables may be required if the
 enclosure does not provide adequate shielding. If I/O cables are
 external to the enclosure, shielded cables should be used, with
 the shields grounded to the enclosure and to the host controller.


 Before you begin
 ----------------
 Verify that the system is switched off and disconnected from main
 power before any installation is attempted.

 Protect yourself, the drive, and your valuable programs and data
 by reading the following cautions and warnings.

 - Do not unpack drive from its static shielded bag until you are
   ready to install it in the system.

 - Always handle the drive by the frame or casting.

 - Do not touch printed circuit board (PCB) or the I/O connector
   pins.

 - Never apply pressure to the PCB or to the drive top cover.

 - Do not tamper with sealed top cover. Doing so voids your warranty.
   The drive contains no user servicable components. See Product
   Repair section for more information.

 - Visually inspect the shipping container for any obvious damage.

 - Inspect drive for possible shipping damage. All claims of this
   type should be filed promptly with the transporter involved.
   Save original packing materials to be used when reshipping.

 - Verify all parts listed on shipping bill are received with the
   equipment. Discrepencies or damage should be reported to the
   shipping company.

 Caution. The circuit assemblies and components contained in this
 equipment can be de-graded or destroyed by Electrostatic Over-
 stress (EOS) or by Electrostatic Discharge (ESD).

 Static electrical charges can accumulate quickly on personnel,
 clothing and synthetic materials. The electrostatic fields due
 to these charges when brought in close prox-imity to susceptable
 circuit assemblies and components, can result in degraded reliabil-
 ity or immediate failure of the affected com-ponent or assembly.

 - When transporting or shipping a drive or system, please ensure
   that they are correctly packed in original Seagate approved (or
   equivalent) container and shipped via an airride carrier
   experienced in handling computer equipment.

 To insure optimum reliable equipment operation, it is required
 that technical support personnel discharge themselves by wear-
 ing a grounding strap around the wrist and be connected to a
 grounding terminal while working in the vicinity of, and while
 handling EOS/ESD susceptible assemblies/parts. If unavailable,
 ground yourself frequently by touching the metal chassis of the
 system before handling any components (this helps only if the
 system is connected to a ground). Avoid static-inducing carpeted
 areas.


 Safety instructions
 -------------------
 1. The disc drive(s) are to be installed in a customer supplied
    enclosure where the surrounding air does not exceed 50 o C.

 2. Four (4) 6-32 UNC-2A screws are required for installation.
    Maximum screw length into side of drive is 0.15 inches (3.81
    mm). Maximum screw length into bottom is 0.20 in. (5.08 mm).

 3. The power requirements are shown in Section 1.0 Product
    Information.

 4. The power supply must satisfy the safety requirements for
    SELV (Safety Extra Low Voltage) circuits.

 5. Service is to be provided by trained Seagate service personnel.

 6. The incorporation of the disc drives listed in this guide into
    a customer enclosure must meet the appropriate safety require-
    ments of the country in which it is used (e.g. UL 1950, CAN/
    CSA-C22.2 No. 950-M89, DIN VDE 0805/05.90 and EN60950: 1988
    (IEC 950).


 Installation Overview
 ---------------------
 Installation of the drive can be divided into distinct phases as
 outlined below. Some of these may not be applicable to your
 particular installation requirements. Refer to the individual
 drive installation sections for specific information on your
 drive model.

 - Drive configuration: The user must select which of the drive
   features are appropriate to enable for installation in their
   system. This is done by installing or removing of the user
   configuration jumpers found on the drive PCB. "NC" models are
   probably configured by the host over the 80 pin interface.

 - Mechanical installation: After setting up the drive configuration
   the drive must be mechanically installed into the host system and
   the power and I/ O cables attached. Previously mentioned
   precautions should be observed

 - SCSI drives should not be defined in the CMOS: The SCSI Host
   adapter has its own BIOS to handle the Input/output procedures. The
   CMOS setting for SCSI drive is either drive type zero, or the "no
   drive installed" option.

 - Low-level formatting: After the drive has been properly configured
   for the system, it does not need to be low-level formatted, as this
   has been done by the factory and does not require this step during
   installation. (The low-level format writes the sector boundaries
   and track information to the drive). Defect management information
   is read from the drive by the host system when required in the
   installation procedure. If an installed drive is low-level
   formatted, all user data stored on the drive will be lost.

 Note. Seagate Technology assumes no liability for lost user data.

 - Partitioning and high level formatting: A drive can be sub-divided
   into "partitions" which behave as individual drives within the
   system. See your system documentation. Present day drive
   installation programs have menus that lead you through these
   installation procedures.


 Product repair information/Service requirements
 -----------------------------------------------
 The special facilities required for the manufacture of these drives
 generally prohibit repair in the field. If problems occur during
 installation, please contact your supplier for assistance. Do not
 attempt to dissassemble or repair. Drives should be sent to the
 repair depot through the purchase source, if possible. Please observe
 the following cautions.

 Caution.
 - Handle drive with care. Do not drop or bump hard.

 - Never remove the cover of these disc drives. Servicing items in
   the sealed HDA (heads, media, actua-tor, etc.) require special
   facilities. The drive contains no user purchasable parts or PCBs.

 - Opening the sealed HDA voids the drive warranty.

 - Applying a soldering device to the components on the PCB voids the
   drive warranty.


 Initial setup information
 -------------------------
 For the initial setup connect the cables, set the SCSI bus address
 and remove, install, or leave as is the SCSI I/O line terminator
 resistor packs. These procedures are described in paragraphs
 following.


 Drive setup/SCSI interface drives
 ---------------------------------
 The SCSI interface handles both drive geometry and defect management
 internally or the "no drive installed" option can be selected for
 systems with SCSI drives.

 All SCSI interface drives are low-level formatted at the factory. If
 you wish to low-level format the drive to optimize its performance
 for your system, consult the controller documentation for information
 on low-level formatting. Partitioning and high-level formatting can
 be done through DOS by way of the FDISK utility for partitioning, and
 FORMAT for high-level formatting. Consult your DOS manual for FORMAT
 and FDISK command options.

 Warning. If an installed drive is low-level formatted, all user data
 stored on the drive is lost.

 Seagate Technology assumes no liability for lost user data.



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
SEAGATE   SUPPORT SERVICES

 Seagate Technology
 ------------------
 Technical Support Services
 If you need assistance installing your drive, consult your dealer.
 Dealers are familiar with their unique system configurations and can
 help you with system conflicts and other technical issues. If you
 need additional assistance with your Seagate(r) drive or other
 Seagate products, use one of the Seagate technical support services
 listed below.

 SeaFONE at 1-800-SEAGATE (1-800-732-4283)
 Seagate's 800 number allows toll-free access to automated self-help
 services, providing answers to commonly asked questions,
 troubleshooting tips and specifications for disc drives and tape
 drives. This service is available 24 hours daily and requires a
 touch-tone phone. If you need to speak to a technical support
 engineer, dial this number and listen to the options for technical
 support. (International callers can also reach this automated
 self-help service by dialing 408-456-4496).


 Seagate Technology online services
 Using a modem, you can obtain troubleshooting tips, free utility
 programs, drive specifications and jumper settings for Seagate's
 entire product line. You can also download software for installing
 and analyzing your drive.

 SeaNET
 You can obtain technical information on Seagate drives, Seagate
 software and much more over the Internet from Seagate's World Wide
 Web home page (http://www.seagate.com) or Seagate's ftp server
 (ftp://ftp.seagate.com).

 You may also send E-mail with your questions to DiscSupport@
 Seagate.com or TapeSupport@Seagate.com.


 SeaBOARD
 SeaBOARD is a computer bulletin board system (BBS) that contains
 information about Seagate's disc and tape drive products and is
 available 24 hours daily. Set your communications software to eight
 data bits, no parity and one stop bit (8-N-1). SeaBOARD phone numbers
 are listed in the following table.

 BBS Location           Modem number
 United States      Disc: 408-434-1080; Tape: 408-456-4415
 England            44-1628-478011
 France                         33 1-48 25 35 95
 Germany            49-89-140-9331
 Singapore          65-292-6973
 Thailand           662-531-8111
 Australia          61-2-9756-2359
 Taiwan             886-2-719-6075

 Seagate CompuServe forum
 Online technical support for Seagate products is available on
 CompuServe. To access our technical support forum, type go seagate.
 This forum provides information similar to that found on SeaBOARD.
 In addition, you can type questions or browse through previous
 questions and answers on the forum messages.

 Seagate Technology FAX services
 SeaFAX
 You can use a touch-tone telephone to access Seagate's automated FAX
 system to receive technical support information by return FAX. This
 service is available 24 hours daily.
 Location               Telephone number
 United States          1-800-SEAGATE or 408-456-4496
 England                44-1628-894084
 Australia              61-2-9756-5170

 Seagate technical support FAX
 You can FAX questions or comments to technical support specialists 24
 hours daily. Responses are sent during business hours.
 Location               FAX number
 United States          408-944-9120
 England                        44-1628-890660
 France                 33 1-46 04 42 50
 Germany                        49-89-1430-5100
 Australia              61-2-9725-4052
 Singapore              65-293-4722
 Hong Kong              852-2368 7173
 Taiwan                 886-2-715-2923
 Korea                          82-2-556-7294/4251


 Seagate technical support
 You can talk to a technical support specialist during business hours
 Monday through Friday for one-on-one technical help.  Before calling,
 note your system configuration and drive model number (STxxxx). There
 are several technical support phone numbers available for various
 Seagate products.

 Location          Telephone  number
 United States Please dial 1-800-SEAGATE for the specific product
               telephone number.
               (6:00 A.M. to 11:15 A.M., 12:30 P.M. to 5:00 P.M.,
               Pacific time, M-F)
 England       44-1628-894083 (10:00 A.M. to 1:00 P.M., 2:00 P.M. to
               5:00 P.M., M-F)
 France        33 1-41 86 10 86 (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Germany       Disc: 49-89-140-9332; (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 4:00 P.M., M-F)
               Tape: 49-89-140-9333
 Australia     61-2-9725-3366 (9:00 A.M. to 5:00 P.M., M-F)
 Singapore     65-290-3998 (9:00 A.M. to 12:00 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Hong Kong     852-2368 9918
 Taiwan        886-2-514-2237
 Korea         82-2-556-8241


 SeaTDD 408-944-9121
 Using a telecommunications device for the deaf (TDD), you can send
 questions or comments 24 hours daily and exchange messages with a
 technical support specialist between 6:00 A.M. to 11:15 A.M. and
 12:30 P.M. to 5:00 P.M. (Pacific time) Monday through Friday.


 Customer Service Centers
 Seagate direct OEM, Distribution, System Integrator and Retail
 customers should contact your Seagate Service Representative for
 warranty information.  Other customers contact your place of
 purchase.  Seagate offers comprehensive customer support for all
 Seagate drives.  Seagate customer service centers are the only
 facilities authorized to service Seagate drives. These services are
 available worldwide.

 Location                       Telephone number                FAX number
 United States          1-800-468-3472;                 405-949-6740
 Other Americas
 (Canada & Brazil)      405-949-6706;               405-949-6738
 Mexico                         525-546-6965;                   525-546-4888
 Europe, Middle
 East & Africa          31-2065-43300;              31-2065-34320
 Asia Pacific &
 Australia              65-485-3595;                    65-485-4980
 Japan                          81-3-5462-2904;                 81-3-3462-2979


 Seagate, Seagate Technology and the Seagate logo are registered
 trademarks of Seagate Technology, Inc. SeaFAX, SeaFONE, SeaBOARD,
 SeaTDD, SeaNET, Medalist and DiscWizard are either trademarks or
 registered trademarks of Seagate Technology, Inc. or one of its
 subsidiaries. All other trademarks or registered trademarks are the
 property of their respective owners.


