
C P - 2 0 4 4 P K    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders     548|  980|     |
Capacity form/unform    43/      MB        Heads           4|    5|     |
Seek time   / track  19.0/10.0 ms          Sector/track   38|   17|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            32 KB LOOK-AHEAD   Landing Zone
Data transfer rate    1.500 MB/S int       Bytes/Sector      512
                      4.500 MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 60
Power: sleep          0.3 W     Humidity     %         8 80    |      8 80
       standby        0.4 W     Altitude    km    -0.061  3.048|        12.192
       idle           1.3 W     Shock        g        10       |    100
       seek           2.8 W     Rotation   RPM      3486
       read/write     2.8 W     Acoustic   dBA        34
       spin-up            W     ECC        Bit   88,REED SOLOMON
                                MTBF         h     100000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,IEC435,UL478,VDE


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CP2044PK  PRODUCT MANUAL 00501-007

  +------------------------------------------------------+
  | +-+                                                  |X44
  | | |                                                I |XX Power
  | | |        E1   E2                                 N |XX +5V 41/42
  | +-+         +-+-+                                  T |XX GND 43
  |             | | |                                  E |XX
  |             +-+-+                                  R |XX
  |                                                    F |X* Position
  |                                                    A |XX 20-Key
  |                                                    C |XX
  |                                                    E |XX
  |                                                      |XX
  |                                                      |XX
  |                                                      |1X
  |                                                      |XX Factory
  |                                                      |XX test
  +------------------------------------------------------+   points




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CP2044PK  PRODUCT MANUAL 00501-007

 Jumper setting
 --------------


 Interface Connector/Signal Levels
 ---------------------------------
 All signal levels are TTL compatible. A logic "1" is > 2.0 Volts. A
 logic "0" is from 0.00 Volts to 0.70 Volts. The drive capabolity of
 each of the inbound signals is described below.

    +--------------------------------------------------------+
    | Pin    Signal             Pin     Signal               |
    +--------------------------------------------------------+
    | 01     -Reset             02      GND                  |
    +--------------------------------------------------------+
    | 03     +Data  7           04      +Data  8             |
    +--------------------------------------------------------+
    | 05     +Data  6           06      +Data  9             |
    +--------------------------------------------------------+
    | 07     +Data  5           08      +Data 10             |
    +--------------------------------------------------------+
    | 09     +Data  4           10      +Data 11             |
    +--------------------------------------------------------+
    | 11     +Data  3           12      +Data 12             |
    +--------------------------------------------------------+
    | 13     +Data  2           14      +Data 13             |
    +--------------------------------------------------------+
    | 15     +Data  1           16      +Data 14             |
    +--------------------------------------------------------+
    | 17     +Data  0           18      +Data 15             |
    +--------------------------------------------------------+
    | 19     GND                20      Key                  |
    +--------------------------------------------------------+
    | 21     Reserved           22      GND                  |
    +--------------------------------------------------------+
    | 23     -IOW               24      GND                  |
    +--------------------------------------------------------+
    | 25     -IOR               26      GND                  |
    +--------------------------------------------------------+
    | 27     IOCHRDY            28      Reserved             |
    +--------------------------------------------------------+
    | 29     Reserved           30      GND                  |
    +--------------------------------------------------------+
    | 31     +IRQ               32      -IO16                |
    +--------------------------------------------------------+
    | 33     +ADDR 1            34      -PDIAG               |
    +--------------------------------------------------------+
    | 35     +ADDR 0            36      +ADDR 2              |
    +--------------------------------------------------------+
    | 37     -CS0               38      -CS1                 |
    +--------------------------------------------------------+
    | 39     -Active            40      GND                  |
    +--------------------------------------------------------+
    | 41     5 Volts (Logic)    42      5 Volts (Motor)      |
    +--------------------------------------------------------+
    | 43     GND                44      Reserved             |
    +--------------------------------------------------------+



 E1/E2   Master/Slave
 --------------------
      E1   E2     For Master (C Drive) when E1 is CLOSED, place
      +-+         Jumper as shown.
      |*|  *
      |*|  *
      +-+

      E1   E2      For Slave (D Drive) when E2 is OPEN.
                   Store Jumper as shown.
       *   *
      +-----+
      |*   *|
      +-----+

 The CP2044PK drives are designed to operate either as a Master drive
 (C Drive) or a Slave Drive (D Drive). This feature is dependent on
 two drive settings; the status of hardware Jumper E1 and the firm-
 ware setting of a feature bit. When (E1) is closed, and the feature
 bit is set, the drive will assume the role of a Master Drive.
 When E1 is open, and the feature reset, the drive will act as the
 Slave. In single drive configurations E1 must remain in the closed
 position.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
CONNER   CP2044PK  PRODUCT MANUAL 00501-007

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive may be mounted in any attitude!


 Recommended Mounting Configuration
 ----------------------------------
 This CP2044PK is designed to be used in applications where the unit
 may experience shock and vibrations at greater levels than larger
 and heavier disk drives.

 The design features which allow greater shock tolerance are the use
 of rugged heads and media, a dedicated landing zone, closed loop
 servo positioning and specially designed motor and actuator
 assemblies.

 Four (4) side mounting points and four (4) bottom mounting points are
 provided to the customer. The drive is mounted using 3mm x 0.5mm
 thread screw. The screw insertion depth should not exceed 4mm into
 the mounting holes. The system integrator should allow ventilation
 to the drive to ensure reliable drive operation over the operating
 temperature range.

 For additional vibration isolation, an external suspension system
 may be used.


 Interface Connector
 -------------------
 The CP2044PK drive has a 44 pin right angle interface/power connec-
 tor mounted on the PCB. The recommended mating connector is DuPont
 part number 69764-044 or equivalent. The maximum cable lenght is two
 feet.


 Magnetic Field
 --------------
 The externally induced magnetic flux density may not exceed 6 gauss
 (DC - 700KHz) or 1.0 gauss (700KHz - 1.5MHz) as measured at the
 drive surface.


 Acoustic Sound Emission
 -----------------------
 Pressure: 34 dB(A) max at 1 meter.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
CONNER   CP2044PK  PRODUCT MANUAL 00501-007

 Key Features
 ------------
 The CP2044PK is a family of high performance 2.5 inch low-profile
 disk drives with formatted capacities of 42.6 megabytes.
 The CP2044PK drive has a 19 ms average seek time and is designed to
 operate on IBM PC/AT or equivalent computers.
 The drive feature a low power requirement and high shock resistance,
 enabling battery operation in a portable environment.

 - 2.5" Form factor

 - Single 5 Volt supply

 - Low power requirements

 - 7 oz. unit weight

 - High performance rotary voice coil actuator with embedded servo
   system.

 - Single connector for power & interface

 - Run length limited code (two of seven)

 - High shock resistance

 - Internal air filtration system

 - Sealed HDA

 - Automatic actuator latch over data free landing zone during standby
   mode or power-down

 - Microprocessor-controlled diagnostic routines that are auto-
   matically executed at start-up.

 - Automatic error correction and retries

 - Block size 512 bytes

 - PC AT Interface

 - 1:1 sector interleave

 - Automativ read look ahead

 - 32K Buffer

 - Master/Slave



 Universal Translate Mode
 ------------------------
 Conner has established a Universal Translate Mode which enables the
 user to configure the drive in an AT environment to any cylinder,
 head, and sector configuration desired. The translate configuration
 is limited only by the maximum capacity of the drive. Upon initial
 power up to the drive it will default to a predetermined configura-
 tion shown below:

             Cylinders        Heads       Sectors
 CP-2044PK     980              5           17

 After the drive is ready, the host system may issue INIT DRIVE PARMS
 COMMAND (command code 91H) to alter the translate configuration
 (number of heads and number of sectors per track). The drive para-
 meters will then be saved in EEPROM for subsequent drive operations.



 Seek Times
 ----------

       +----------------------------------+--------+
       |Physical track to track      max. |   5 ms |
       |Logical                      max. |  10 ms |
       +----------------------------------+--------+
       |               Average msec. typ. |  19    |
       |               Average msec. max. |  40    |
       +----------------------------------+--------+
       |Latency                msec. avg. |   8.7  |
       +----------------------------------+--------+
       The timing is measured through the interface with the drive
       operating at nominal DC input voltages. The timing also assumes
       that:
             - BIOS and PC system hardware dependency have been
               subtracted from timing measurements.

             - The drive is operated using its translation parameters.


       The average seek time is determined by averaging the seek time
       for a minimum of 1000 seeks of random length over the surface
       of the disk.


 Write Precomp Register
 ----------------------
 (CSO, address 1 write only) A register previously used to set write
 precompensation, now is used only for enabling or disabling LOOK
 AHEAD READs or to activate extended commands.


 Functional Description
 ----------------------
 The CP2044PK contains all necessary mechanical and electronic parts
 to interpret control signals, position the recording heads over the
 desired track, read and write data, and provide a contaminant free
 environment for the heads and disks.


 Read/Write and Control Electronics
 ----------------------------------
 One integrated circuit is mounted within the sealed enclosure in
 close proximity to the read/write heads. Its function is to provide
 head selection, read preamplification, and write drive circuitry.

 The single microprocessor controlled circuit card provides the
 remaining electronic functions which include:

        - Read/Write Circuitry

        - Rotary Actuator Control

        - Interface Control

        - Spin Speed Control

        - Dynamic Braking

        - Power Management

 At power down or the start of STANDBY MODE or SLEEP MODE the heads
 are automatically retracted to the inner diameter of the disk and
 are latched and parked on a landing zone that is inside the data
 tracks.


 Drive Mechanism
 ---------------
 A brushless DC direct drive motor rotates the spindle at 3486 RPM.
 The motor/spindle assembly is balanced to provide minimal mechanical
 runout to the disks and to reduce vibration of the HDA. A dynamic
 brake is used to provide a fast stop to the spindle motor when power
 is removed, or upon initiation of STANDBY MODE.


 Air Filtration System
 ---------------------
 Within the sealed enclosure, a 0.3 micron filter which provides a
 clean environment for the heads and disks.


 Head Positioning Mechanism
 --------------------------
 The read/write heads for the CP2044PK are supported by a mechanism
 coupled to the voice coil actuator.


 Read/Write Heads and Disks
 --------------------------
 Data is recorded on 65mm diameter thin film disk through micro-
 miniature thin film heads.


 Error Correction
 ----------------
 The CP2044PK use a Reed-Solomon code to perform error detection and
 correction. The error correction polynominal is capable of correcting
 one error burst with a maximum of 22 bits or 2 error bursts of up to
 11 bits each, per 512 byte block. Single bursts of 11 bits or less
 are corrected with no performance degradation.


 Reliability and Maintenance
 ---------------------------
 MTBF                     100,000 hours POH (population is min. of 100
                          units)
 MTTR                     10 minutes typical
 Preventive Maintenance   None
 Component Design Life    5 years


 Safety Standard
 ---------------
 The CP2044PK disk drive is designed to comply with relevant product
 safety standards such as:

 - UL 478, 5th edition, Standard for Safety of Information Processing
   and Business Equipment, and UL 1950, Standard for Safety of
   Information Technology Equipment

 - CSA 22.2#154, Data Processing Equipment and CSA 22.2#220, Inform-
   ation Processing and Business Equipment

 - IEC 435 Safety Requirements for Data Processing Equipment, IEC 380,
   Safety of Electrically Energized Office Machines, and IEC 950,
   Safety of Information Technology Equipment Including Electrical
   Business Equipment

 - VDE 0805 Equivalent to IEC 435, VDE 0805 TIEL 100, Equivalent to
   IEC 950, and VDE 0806, Equivalent to IEC 380


