
R O 5 0 9 0 R    RODIME
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/HH              Cylinders    1224|     |     |
Capacity form/unform   114/      MB        Heads           7|     |     |
Seek time   / track  28.0/ 5.0 ms          Sector/track   26|     |     |
Controller           RLL / ST506           Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate    0.938 MB/S int       Bytes/Sector      512
                      0.938 MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C        10 50    |
Power: sleep              W     Humidity     %        10 85    |
       standby            W     Altitude    km                 |
       idle               W     Shock        g         2       |     30
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   24
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     NO           Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
RODIME   RO 5065/5090 RIGID DISK DRIVE  USER MANUAL PN USM-21550

  +---------------------------------------------------------+  1
  |                                              (under PCB)|XX P3
  |                                                         |XX
  |++LED                                                    |
  |++                                              +---+    |XX
  |                                            EPROM   |    |XX P2
  |                                                |   |    |XX
  |                                                +---+    |X1
  |                                                         |
  |                                                * *4     |XX
  |                                         Drive  * *3     |XX
  |                                         Select * *2     |XX
  |                                                * *1 ++  |XX
  |                                          Terminator ||  |XX
  |                                          Resistor   ||  |XX P1
  |                                                     ||  |XX
  |                                                     ++  |X1
  +---------------------------------------------------------+







      2    P1       34  2    P2    20
     +XXXXXXXXXXXXXXXX--XXXXXXXXXXXX--------+
     |1             33  1          19XXXXXXX|
     |                                  P3 1|
     |                                      |
     +--------------------------------------+
                                     Power



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
RODIME   RO 5065/5090 RIGID DISK DRIVE  USER MANUAL PN USM-21550

 Jumper Setting
 ==============

 x = Jumpers set at factory


 Up to four drives may be connected to any host in a daisy-chain
 fashion. Drive numbering is effected by drive selector pins which are
 connected by means of a jumper provided. To identify a drive as
 number 1, short the pins furthest from the EPROM. All daisy-chained
 drives should have the line terminator pack removed except for the
 last drive in the chain.

 All drives are shipped for single usuage; drive 1 selected and the
 terminator pack present.

 Note that in the multiple drive configuration, all the DATA interface
 lines are radially connected to the host.



    STANDARD SYSTEN WITH FOUR DRIVES
   +-----------+---------+---------+---------+---------+
   | Drive     |         |         |         |         |
   | Select    |Pins 1   |Pins 2   |Pins 3   |Pins 4   |
   +-----------+---------+---------+---------+---------+
 x | Drive 1   |CLOSED   |OPEN     |OPEN     |OPEN     |
   +-----------+---------+---------+---------+---------+
   | Drive 2   |OPEN     |CLOSED   |OPEN     |OPEN     |
   +-----------+---------+---------+---------+---------+
   | Drive 3   |OPEN     |OPEN     |CLOSED   |OPEN     |
   +-----------+---------+---------+---------+---------+
   | Drive 4   |OPEN     |OPEN     |OPEN     |CLOSED   |
   +-----------+---------+---------+---------+---------+


   IBM-STYLE SYSTEM WITH TWO DRIVES
   +-----------+---------+---------+---------+---------+
   | Drive     |         |         |         |         |
   | Select    |Pins 1   |Pins 2   |Pins 3   |Pins 4   |
   +-----------+---------+---------+---------+---------+
   | Drive C:  |OPEN     |CLOSED   |OPEN     |OPEN     |
   +-----------+---------+---------+---------+---------+
   | Drive D:  |OPEN     |CLOSED   |OPEN     |OPEN     |
   +-----------+---------+---------+---------+---------+
 To install any hard disk drive in an IBM AT, drive address must be
 configured as the SECOND drive, regardless of whether it is being
 used as drive C: or D:.


 P3  DC Power and pin connector assignments
 ------------------------------------------
     +--------------+
     |+-----J3-----+|  pin 1    +12 VDC
     || 4  3  2  1 ||  pin 2    +12 Volts Return
     |+------------+|  pin 3    + 5 Volts Return
     +--------------+  pin 4    + 5 VDC


