
D K 3 2 6 C - 6 W D    HITACHI
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    3202|     |     |
Capacity form/unform   601/      MB        Heads           4|     |     |
Seek time   / track   9.8/ 2.0 ms          Sector/track     |     |     |
Controller           SCSI2 DI/WI/FAST      Precompensation
Cache/Buffer           448 KB LOOK-AHEAD   Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C        10 50    |    -20 60
Power: sleep              W     Humidity     %         8 80    |      8 90
       standby            W     Altitude    km                 |
       idle               W     Shock        g         5       |     40
       seek               W     Rotation   RPM      6300
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     400000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


